For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Output Carrier Thrust Bearing Assembly
2 | Output Carrier Internal Front Gear Caution: Install the gear flat side down. Failure to install the gear flat side down may result in transmission damage. Tip Use 2 small blocks next to the output carrier assembly in order to keep the internal front gear engaged with the front pinion gears.
3 | Output Shaft Assembly
4 | Output Carrier Internal Gear Retaining Ring Tip Grasp the output shaft and carrier with both hands to turn over.