For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adjustment Link to Frame Mounting Bolt | 169 N·m | 125 lb ft
Adjustment Link to Knuckle Mounting Bolt | 158 N·m | 116 lb ft
Brake Pipe Bracket to Body Retaining Nuts | 10 N·m | 89 lb in
Frame to Body Bolts, Front | 277 N·m | 204 lb ft
Frame to Body Bolts, Rear | 198 N·m | 146 lb ft
Lower Control Arm to Frame Mounting Bolt Retaining Nut | 136 N·m | 100 lb ft
Lower Control Arm to Knuckle Retaining Bolt | 161 N·m | 118 lb ft
Shock Absorber Upper Mounting Nuts | 25 N·m | 18 lb ft
Shock Lower Mounting Bolt | 165 N·m | 121 lb ft
Stabilizer Shaft Bracket Mounting Bolts | 62 N·m | 45 lb ft
Stabilizer Shaft Link Retaining Nuts | 66 N·m | 49 lb ft
Trailing Arm to Frame Bolt | 153 N·m | 113 lb ft
Trailing Arm to Knuckle Mounting Bolt Retaining Nut | 172 N·m | 127 lb ft
Upper Control Arm Ball Stud to Knuckle Mounting Nut | 66 N·m | 48 lb ft
Upper Control Arm to Frame Mounting Bolt Retaining Nut - Rear | 119 N·m | 84 lb ft
Wheel Bearing/Hub to Knuckle Mounting Bolt | 125 N·m | 92 lb ft
Wheel Drive Shaft to Wheel Bearing Retaining Nut | 160 N·m | 118 lb ft
Upper Control Arm to Frame Mounting Bolt Retaining Nut - Front | 132 N·m | 97 lb ft