For 1990-2009 cars

Table 1: | Accelerator Pedal Position (APP) Sensor
Table 2: | Barometric Pressure (BARO) Sensor
Table 3: | Camshaft Position (CMP) Actuator Solenoid - Exhaust Bank 2
Table 4: | Camshaft Position (CMP) Actuator Solenoid - Intake Bank 2
Table 5: | Camshaft Position (CMP) Sensor - Exhaust Bank 1
Table 6: | Camshaft Position (CMP) Sensor - Exhaust Bank 2
Table 7: | Camshaft Position (CMP) Sensor - Intake Bank 1
Table 8: | Camshaft Position (CMP) Sensor - Intake Bank 2
Table 9: | Crankshaft Position (CKP) Sensor
Table 10: | Engine Coolant Temperature (ECT) Sensor
Table 11: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Table 12: | Evaporative Emission (EVAP) Canister Vent Solenoid
Table 13: | Fuel Injector 1
Table 14: | Fuel Injector 2
Table 15: | Fuel Injector 3
Table 16: | Fuel Injector 4
Table 17: | Fuel Injector 5
Table 18: | Fuel Injector 6
Table 19: | Fuel Pump and Sender Assembly
Table 20: | Fuel Tank Pressure (FTP) Sensor
Table 21: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1
Table 22: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2
Table 23: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1
Table 24: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2
Table 25: | Ignition Coil 1
Table 26: | Ignition Coil 2
Table 27: | Ignition Coil 3
Table 28: | Ignition Coil 4
Table 29: | Ignition Coil 5
Table 30: | Ignition Coil 6
Table 31: | Intake Manifold Runner Control (IMRC) Solenoid
Table 32: | Knock Sensor (KS) Bank 1
Table 33: | Knock Sensor (KS) Bank 2
Table 34: | MAF/IAT Sensor
Table 35: | Secondary Fuel Sender Assembly
Table 36: | Throttle Body Assembly

### Accelerator Pedal Position (APP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 1272 | Accelerator Pedal Position Low Reference (2)
B | L-BU | 1162 | Accelerator Pedal Position Signal (2)
C | TN | 1274 | Accelerator Pedal Position 5-Volt Reference (2)
D | BN | 1271 | Accelerator Pedal Position Low Reference (1)
E | D-BU | 1161 | Accelerator Pedal Position Signal (1)
F | WH/BK | 1164 | Accelerator Pedal Position 5-Volt Reference (1)

### Barometric Pressure (BARO) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 605 | Reference Voltage Feed - 5-Volt Reference
2 | TN | 470 | Sensor Return
3 | L-GN | 432 | Manifold Absolute Pressure Sensor Signal

### Camshaft Position (CMP) Actuator Solenoid - Exhaust Bank 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | 5293 | Engine Main Relay Fused Control (4)
2 | L-GN | 5282 | Camshaft Phaser Exhaust Solenoid (1)

### Camshaft Position (CMP) Actuator Solenoid - Exhaust Bank 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | 5293 | Engine Main Relay Fused Control (4)
2 | WH/BK | 5283 | Camshaft Phaser Exhaust Solenoid (2)

### Camshaft Position (CMP) Actuator Solenoid - Intake Bank 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | 5293 | Engine Main Relay Fused Control (4)
2 | PU | 5284 | Camshaft Phaser Intake Solenoid (1)

### Camshaft Position (CMP) Actuator Solenoid - Intake Bank 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | 5293 | Engine Main Relay Fused Control (4)
2 | OG/BK | 5272 | Camshaft Phaser Intake Solenoid (2)

### Camshaft Position (CMP) Sensor - Exhaust Bank 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | TN | 470 | Sensor Return
2 | D-GN | 5273 | Camshaft Position Exhaust Sensor (1)
3 | GY | 705 | Reference Voltage Feed - 5-Volt Reference

### Camshaft Position (CMP) Sensor - Exhaust Bank 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | TN | 470 | Sensor Return
2 | PU | 5274 | Camshaft Position Exhaust Sensor (2)
3 | GY | 705 | Reference Voltage 5-Volt Reference

### Camshaft Position (CMP) Sensor - Intake Bank 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | TN | 470 | Sensor Return
2 | OG | 5275 | Camshaft Position Intake Sensor (1)
3 | GY | 705 | Reference Voltage Feed 5-Volt Reference

### Camshaft Position (CMP) Sensor - Intake Bank 2

Pin | Wirer | Circuit | Function
--- | --- | --- | ---
1 | TN | 470 | Sensor Return
2 | YE | 5276 | Camshaft Position Intake Sensor (2)
3 | GY | 705 | Reference Voltage Feed 5-Volt Reference

### Crankshaft Position (CKP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU/WH | 5024 | Engine Speed Sensor Low
2 | WH/BK | 5039 | Engine Speed Sensor High

### Engine Coolant Temperature (ECT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 410 | Coolant Temperature Sensor Signal
2 | TN | 470 | Sensor Return

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | 5293 | Engine Main Relay Fused Control (4)
2 | D-GN/WH | 428 | Canister Purge Solenoid Output

### Evaporative Emission (EVAP) Canister Vent Solenoid

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | RD/WH | 1540 | Fuse Output - Battery - Type III Fuse
B | WH | 1310 | Canister Purge Solenoid Output

### Fuel Injector 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK/BK | 5291 | Engine Main Relay Fused Control (2)
B | TN | 1744 | Fuel Injector 1 Output

### Fuel Injector 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK/BK | 5292 | Engine Main Relay Fused Control (3)
B | L-GN/BK | 1745 | Fuel Injector 2 Output

### Fuel Injector 3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK/BK | 5291 | Engine Main Relay Fused Control (2)
B | PK/BK | 1746 | Fuel Injector 3 Output

### Fuel Injector 4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK/BK | 5292 | Engine Main Relay Fused Control (3)
B | L-BU/BK | 844 | Fuel Injector 4 Output

### Fuel Injector 5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK/BK | 5291 | Engine Main Relay Fused Control (2)
B | TN/WH | 845 | Fuel Injector 5 Output

### Fuel Injector 6

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK/BK | 5292 | Engine Main Relay Fused Control (3)
B | YE/BK | 846 | Fuel Injector 6 Output

### Fuel Pump and Sender Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-BU | 1936 | Primary Fuel Level Sensor Signal
B | GY | 120 | Fuel Pump Motor Feed
C | BK | 1050 | Ground
D | TN | 452 | Fuel Tank Pressure Sensor Low Reference

### Fuel Tank Pressure (FTP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | TN | 452 | Sensor Return - Fuel Tank Pressure 1 Sensor
B | D-GN | 890 | Fuel Tank Pressure Sensor Signal
C | GY | 596 | Reference Voltage Feed - 5-Volt Reference Fuel Tank Pressure 1 Sensor

### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | 5278 | Heated Oxygen Sensor Input Pump Current Bank 1 Sensor
2 | TN | 1664 | HO2S Heater Low Signal - Bank 1 Sensor 1
3 | GY/WH | 3113 | HO2S Heater Low Control - Bank 1 Sensor 1
4 | PK/BK | 5293 | Engine Main Relay Fused Control
5 | WH | 5279 | Output Pump Current
6 | PU | 1665 | HO2S High Signal - Bank 1 Sensor 1

### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | TN/WH | 1669 | Oxygen Sensor Return - Left - Rear of Catalytic Converter
B | PU/WH | 1668 | Oxygen Sensor Signal - Left - Rear of Catalytic Converter
C | BK/WH | 3122 | Oxygen Sensor Heater Control Low - Front
D | PK/BK | 5294 | Engine Main Relay Fused Control (5)

### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 5280 | HO2S Input Pump Current - Bank 2 Sensor (1)
2 | TN | 1667 | HO2S High Signal - Bank 2 Sensor 1
3 | L-BU | 3212 | HO2S Heater Low Control - Bank 2 Sensor 1
4 | PK/BK | 5293 | Engine Main Relay Fused Control
5 | PU/WH | 5281 | HO2S Low Signal - Bank 2 Sensor 1 Output Pump Current
6 | PU | 1666 | HO2S High Signal - Bank 2 Sensor 1

### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2

Pin | Wire C | Circuit | Function
--- | --- | --- | ---
A | TN | 1671 | Oxygen Sensor Return - Right - Rear of Catalytic Converter
B | PU | 1670 | Oxygen Sensor Signal - Right - Rear of Catalytic Converter
C | OG/WH | 3223 | Oxygen Sensor Signal - Bank 2 Sensor 2 Heater Control Low
D | PK/BK | 5294 | Engine Main Relay Fused Control (5)

### Ignition Coil 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | 2121 | Electronic Spark Timing Signal Cylinder 1
2 | PK/BK | 5291 | Engine Main Relay Fused Control (2)
3 | BK/WH | 1551 | Ground - Clean
4 | BK | 1550 | Ground

### Ignition Coil 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/WH | 2122 | Electronic Spark Timing Signal Cylinder 2
2 | PK/BK | 5292 | Engine Main Relay Fused Control (3)
3 | BK/WH | 151 | Ground - Clean
4 | BK | 150 | Ground

### Ignition Coil 3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 2123 | Electronic Spark Timing Signal Cylinder 3
2 | PK/BK | 5291 | Engine Main Relay Fused Control (2)
3 | BK/WH | 1551 | Ground - Clean
4 | BK | 1550 | Ground

### Ignition Coil 4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | 2124 | Electronic Spark Timing Signal Cylinder 4
2 | PK/BK | 5292 | Engine Main Relay Fused Control (3)
3 | BK/WH | 151 | Ground - Clean
4 | BK | 150 | Ground

### Ignition Coil 5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 2125 | Electronic Spark Timing Signal Cylinder 5
2 | PK/BK | 5291 | Engine Main Relay Fused Control (2)
3 | BK/WH | 1551 | Ground - Clean
4 | BK | 1550 | Ground

### Ignition Coil 6

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/WH | 2126 | Electronic Spark Timing Signal Cylinder 6
2 | PK/BK | 5292 | Engine Main Relay Fused Control (3)
3 | BK/WH | 151 | Ground - Clean
4 | BK | 150 | Ground

### Intake Manifold Runner Control (IMRC) Solenoid

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TN | 470 | Sensor Low Reference
B | YE | 7017 | Variable Intake Manifold Position Signal
C | L-BU/WH | 5041 | Intake Manifold Control
D | BK | 1450 | Ground
E | PK/BK | 5293 | Engine Main Relay Fused Control (4)

### Knock Sensor (KS) Bank 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 496 | Knock Sensor Signal 1
2 | GY | 1716 | Knock Sensor Return

### Knock Sensor (KS) Bank 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 1876 | Knock Sensor Signal 2
2 | TN | 407 | Sensor Return

### MAF/IAT Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | TN | 472 | Manifold Absolute Temperature Sensor Signal
2 | PK | 439 | Run/Crank Ignition 1 Voltage
3 | TN | 2760 | Sensor Return - Induction Air Temperature
4 | GY | 596 | Reference Voltage Feed - 5-Volt Reference
5 | YE | 492 | Mass Air Flow Sensor Signal

### Secondary Fuel Sender Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | 1937 | Secondary Fuel Level Sensor Signal
B-C | -- | -- | Not Used
D | TN | 2759 | Fuel Tank Pressure Sensor Low Reference

### Throttle Body Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 485 | Throttle Position Sensor Signal 1
2 | GY | 2701 | Throttle Position Sensor 5-Volt Reference
3 | BN | 582 | Throttle Actuator Control Close
4 | PU | 486 | Throttle Position Sensor Signal 2
5 | YE | 581 | Throttle Actuator Control Open
6 | TN | 2752 | Throttle Position Sensor Low Reference