For 1990-2009 cars

### Removal Procedure

1. Remove the front console upper trim plate. Refer to Front Floor Console Extension Panel Replacement .
2. Remove the bolts securing the left and right center air outlets.
3. Remove the left and right center air outlets.

### Installation Procedure

1. Install the left and right center air outlets.
2. Install the bolts securing the left and right center air outlets.
3. Install the front console upper trim plate. Refer to Front Floor Console Extension Panel Replacement .