For 1990-2009 cars

## Rear Side Door Upper Hinge and Lower Hinge Replacement Lower

Callout | Component Name
--- | ---

#### Rear Side Door Lower Hinge Assembly Replacement

Tip
Replace only one hinge at a time.

1 | Rear Side Door Hinge Lower Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Rear Side Door Hinge Lower Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
3 | Rear Side Door Lower Hinge Assembly Replacement

## Rear Side Door Upper Hinge and Lower Hinge Replacement Upper

Callout | Component Name
--- | ---

#### Rear Side Door Upper Hinge Assembly Replacement

Tip
Replace only one hinge at a time.

1 | Rear Side Door Hinge Upper Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Rear Side Door Hinge Upper Bolt (Qty: 2) Tighten 25 N·m (18 lb ft)
3 | Rear Side Door Upper Hinge Assembly