For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Inflatable Restraint Front End Sensor | 9 N·m | 80 lb in
Inflatable Restraint IP Module Fasteners | 12 N·m | 9 lb ft
Inflatable Restraint Roof Rail Module Fasteners | 9 N·m | 80 lb in
Inflatable Restraint Sensing and Diagnostic Module (SDM) Fasteners | 9 N·m | 80 lb in
Inflatable Restraint Side Impact Module Bracket Bolts | 9 N·m | 80 lb in
Inflatable Restraint Side Impact Module Bracket to Seat Frame Bolts | 9 N·m | 80 lb in
Inflatable Restraint Side Impact Sensor (SIS) Bolts | 9 N·m | 80 lb in
Seat Belt Buckle Pretensioner Bolt | 50 N·m | 37 lb ft
Steering Column Shrouds | 2 N·m | 18 lb in
Steering Wheel Nut | 41 N·m | 30 lb ft