For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Floor Console Refer to Front Floor Console Replacement.
2 | Center Console End Panel

#### Procedure

1. Using blunt trim tool release the retaining clips. Refer to Front Floor Console Side Trim Rear Panel Replacement.
2. Removing the end panel allows the removal of the air distribution duct (6).

3 | Side Impact Brace Screw (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
4 | Side Impact Brace
5 | Air Distribution Duct Screw (Qty: 3) Tighten 2 N·m (18 lb in)
6 | Air Distribution Duct
7 | Retainer Actuator Screw (Qty: 2) Tighten 1 N·m (9 lb in)
8 | Mode Actuator Connector
9 | Mode Actuator