For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the shift control handle. Refer to Transmission Control Lever Knob Replacement.
2. Remove the center console assembly. Refer to Front Floor Console Replacement.

1 | Shift Select Control
2 | Shift Control Indicator Tip

• | Remove the shift indicator lamp sockets from the shift indicator by rotating the lamp sockets one quarter turn counter-clockwise.

• | Install the shift indicator lamp sockets to the shift indicator. Rotate each lamp socket one quarter turn clockwise to lock in place.

3 | Shift Control Indication Panel