For 1990-2009 cars

Check | Causes
--- | ---
DEFINITION: The transmission only provides fifth gear in Drive range. The vehicle accelerates from a stop in fifth gear.
Control Valve Body Accumulator Assembly | Feed limit valve or spring stuck in the exhaust position
Wiring Harness | Improper electrical connection to shift solenoids
Inspect for active transmission DTCs | Transmission DTC default action active