For 1990-2009 cars

### Removal Procedure

1. Remove the rear floor console. Refer to Rear Floor Console Replacement.
2. Remove the rear console cover panel.
3. Remove the bolts securing the rear console armrest from the back.
4. Remove the armrest from the rear console.

### Installation Procedure

1. Install the armrest to the rear console.
2. Install the bolts securing the armrest to the rear console.
3. Install the rear console cover panel.
4. Install the rear console. Refer to Rear Floor Console Replacement.