For 1990-2009 cars

Callout | Component Name
--- | ---

#### Front Door Check Link Assembly Replacement

1 | Front Side Door Trim Assembly Refer to Front Side Door Trim Panel Replacement.
2 | Front Side Door Water Deflector Assembly
3 | Front Side Door Check Link Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 32 N·m (24 lb ft)
4 | Front Side Door Check Link Bolt (Qty: 2) Tighten 10 N·m (89 lb in)
5 | Front Side Door Check Link Assembly Tip Check link assembly is removed and installed from the inside of the door.