For 1990-2009 cars

### Removal Procedure

1. Remove the rear upper compartment trim. Refer to Rear Wheelhouse Panel Liner Replacement .
2. Release the tabs securing the rear integration module (2) to the module bracket.
3. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.
2. Install the module (2) to the bracket.
3. Install the rear upper compartment trim. Refer to Rear Wheelhouse Panel Liner Replacement .
4. Re-program the module. Refer to Control Module References .