For 1990-2009 cars

## Rear Seat Latch Release Handle Replacement With 40 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Recliner Handle Bolt Cap
2 | Rear Seat Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (35 lb in)
3 | Rear Seat Latch Release Handle

## Rear Seat Latch Release Handle Replacement With 60 Percent Seat

Callout | Component Name
--- | ---
1 | Rear Seat Recliner Handle Bolt Cap
2 | Rear Seat Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 4 N·m (35 lb in)
3 | Rear Seat Latch Release Handle