For 1990-2009 cars

Callout | Component Name
--- | ---
1 | DT-47811-A Transmission Lift Plate Warning: Handle with care, the transmission assembly weighs over 200 lbs. Bodily injury could occur if not handled properly. Tip After Installation of lift plate, raise the transmission with an overhead hoist. Tighten
12 N·m (9 lb ft)

#### Special Tools

DT-47811-A Transmission Lift Plate

For equivalent regional tools, refer to Special Tools.

2 | J-46625 Transmission Holding Fixture Caution: Refer to Fastener Caution in the Preface section. Tip Adjust mounting block on fixture to match bosses on case, then tighten bolts to: Tighten
13 N·m (10 lb ft)

#### Special Tools

J-46625 Transmission Holding Fixture

For equivalent regional tools, refer to Special Tools.