For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .

1 | Locknut
2 | Front Park Brake Cable Connector
3 | Right Park Brake Cable

#### Procedure

Using the J 37043 , compress the locking tabs on the park brake cable conduit and remove the cable from the equalizer.

#### Special Tools

J 37043 Parking Brake Cable Release Tool

4 | Left Park Brake Cable
5 | Equalizer

#### Procedure

Adjust the park brake. Refer to Park Brake Adjustment .