For 1990-2009 cars

## Instrument Panel Cluster Trim Plate Applique Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the instrument panel cluster trim plate cover. Refer to Instrument Panel Cluster Trim Plate Cover Replacement.
2. Remove the left side instrument panel trim panel. Refer to Instrument Panel Trim Panel Replacement - Left Side.

1 | Instrument Panel Cluster Trim Plate Applique Screw (Qty 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Cluster Trim Plate Applique Assembly
3 | Retainer Clip (Qty: 6)