For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: After cleaning the transmission components, allow to air dry. Do not use cloth or paper towels in order to dry any transmission components. Lint from the towels can cause component failure. Caution: Do not reuse cleaning solvents. Previously used solvents may deposit sediment which may damage the component.
1 | Control Valve Body Spacer Plate Retainer (Qty: 2)
2 | Control Valve Upper Body Spacer Plate Assembly
3 | Actuator Feed Accumulator Spring (Qty: 3)
4 | Actuator Feed Accumulator Piston (Qty: 3)
5 | Control Valve Body Locating Pin (Qty: 2) Tip Inspect locating pins for proper installed height of 4.25 mm (0.17 in).