For 1990-2009 cars

## Front Bumper Fascia Headlamp Opening Flange Support Replacement With and without TVP

Callout | Component Name
--- | ---

#### Procedure

Remove the headlamp assembly. Refer to Headlamp Replacement.

1 | Front Bumper Fascia Headlamp Opening Flange Support Screw (Qty: 6) Caution: Refer to Fastener Caution in the Preface section. Tighten Hand tighten the screws.
2 | Front Bumper Fascia Headlamp Opening Flange Support