For 1990-2009 cars

This master DTC list includes all applicable DTCs in alphanumeric order with descriptors.

DTC | DTC Descriptor | Module That Sets the DTC | Diagnostic Procedure
--- | --- | --- | ---
B0000 | Vehicle Speed Information Circuit | EBCM | DTC B0000
B0012 | Driver Frontal Deployment Loop Stage 1 Circuit | SDM | DTC B0012 or B0013
B0013 | Driver Frontal Deployment Loop Stage 2 Circuit | SDM | DTC B0012 or B0013
B0014 | LF Side Deployment Loop | SDM | DTC B0014-B0045
B0015 | LF Pretensioner Deployment Loop | SDM | DTC B0014-B0045
B0016 | LF Roof Rail Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B0019 | Passenger Frontal Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B001A | Left Front Seat belt Pretensioner Deployment Loop | SDM | DTC B001A
B001B | Right Front Seat belt Pretensioner Deployment Loop | SDM | DTC B001B
B0020 | Passenger Frontal Deployment Loop Stage 2 | SDM | DTC B0014-B0045
B0021 | RF Side Deployment Loop | SDM | DTC B0014-B0045
B0022 | RF Pretensioner Deployment Loop | SDM | DTC B0014-B0045
B0023 | RF Roof Rail Deployment Loop Stage 1 | SDM | DTC B0014-B0045
B0052 | Deployment Commanded | SDM | DTC B0052, B0053, or B0055
B0053 | Deployment Commanded with Loop DTCs Present | SDM | DTC B0052, B0053, or B0055
B0055 | Side Airbag Deployment Commanded | SDM | DTC B0052, B0053, or B0055
B0056 | Passenger Frontal Airbag Suppressed | SDM | DTC B0056-B0058
B0057 | Passenger Side Airbag Suppressed | SDM | DTC B0056-B0058
B0058 | Passenger Pretensioner Suppressed | SDM | DTC B0056-B0058
B0073 | Passenger Seat Belt Sensor Circuit | SDM | DTC B0073
B0074 | Passenger Occupant Classification Sensor Circuit | PPS | DTC B0074
B0081 | Passenger Occupant Classification Sensor Circuit | PPS, SDM | DTC B0081
B0083 | Front End Sensor 1 Circuit | SDM | DTC B0083-B0088
B0084 | Front End Sensor 2 Circuit | SDM | DTC B0083-B0088
B0085 | Left Front Side Impact Sensor Circuit | SDM | DTC B0083-B0088
B0086 | Right Front Side Impact Sensor Circuit | SDM | DTC B0083-B0088
B0087 | LR Side Impact Sensor Circuit | SDM | DTC B0083-B0088
B0088 | RR Side Impact Sensor Circuit | SDM | DTC B0083-B0088
B0090 | Rollover Sensor Performance | SDM | DTC B0090
B0158 | Outside Air Temperature Sensor Circuit | HVAC | DTC B0158
HVAC - Manual | DTC B0158
B0163 | Passenger Compartment Temperature Sensor Circuit Short | HVAC | DTC B0163
B0173 | Output Air Temperature Sensor 1 Circuit Short to Battery or Open | HVAC | DTC B0173, B0178, B0509, or B0514
B0178 | Output Air Temperature Sensor 2 Circuit Short | HVAC | DTC B0173, B0178, B0509, or B0514
B0183 | Solar Load Sensor 1 Circuit | BCM | DTC B0183 or B0188
B0188 | Solar Load Sensor 2 Circuit | BCM | DTC B0183 or B0188
B0228 | Recirculate Position Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782 w/CJ2
HVAC- Manual | DTC B0228, B0413, B0433, B3779, or B3782
B0283 | Electric Rear Defrost Circuit | HVAC | DTC B0283
B0413 | Temperature Control 1 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
HVAC- Manual | DTC B0228, B0413, B0433, B3779, or B3782
B0423 | Temperature Control 2 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
B0433 | Temperature Control 3 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
HVAC- Manual | DTC B0228, B0413, B0433, B3779, or B3782
B0509 | Output Air Temperature Sensor 3 Circuit Short | HVAC | DTC B0173, B0178, B0509, or B0514
B0514 | Output Air Temperature Sensor 4 Circuit Short | HVAC | DTC B0173, B0178, B0509, or B0514
B0958 | Parking Aid Rear Sensor 1 Left Corner Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B0959 | Parking Aid Rear Sensor 1 Left Middle Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B0960 | Parking Aid Rear Sensor 1 Right Middle Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B0961 | Parking Aid Rear Sensor 1 Right Middle Circuit | Object Alarm Module | DTC B0958, B0959, B0960, or B0961
B0968 | Parking Aid Indicator Circuit | Object Alarm Module | DTC B0968
B1000 | Electronic Control Unit (ECU) Performance | BCM, DDM, DRR, HVAC, PDM, PLGM, PPS, Radio, RCDLR, ROS, RSA, SDM, TDM, UPA, VCIM | DTC B1000
B1001 | Option Configuration Error | BCM, MSM, PPS, Radio, ROS, VCIM | DTC B1001
SDM | DTC B1001
B1008 | Calibration Data Not Programmed | Object Alarm Module | DTC B1008
Remote Functions | DTC B1008
B1011 | System Disabled Information Stored Invalid Serial Data Received | Rollover Sensor | DTC B1011
B1015 | Vehicle Identification Number (VIN) Information Error | Object Alarm Module | DTC B1015
B1016 | VIN Not Programmed | BCM, DDM, PDM, TDM | DTC B1016
B1019 | System Configuration Error | SDM | DTC B1019
PLGM | DTC B1019
B101D | ECU Hardware Performance | PPS | DTC B101D
B101E | ECU Software Performance | PPS | DTC B101E
B1023 | Integral Switch Performance | DDM, PDM | DTC B1023
B1025 | Audio Output 1 Left Front Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1035 | Audio Output 2 Right Front Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1045 | Audio Output 3 Left Rear Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1055 | Audio Output 4 Right Rear Circuit | Radio | DTC B1025, B1035, B1045, or B1055
B1259 | Antenna Ground Circuit Short | DRR | DTC B1259
B1287 | Amplifier Control Signal Circuit Short | Radio | DTC B1287
B1288 | Video Display Mode Control Signal | Radio | DTC B1288
B1289 | Video Display Brightness Control Signal | Radio | DTC B1289
B1325 | Device Power Circuit | HUD, IPC, PPS, Radio, UPA | DTC B1325
B1335 | Device Power 3 Circuit | MSM | DTC B1335
B1340 | Device Power 3 Circuit | MSM | DTC B1340
B1370 | Device Ignition 1 Circuit | SDM | DTC B1370
Device Ignition 1 ON and START Circuit | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B1380 | Device Ignition Accessory Circuit | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B1395 | Device Voltage Reference Output Circuit | BCM | DTC B1395
MSM | DTC B1395
B1397 | Diming Reference Voltage Circut Low | BCM | DTC B1397
B1424 | Device 1 Voltage Low | TDM | DTC B1424
B1428 | Ignition Switched Power Run/Crank Relay Circuit | BCM | DTC B1428
B1433 | Ignition Switched Power Relay 2 Circuit | BCM | DTC B1433
B1440 | Power Mode Master Input Circuits Mismatch | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B1441 | Device Ignition Off/Run/Crank Circuit | BCM | DTC B1370-B1379, B1380-B1389, or B1440-B1443
B1449 | Remote Device Voltage | RSA | DTC B1449
B1461 | Left Headlamp Horizontal Motor Circut | AFL | DTC B1461 or B1462
B1462 | Right Headlamp Horizontal Motor Circut | AFL | DTC B1461 or B1462
B1475 | Retained Accessory Power Circuit | BCM | DTC B1475
B1480 | Battery Rundown Protection Circuit | BCM | DTC B1480
B1516 | Battery Current Sensor Signal | BCM | DTC B1516
B1517 | Battery Voltage | BCM | DTC B1517
B1527 | High Parasitic Load Detected | BCM | DTC B1527
B1529 | Device Voltage Reference Output Circuit | BCM | DTC B1529
B153A | Liftgate Latch Switch Signal Circuit | PLGM | DTC B153A
B153B | Liftgate Open Switch Signal Circuit | PLGM | DTC B153B
B153E | Liftgate Position Sensor Signal Circuit | PLGM | DTC B153E
B153F | Liftgate Object Sensor Signal Circuit | PLGM | DTC B153F
B1544 | Mirror Motors Common Circuit | DDS, PDS | DTC B1544, B1600, or B1605
B1580 | Mirror Horizontal Position Sensor Circuit | DDS, PDS | DTC B1580 or B1590
B1590 | Mirror Vertical Position Sensor Circuit | DDS, PDS | DTC B1580 or B1590
B1600 | Mirror Motor Vertical Circuit | DDS, PDS | DTC B1544, B1600, or B1605
B1605 | Mirror Motor Horizontal Circuit | DDS, PDS | DTC B1544, B1600, or B1605
B1640 | Mirror Heater Circuit | DDS, PDS | DTC B1640
B1722 | Mirror Power Fold Circut | DDM, PDM | DTC B1722
B1735 | Driver Seat Front Up Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1740 | Driver Seat Front Down Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1745 | Driver Seat Rear Up Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1750 | Driver Seat Rear Down Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1755 | Driver Seat Assembly Horizontal Forward Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1760 | Driver Seat Assembly Horizontal Rearward Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1815 | Driver Seat Recline Forward Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1820 | Driver Seat Recline Rearward Switch Circuit | MSM | DTC B1735, B1740, B1745, B1750, B1755, B1760, B1815, or B1820
B1825 | Driver Seat Recline Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B1850 | Driver Seat Lumbar Horizontal Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B1860 | Driver Seat Lumbar Vertical Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B1925 | Left Seat Heater Cushion Sensor Circuit | MSM | DTC B1925 or B2170
B1935 | Left Seat Back Heater Circuit | MSM | DTC B1935 or B2180
B1E3A | Sensor Power Circuit Voltage | Object Alarm Module | DTC B1E3A
B2170 | Right Seat Heater Cushion Sensor Circuit | MSM | DTC B1925 or B2170
B2180 | Right Seat Back Heater Circuit | MSM | DTC B1935 or B2180
B2345 | Seat Heater Disable Circuit | MSM | DTC B2345
B2355 | Driver Seat Front Vertical Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B2365 | Driver Seat Rear Vertical Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B2375 | Driver Seat Assembly Horizontal Position Sensor Circuit | MSM | DTC B1825, B1850, B1860, B2355, B2365, or B2375
B2425 | Left Seat Cushion Heater Circuit | MSM | DTC B2425 or B2430
B2430 | Right Seat Cushion Heater Circuit | MSM | DTC B2425 or B2430
B2435 | Left Seat Back Heater Sensor Circuit | MSM | DTC B2435 or B2440
B2440 | Right Seat Back Heater Sensor Circuit | MSM | DTC B2435 or B2440
B2455 | Cellular Phone Microphone Circuit | VCIM | DTC B2455
B2462 | Global Positioning System (GPS) | Navigation Radio | DTC B2462
B2470 | Cellular Phone Antenna Circuit Malfunction | VCIM | DTC B2470
B2474 | Navigation Display Head Backlighting Performance | Navigation Radio | DTC B2474
B2476 | Cellular Phone Select Service Switch Malfunction | VCIM | DTC B2476 or B2482
B2482 | Cellular Phone Select Service Switch Range/Performance | VCIM | DTC B2476 or B2482
B2485 | Wireless Communication Antenna Circut (Bluetooth) | VCIM | DTC B2485
B2494 | Liftgate Handle Switch Circuit | BCM, PLGM | DTC B2494
B2495 | Liftgate Latch Control Circuit | PLGM | DTC B2495
B2508 | Seat Heater Relay Circuit | MSM | DTC B2508 or B2509
B2530 | Front Fog Lamp Control Circuit | BCM | DTC B2530
B2545 | Backup Lamps Circuit | BCM | DTC B2545
B2555 | Passenger Compartment Lamp Control Circuit | BCM | DTC B2555
B2575 | Headlamp Control Circuit | BCM | DTC B2575
B257A | Headlamp Switch Input Signal Mismatch | BCM | DTC B257A
B257C | Left Headlamp Assembly | BCM | DTC B257C
B257D | Right Headlamp Assembly | BCM | DTC B257D
B2580 | Headlamp High Beam Control Circuit | BCM | DTC B2580
B2585 | Park Lamp Circuit | BCM | DTC B2585
B2600 | Daytime Running Lamp Control Circuit | BCM | DTC B2600
B2605 | Daytime Running Lamp Control Circuit | BCM | DTC B2605
B2610 | Passenger Compartment Dimming 1 Circuit | BCM | DTC B2610
B2615 | Passenger Compartment Dimming 2 Circuit | BCM | DTC B2615
B2625 | Display Dimming Pulse Width Modulation (PWM) Output Circut | BCM | DTC B2625
B2645 | Ambient Light Sensor Circuit | BCM | DTC B2645
B2652 | Passenger Compartment Dimming 3 Circuit | BCM | DTC B2652
B2705 | Gearshift Unlock Circuit | BCM | DTC B2705
B2750 | Horn Relay Coil Circuit | BCM | DTC B2750
B2850 | Telescope Forward Switch Circut Short to Battery | MSM | DTC B2850
B2855 | Telescope Rearward Switch Circut Short to Battery | MSM | DTC B2855
B2860 | Telescope PositionSensor Circut Short | MSM | DTC B2860
B2870 | Tilt Up Switch Circut Short to Battery | MSM | DTC B2870
B2875 | Tilt Down Switch Circut Short to Battery | MSM | DTC B2875
B2880 | Tilt Position Sensor Circut | MSM | DTC B2880
B2890 | Tilt and Telescope Motor Circut Calibration Not Learned | MSM | DTC B2890
B2976 | Door Ajar Circut | BCM, IPC, DIC | DTC B2976
B3006 | Hood Ajar Circuit | BCM | DTC B3006
B302A | Telematic Requested Immobilization | TDM | DTC B302A
B3031 | Security System Controller In Learn Mode | TDM | DTC B3031
B3055 | No Transponder Modulation or No Transponder | TDM | DTC B3055
B3060 | Unprogrammed Transponder Identification Code Received | TDM | DTC B3060
B3105 | Keyless Entry System Key Fobs Not Programmed | RCDLR | DTC B3105
B3109-B3112 | Keyless Entry Transmitter 1-4 Low Battery | RCDLR | DTC B3109, B3110, B3111, or B3112
B3125 | Driver Door Only, Unlock Circuit | BCM | DTC B3125, B3130, or B3135
B3130 | All Door Unlock Circuit | BCM | DTC B3125, B3130, or B3135
B3135 | All Door Lock Circuit | BCM | DTC B3125, B3130, or B3135
B3140 | Driver Unlock Switch Circut | BCM | DTC B3140, B3145, B3150, or B3155
B3145 | Passenger Unlock Switch Circut | BCM | DTC B3140, B3145, B3150, or B3155
B3150 | Driver Lock Switch Circut | BCM | DTC B3140, B3145, B3150, or B3155
B3155 | Passenger Lock Switch Circut | BCM | DTC B3140, B3145, B3150, or B3155
B3205 | Window Inactive Over Current Fault | PDM | DTC B3205
B320A | Front Door Window Motor | DDM, PDM | DTC B320A
B3265 | Hatch Release Output Circut | BCM | DTC B3265
B3445 | Stop Lamp Circuit | BCM | DTC B3445
B3567 | Driver Information Center (DIC) Select Switch Circuit | HUD, IPC | DTC B3567
Head-Up Display (HUD) Select Switch Circuit
B3600 | Passenger Compartment Dimming Request Signal Circuit | BCM | DTC B3600
B3622 | Steering Wheel Controls Signal Circuit | BCM | DTC B3622
B3715 | Front Wiper Relay Drive Circuit | BCM | DTC B3715
B3779 | Air Flow Control 9 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
HVAC- Manual | DTC B0228, B0413, B0433, B3779, or B3782
B3782 | Air Flow Control 10 Feedback Circuit | HVAC | DTC B0228, B0413, B0423, B0433, B3779, or B3782
HVAC- Manual | DTC B0228, B0413, B0433, B3779, or B3782
B3794 | Cruise Control Function Request Circuit | BCM | DTC B3794
B3819 | Left Rear Up Control Circuit | BCM | DTC B3819, B3820, B3822, or B3823
B3820 | Left Rear Window Down Control Circuit | BCM | DTC B3819, B3820, B3822, or B3823
B3821 | Left Rear Window Relay Power Circuit | BCM | DTC B3821 or B3824
B3822 | Right Rear Up Control Circuit | BCM | DTC B3819, B3820, B3822, or B3823
B3823 | Right Rear Window Down Control Circuit | BCM | DTC B3819, B3820, B3822, or B3823
B3824 | Right Rear Window Relay Power Circuit | BCM | DTC B3821 or B3824
B3873 | Front Washer Relay Circuit | BCM | DTC B3873
B3875 | Wiper High Speed Relay Circuit | BCM | DTC B3875
B3920 | Group 1 Seat Motors Circuit | MSM | DTC B3920 or B3921
B3921 | Group 2 Seat Motors Circuit | MSM | DTC B3920 or B3921
B3922 | Front Wiper Function Select Circuit | BCM | DTC B3922
B3933 | Evaporator Air Temperature Circuit | HVAC | DTC B3933 w/CJ2 or DTC B3933 w/C67
B3935 | Transponder Authentication Error | TDM | DTC B3935
B396A | Liftgate Motor Control Circuit | PLGM | DTC B396A
B396B | Liftgate Motor Clutch Control Circuit | PLGM | DTC B396B
B3976 | Unconfigured Transponder/Vehicle Configuration Not Programmed | TDM | DTC B3976
C0035 | Left Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0040 | Right Front Wheel Speed Sensor Circuit | EBCM | DTC C0035-C0050
C0045 | Left Rear Wheel Speed Sensor | EBCM | DTC C0035-C0050
C0050 | Right Rear Wheel Speed Sensor | EBCM | DTC C0035-C0050
C0110 | Pump Motor Circuit | EBCM | DTC C0110
C0131 | ABS Pressure Circuit | EBCM | DTC C0131
C0161 | Antilock Brake System (ABS) Brake Switch/Sensor Circuit | EBCM | DTC C0161
C0186 | Lateral Accelerometer Circuit | EBCM | DTC C0186 or C0196
C0196 | Yaw Rate Circuit | EBCM | DTC C0186 or C0196
C0201 | Antilock Brake System (ABS) Enable Relay Contact Circuit | EBCM | DTC C0201
C0242 | Engine Control Module (ECM) Indicated TCS Malfunction | EBCM | DTC C0242 or P0856
C0245 | Wheel Speed Sensor Frequency Error | EBCM | DTC C0245
C0252 | VSES Sensors Uncorrelated | EBCM | DTC C0252
C0253 | Centering Error | EBCM | DTC C0253
C0267 | Low Brake Fluid Indicated | EBCM | DTC C0267
C0277 | Brake Pedal Position Sensor Circuit | BCM | DTC C0277 or C0890
C0297 | Brake Applied Output Circuit | BCM | DTC C0297
C0299 | Brake Booster Performance | EBCM | DTC C0299
C0393 | Rear Axle Coupling Solenoid Control Circuit | CCM | DTC C0393
C0394 | Rear Axle Coupling Temperature Sensor Circuit | CCM | DTC C0394
C0450 | Steering Assist Control Actuator Circuit | EBCM | DTC C0450
C0550 | Electronic Control Unit (ECU) Performance | CCM | DTC C0550
EBCM | DTC C0550
C0558 | Calibration Mismatch | CCM | DTC C0558
C0561 | System Disabled Information Stored | EBCM | DTC C0561
CCM | DTC C0561
C0569 | System Configuration Error | EBCM | DTC C0569
RCDLR | DTC C0569
C0710 | Steering Position Signal | EBCM | DTC C0710
C0750 | Left Front Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0755 | Right Front Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0760 | Left Rear Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0765 | Right Rear Low Tire Pressure Sensor | RCDLR | DTC C0750, C0755, C0760, or C0765
C0774 | Low Tire Pressure System Performance | EBCM | DTC C0774
C0775 | Low Tire Pressure System Sensors Not Learned | RCDLR | DTC C0775
C0856 | Traction Control Torque Reqiest Circut | EBCM, ECM | DTC C0242 or P0856
C0890 | Device Voltage Reference Output 3 Circuit | BCM | DTC C0277 or C0890
C0899 | Device Voltage Low | EBCM | DTC C0899 or C0900
C0900 | Device Voltage High | EBCM | DTC C0899 or C0900
C1100 | Brake Booster Vacuum Sensor Performance | EBCM | DTC C1100
P0008 | Engine Position System Performance Bank 1 | ECM | DTC P0008 or P0009
P0009 | Engine Position System Performance Bank 2 | ECM | DTC P0008 or P0009
P000A | Intake Camshaft Position (CMP) System Slow Response Bank 1 | ECM | DTC P000A-P000D, P0011, P0014, P0021, or P0024
P000B | Exhaust Camshaft Position (CMP) System Slow Response Bank 1 | ECM | DTC P000A-P000D, P0011, P0014, P0021, or P0024
P000C | Intake Camshaft Position (CMP) System Slow Response Bank 2 | ECM | DTC P000A-P000D, P0011, P0014, P0021, or P0024
P000D | Exhaust Camshaft Position (CMP) System Slow Response Bank 2 | ECM | DTC P000A-P000D, P0011, P0014, P0021, or P0024
P0010 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0011 | Intake Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P000A-P000D, P0011, P0014, P0021, or P0024
P0013 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 1 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0014 | Exhaust Camshaft Position (CMP) System Performance Bank 1 | ECM | DTC P000A-P000D, P0011, P0014, P0021, or P0024
P0016 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019
P0017 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 1 | ECM | DTC P0016, P0017, P0018, or P0019
P0018 | Crankshaft Position (CKP) - Intake Camshaft Position (CMP) Correlation Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019
P0019 | Crankshaft Position (CKP) - Exhaust Camshaft Position (CMP) Correlation Bank 2 | ECM | DTC P0016, P0017, P0018, or P0019
P0020 | Intake Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0021 | Intake Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P000A-P000D, P0011, P0014, P0021, or P0024
P0023 | Exhaust Camshaft Position (CMP) Actuator Solenoid Control Circuit Bank 2 | ECM | DTC P0010, P0013, P0020, P0023, P2088, P2089, P2090, P2091, P2092, P2093, P2094, or P2095
P0024 | Exhaust Camshaft Position (CMP) System Performance Bank 2 | ECM | DTC P000A-P000D, P0011, P0014, P0021, or P0024
P0030 | HO2S Heater Control Circuit Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0031 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0032 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0036 | HO2S Heater Control Circuit Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0037 | HO2S Heater Control Circuit Low Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0038 | HO2S Heater Control Circuit High Voltage Bank 1 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0050 | HO2S Heater Control Circuit Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0051 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0052 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0056 | HO2S Heater Control Circuit Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0057 | HO2S Heater Control Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0058 | HO2S Heater Control Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0030, P0031, P0032, P0036, P0037, P0038, P0050, P0051, P0052, P0056, P0057, or P0058
P0087 | Fuel Rail Pressure (FRP) Too Low | ECM | DTC P0087, P0088, or P0089
P0088 | Fuel Rail Pressure (FRP) Too High | ECM | DTC P0087, P0088, or P0089
P0089 | Fuel Pressure Regulator Performance | ECM | DTC P0087, P0088, or P0089
P0090 | Fuel Pressure Regulator Control Circuit | ECM | DTC P0090, P0091, or P0092
P0091 | Fuel Pressure Regulator Solenoid 1 Control Circuit Low Voltage | ECM | DTC P0090, P0091, or P0092
P0092 | Fuel Pressure Regulator Solenoid 1 Control Circuit High Voltage | ECM | DTC P0090, P0091, or P0092
P0100 | Mass Air Flow (MAF) Sensor Circuit | ECM | DTC P0100, P0102, or P0103
P0101 | Mass Air Flow (MAF) Sensor Performance | ECM | DTC P0101
P0102 | Mass Air Flow (MAF) Sensor Circuit Low Frequency | ECM | DTC P0100, P0102, or P0103
P0103 | Mass Air Flow (MAF) Sensor Circuit High Frequency | ECM | DTC P0100, P0102, or P0103
P0111 | Intake Air Temperature (IAT) Sensor Circuit Performance | ECM | DTC P0111-P0113
P0112 | Intake Air Temperature (IAT) Sensor Circuit Low Voltage | ECM | DTC P0111-P0113
P0113 | Intake Air Temperature (IAT) Sensor Circuit High Voltage | ECM | DTC P0111-P0113
P0116 | Engine Coolant Temperature (ECT) Sensor Performance | ECM | DTC P0116
P0117 | Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage | ECM | DTC P0117 or P0118
P0118 | Engine Coolant Temperature (ECT) Sensor Circuit High Voltage | ECM | DTC P0117 or P0118
P0119 | Engine Coolant Temperature (ECT) Sensor Circuit Intermittent | ECM | DTC P0119
P0121 | Throttle Position (TP) Sensor Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0122 | Throttle Position (TP) Sensor 1 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0123 | Throttle Position (TP) Sensor 1 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0128 | Engine Coolant Temperature (ECT) Below Thermostat Regulations Temperature | ECM | DTC P0128
P0130 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 1 | ECM | DTC P0130 or P0150
P0131 | Fuel Trim System Lean Bank 1 | ECM | DTC P0131 or P0151
P0132 | Fuel Trim System Rich Bank 1 | ECM | DTC P0132 or P0152
P0133 | HO2S Slow Response Bank 1 Sensor 1 | ECM | DTC P0133 or P0153
P0134 | HO2S Circuit Insufficient Activity Bank 1 Sensor 1 | ECM | DTC P0134 or P0154
P0135 | HO2S Heater Performance Bank 1 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161
P0137 | Fuel Trim System Lean Bank 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0138 | Fuel Trim System Rich Bank 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P013A | HO2S Slow Response Rich to Lean Bank 1 Sensor 2 | ECM | DTC P013A, P013C, P013E, or P014A
P013C | HO2S Slow Response Rich to Lean Bank 2 Sensor 2 | ECM | DTC P013A, P013C, P013E, or P014A
P013E | HO2S Delayed Response Rich to Lean Bank 1 Sensor 2 | ECM | DTC P013A, P013C, P013E, or P014A
P0140 | HO2S Circuit Insufficient Activity Bank 1 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0141 | HO2S Heater Performance Bank 1 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161
P014A | HO2S Delayed Response Rich to Lean Bank 2 Sensor 2 | ECM | DTC P013A, P013C, P013E, or P014A
P0150 | HO2S Signal Circuit Shorted to Heater Circuit Bank 2 Sensor 1 | ECM | DTC P0130 or P0150
P0151 | HO2S Circuit Low Voltage Bank 2 Sensor 1 | ECM | DTC P0131 or P0151
P0152 | HO2S Circuit High Voltage Bank 2 Sensor 1 | ECM | DTC P0132 or P0152
P0153 | HO2S Slow Response Bank 2 Sensor 1 | ECM | DTC P0133 or P0153
P0154 | HO2S Circuit Insufficient Activity Bank 2 Sensor 1 | ECM | DTC P0134 or P0154
P0155 | HO2S Heater Performance Bank 2 Sensor 1 | ECM | DTC P0135, P0141, P0155, or P0161
P0157 | HO2S Circuit Low Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0158 | HO2S Circuit High Voltage Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0160 | HO2S Circuit Insufficient Activity Bank 2 Sensor 2 | ECM | DTC P0137, P0138, P0140, P0157, P0158, or P0160
P0161 | HO2S Heater Performance Bank 2 Sensor 2 | ECM | DTC P0135, P0141, P0155, or P0161
P0191 | Fuel Rail Pressure (FRP) Sensor Performance | FPCM | DTC P0191
P0192 | Fuel Rail Pressure (FRP) Sensor Circuit Low Voltage | FPCM | DTC P0192 or P0193
P0193 | Fuel Rail Pressure (FRP) Sensor Circuit High Voltage | FPCM | DTC P0192 or P0193
P0201 | Injector 1 Control Circuit | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0202 | Injector 2 Control Circuit | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0203 | Injector 3 Control Circuit | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0204 | Injector 4 Control Circuit | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0205 | Injector 5 Control Circuit | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0206 | Injector 6 Control Circuit | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0218 | Transmission Fluid Overtemperature | TCM | DTC P0218
P0221 | Throttle Position (TP) Sensor 1 Performance | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0222 | Throttle Position (TP) Sensor 2 Circuit Low Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0223 | Throttle Position (TP) Sensor 2 Circuit High Voltage | ECM | DTC P0121, P0122, P0123, P0221, P0222, or P0223
P0231 | Fuel Pump Relay Control Circuit | ECM, FPCM | DTC P0231, P0232, or P023F
P0232 | Fuel Pump Control Circuit High Voltage | ECM, FPCM | DTC P0231, P0232, or P023F
P023F | Fuel Pump Control Circuit | ECM, FPCM | DTC P0231, P0232, or P023F
P025A | Fuel Pump Control Circuit | ECM, FPCM | DTC P025A
P0261 | Injector 1 Control Circuit Low Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0262 | Injector 1 Control Circuit High Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0264 | Injector 2 Control Circuit Low Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0265 | Injector 2 Control Circuit High Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0267 | Injector 3 Control Circuit Low Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0268 | Injector 3 Control Circuit High Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0270 | Injector 4 Control Circuit Low Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0271 | Injector 4 Control Circuit High Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0273 | Injector 5 Control Circuit Low Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0274 | Injector 5 Control Circuit High Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0276 | Injector 6 Control Circuit Low Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P0277 | Injector 6 Control Circuit High Voltage | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P029D | Injector 1 Leak | ECM | DTC P029D, P02A1, P02A5, P02A9, P02AD, or P02B1
P02A1 | Injector 2 Leak | ECM | DTC P029D, P02A1, P02A5, P02A9, P02AD, or P02B1
P02A5 | Injector 3 Leak | ECM | DTC P029D, P02A1, P02A5, P02A9, P02AD, or P02B1
P02A9 | Injector 4 Leak | ECM | DTC P029D, P02A1, P02A5, P02A9, P02AD, or P02B1
P02AD | Injector 5 Leak | ECM | DTC P029D, P02A1, P02A5, P02A9, P02AD, or P02B1
P02B1 | Injector 6 Leak | ECM | DTC P029D, P02A1, P02A5, P02A9, P02AD, or P02B1
P0300 | Engine Misfire Detected | ECM | DTC P0300-P0306
P0301 | Cylinder 1 Misfire Detected | ECM | DTC P0300-P0306
P0302 | Cylinder 2 Misfire Detected | ECM | DTC P0300-P0306
P0303 | Cylinder 3 Misfire Detected | ECM | DTC P0300-P0306
P0304 | Cylinder 4 Misfire Detected | ECM | DTC P0300-P0306
P0305 | Cylinder 5 Misfire Detected | ECM | DTC P0300-P0306
P0306 | Cylinder 6 Misfire Detected | ECM | DTC P0300-P0306
P0324 | Knock Sensor (KS) Module Performance | ECM | DTC P0324
P0326 | Knock Sensor (KS) Performance Bank 1 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0327 | Knock Sensor (KS) Circuit Low Bank 1 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0328 | Knock Sensor (KS) Circuit High Bank 1 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0331 | Knock Sensor (KS) System Performance Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0332 | Knock Sensor (KS) Circuit Low Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0333 | Knock Sensor (KS) Circuit High Bank 2 | ECM | DTC P0326, P0327, P0328, P0331, P0332, or P0333
P0335 | Crankshaft Position (CKP) Sensor Circuit | ECM | DTC P0335, P0336, or P0338
P0336 | Crankshaft Position (CKP) Sensor Performance | ECM | DTC P0335, P0336, or P0338
P0338 | Crankshaft Position (CKP) Sensor Circuit High Duty Cycle | ECM | DTC P0335, P0336, or P0338
P0341 | Intake Camshaft Position (CMP) Sensor Performance Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0342 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0343 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0346 | Intake Camshaft Position (CMP) Sensor Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0347 | Intake Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0348 | Intake Camshaft Position (CMP) Sensor Circuit High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0351 | Ignition Coil 1 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0352 | Ignition Coil 2 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0353 | Ignition Coil 3 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0354 | Ignition Coil 4 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0355 | Ignition Coil 5 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0356 | Ignition Coil 6 Control Circuit | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P0366 | Exhaust Camshaft Position (CMP) Sensor Performance Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0367 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0368 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage Bank 1 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0391 | Exhaust Camshaft Position (CMP) Sensor Performance Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0392 | Exhaust Camshaft Position (CMP) Sensor Circuit Low Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0393 | Exhaust Camshaft Position (CMP) Sensor Circuit High Voltage Bank 2 | ECM | DTC P0341, P0342, P0343, P0346, P0347, P0348, P0366, P0367, P0368, P0391, P0392, or P0393
P0420 | Catalyst System Low Efficiency Bank 1 | ECM | DTC P0420 or P0430
P0430 | Catalyst System Low Efficiency Bank 2 | ECM | DTC P0420 or P0430
P0442 | Evaporative Emission (EVAP) System Small Leak Detected | ECM | DTC P0442
P0443 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit | ECM | DTC P0443, P0458, or P0459
P0446 | Evaporative Emission (EVAP) Vent System Performance | ECM | DTC P0446
P0449 | Evaporative Emission (EVAP) Vent Solenoid Control Circuit | ECM | DTC P0449, P0498, or P0499
P0450 | Fuel Tank Pressure (FTP) Sensor Circuit | ECM | DTC P0450 or P0451
P0451 | Fuel Tank Pressure (FTP) Sensor Performance | ECM | DTC P0450 or P0451
P0452 | Fuel Tank Pressure (FTP) Sensor Circuit Low Voltage | ECM | DTC P0452 or P0453
P0453 | Fuel Tank Pressure (FTP) Sensor Circuit High Voltage | ECM | DTC P0452 or P0453
P0455 | Evaporative Emission (EVAP) System Large Leak Detected | ECM | DTC P0455 or P0497
P0458 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit Low Voltage | ECM | DTC P0443, P0458, or P0459
P0459 | Evaporative Emission (EVAP) Purge Solenoid Control Circuit High Voltage | ECM | DTC P0443, P0458, or P0459
P0461 | Fuel Level Sensor 1 Performance | ECM | DTC P0461
P0462 | Fuel Level Sensor 1 Circuit Low Voltage | ECM | DTC P0462
P0463 | Fuel Level Sensor 1 Circuit High Voltage | ECM | DTC P0463
P0464 | Fuel Level Sensor 1 Circuit Intermittent | ECM | DTC P0464
P0480 | Cooling Fan Relay 1 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0481 | Cooling Fan Relay 2 Control Circuit | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0496 | Evaporative Emission (EVAP) System Flow During Non-Purge | ECM | DTC P0496
P0497 | Evaporative Emission (EVAP) System No Flow During Purge | ECM | DTC P0455 or P0497
P0498 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit Low Voltage | ECM | DTC P0449, P0498, or P0499
P0499 | Evaporative Emission (EVAP) Vent Solenoid Valve Control Circuit High Voltage | ECM | DTC P0449, P0498, or P0499
P0506 | Idle Speed Low | ECM | DTC P0506, P0507, or P050A
P0507 | Idle Speed High | ECM | DTC P0506, P0507, or P050A
P050A | Cold Start Idle Air Control (IAC) System Performance | ECM | DTC P0506, P0507, or P050A
P0513 | Theft Deterrent Key Incorrect | ECM | DTC P0513
P0520 | Engine Oil Pressure (EOP) Switch Circuit | ECM | DTC P0520
P0532 | Air Conditioning A/C Refrigerant Pressure Sensor Circuit Low Voltage | ECM | DTC P0532 or P0533 w/C67 or DTC P0532 or P0533 w/CJ2
P0533 | Air Conditioning A/C Refrigerant Pressure Sensor Circuit High Voltage | ECM | DTC P0532 or P0533 w/C67 or DTC P0532 or P0533 w/CJ2
P0562 | System Voltage Low | ECM | DTC P0562
TCM | DTC P0562, P0563, or P2534
P0563 | System Voltage High | ECM | DTC P0563
TCM | DTC P0562, P0563, or P2534
P0571 | Brake Switch Circuit | ECM | DTC P0571
P0572 | Brake Switch Circuit 1 Low Voltage | ECM | DTC P0572 or P0573
P0573 | Brake Switch Circuit 1 High Voltage | ECM | DTC P0572 or P0573
P0575 | Cruise Control Switch Signal Circuit | ECM | DTC P0575
P0601 | Control Module Read Only Memory (ROM) | ECM | DTC P0601-P0604, P0606, or P062F
FPCM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610
Transmission Control Module (TCM) Read Only Memory (ROM) | TCM | DTC P0601-P0604 or P062F
P0602 | Control Module Read Only Memory (ROM) | ECM | DTC P0601-P0604, P0606, or P062F
FPCM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610
Transmission Control Module (TCM) Not Programmed | TCM | DTC P0601-P0604 or P062F
P0603 | Control Module Read Only Memory (ROM) | ECM | DTC P0601-P0604, P0606, or P062F
FPCM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610
Transmission Control Module (TCM) Long Term Memory Reset | TCM | DTC P0601-P0604 or P062F
P0604 | Control Module Random Access Memory (RAM) | ECM | DTC P0601-P0604, P0606, or P062F
FPCM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610
Transmission Control Module (TCM) Random Access Memory (RAM) | TCM | DTC P0601-P0604 or P062F
P0606 | Control Module Internal Performance | ECM | DTC P0601-P0604, P0606, or P062F
FPCM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610
P0615 | Starter Relay Control Circuit | ECM | DTC P0615
P0621 | Generator L-Terminal Circuit | ECM | DTC P0621
P0622 | Generator F-Terminal Circuit | ECM | DTC P0622
P062B | Control Module Fuel Injector Control Performance | ECM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610
P062F | Control Module Long Term Memory Performance | ECM | DTC P0601-P0604, P0606, or P062F
FPCM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610
Transmission Control Module (TCM) Long Term Memory Performance | TCM | DTC P0601-P0604 or P062F
P0627 | Fuel Pump Relay Control Circuit | ECM | DTC P0627, P0628, or P0629
P0628 | Fuel Pump Relay Control Circuit Low Voltage | ECM | DTC P0627, P0628, or P0629
P0629 | Fuel Pump Relay Control Circuit High Voltage | ECM | DTC P0627, P0628, or P0629
P0633 | Theft Deterrent Key Not Programmed | ECM | DTC P0633
P0634 | Transmission Control Module (TCM) Overtemperature | TCM | DTC P0634
P0638 | Throttle Actuator Control (TAC) Command Performance | ECM | DTC P0638, P2100, P2101, or P2119
P0641 | 5-Volt Reference 1 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
FPCM | DTC P0641 or P06A6
P0642 | 5-Volt Reference 1 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0643 | 5-Volt Reference 1 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0645 | Air Conditioning (A/C) Clutch Relay Control Circuit | ECM | DTC P0645 w/C67 or DTC P0645 w/CJ2
P064A | Fuel Pump Flow Control Module Performance | FPCM | DTC P1255 or P064A
P06A6 | 5-Volt Reference Circuit Performance | FPCM | DTC P0641 or P06A6
P0650 | Malfunction Indicator Lamp (MIL) Control Circuit | ECM | DTC P0650
P0651 | 5-Volt Reference 2 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0652 | 5-Volt Reference 1 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0653 | 5-Volt Reference 2 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0667 | Transmission Control Module (TCM) Temperature Sensor Performance | TCM | DTC P0667, P0668, or P0669
P0668 | Transmission Control Module (TCM) Temperature Sensor Circuit Low Voltage | TCM | DTC P0667, P0668, or P0669
P0669 | Transmission Control Module (TCM) Temperature Sensor Circuit High Voltage | TCM | DTC P0667, P0668, or P0669
P0685 | Engine Controls Ignition Relay Control Circuit | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0686 | Engine Controls Ignition Relay Control Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0687 | Engine Controls Ignition Relay Control Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0689 | Engine Controls Ignition Relay Feedback Circuit Low Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0690 | Engine Controls Ignition Relay Feedback Circuit High Voltage | ECM | DTC P0685, P0686, P0687, P0689, or P0690
P0691 | Cooling Fan Relay 1 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0692 | Cooling Fan Relay 1 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0693 | Cooling Fan Relay 2 Control Circuit Low Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0694 | Cooling Fan Relay 2 Control Circuit High Voltage | ECM | DTC P0480, P0481, P0691, P0692, P0693, or P0694
P0697 | 5-Volt Reference 3 Circuit | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0698 | 5-Volt Reference 3 Circuit Low Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P0699 | 5-Volt Reference 3 Circuit High Voltage | ECM | DTC P0641-P0643, P0651-P0653, or P0697-P0699
P069E | Fuel Pump Flow Control Module (FPCM) Requested MIL Illumination | FPCM | DTC P069E
P0700 | Transmission Control Module (TCM) Requested MIL Illumination | ECM | DTC P0700
P0703 | Brake Switch Circuit 2 | ECM | DTC P0703
P0711 | Transmission Fluid Temperature (TFT) Sensor Performance | TCM | DTC P0711, P0712, or P0713
P0712 | Transmission Fluid Temperature (TFT) Sensor Circuit Low Voltage | TCM | DTC P0711, P0712, or P0713
P0713 | Transmission Fluid Temperature (TFT) Sensor Circuit High Voltage | TCM | DTC P0711, P0712, or P0713
P0716 | Input Speed Sensor Performance | TCM | DTC P0716 or P0717
P0717 | Input Speed Sensor Circuit Low Voltage | TCM | DTC P0716 or P0717
P0722 | Output Speed Sensor (OSS) Circuit Low Voltage | TCM | DTC P0722 or P0723
P0723 | Output Speed Sensor (OSS) Intermittent | TCM | DTC P0722 or P0723
P0741 | Torque Converter Clutch (TCC) - Stuck Off | TCM | DTC P0741 or P0742
P0742 | Torque Converter Clutch (TCC) - Stuck On | TCM | DTC P0741 or P0742
P0751 | Shift Solenoid (SS) 1 Valve Performance - Stuck Off | TCM | DTC P0751 or P0752
P0752 | Shift Solenoid (SS) 1 Valve Performance - Stuck On | TCM | DTC P0751 or P0752
P0756 | Shift Solenoid (SS) 2 Valve Performance - Stuck Off | TCM | DTC P0756
P0776 | Clutch Pressure Control (PC) Solenoid 2 - Stuck Off | TCM | DTC P0776 or P0777
P0777 | Clutch Pressure Control (PC) Solenoid 2 - Stuck On | TCM | DTC P0776 or P0777
P0796 | Clutch Pressure Control (PC) Solenoid 3 - Stuck Off | TCM | DTC P0796 or P0797
P0797 | Clutch Pressure Control (PC) Solenoid 3 - Stuck On | TCM | DTC P0796 or P0797
P0815 | Upshift Switch Circuit | TCM | DTC P0815, P0816, or P0826
P0816 | Downshift Switch Circuit | TCM | DTC P0815, P0816, or P0826
P0826 | Up and Down Shift Switch Circuit | TCM | DTC P0815, P0816, or P0826
P0842 | Transmission Fluid Pressure (TFP) Switch 1 Circuit Low Voltage | TCM | DTC P0842 or P0843
P0843 | Transmission Fluid Pressure (TFP) Switch 1 Circuit High Voltage | TCM | DTC P0842 or P0843
P0851 | Park/Neutral Position (PNP) Switch Circuit Low Voltage | TCM | DTC P0850-P0852
P0852 | Park/Neutral Position (PNP) Switch Circuit High Voltage | TCM | DTC P0850-P0852
P0856 | Engine Control Module (ECM) Indicated TCS Malfunction | ECM | DTC C0242 or P0856
P0872 | Transmission Fluid Pressure (TFP) Switch 3 Circuit Low Voltage | TCM | DTC P0872 or P0873
P0873 | Transmission Fluid Pressure (TFP) Switch 3 Circuit High Voltage | TCM | DTC P0872 or P0873
P0877 | Transmission Fluid Pressure (TFP) Switch 4 Circuit Low Voltage | TCM | DTC P0877 or P0878
P0878 | Transmission Fluid Pressure (TFP) Switch 4 Circuit High Voltage | TCM | DTC P0877 or P0878
P0961 | Line Pressure Control (PC) Solenoid System Performance | TCM | DTC P0961-P0963
P0962 | Line Pressure Control (PC) Solenoid Control Circuit Low Voltage | TCM | DTC P0961-P0963
P0963 | Line Pressure Control (PC) Solenoid Control Circuit High Voltage | TCM | DTC P0961-P0963
P0965 | Clutch Pressure Control (PC) Solenoid 2 System Performance | TCM | DTC P0965-P0967
P0966 | Clutch Pressure Control (PC) Solenoid 2 Control Circuit Low Voltage | TCM | DTC P0965-P0967
P0967 | Clutch Pressure Control (PC) Solenoid 2 Control Circuit High Voltage | TCM | DTC P0965-P0967
P0969 | Clutch Pressure Control (PC) Solenoid 3 System Performance | TCM | DTC P0969-P0971
P0970 | Clutch Pressure Control (PC) Solenoid 3 Control Circuit Low Voltage | TCM | DTC P0969-P0971
P0971 | Clutch Pressure Control (PC) Solenoid 3 Control Circuit High Voltage | TCM | DTC P0969-P0971
P0973 | Shift Solenoid (SS) 1 Control Circuit Low Voltage | TCM | DTC P0973 or P0974
P0974 | Shift Solenoid (SS) 1 Control Circuit High Voltage | TCM | DTC P0973 or P0974
P0976 | Shift Solenoid (SS) 2 Control Circuit Low Voltage | TCM | DTC P0976 or P0977
P0977 | Shift Solenoid (SS) 2 Control Circuit High Voltage | TCM | DTC P0976 or P0977
P0989 | Transmission Fluid Pressure (TFP) Switch 5 Circuit Low Voltage | TCM | DTC P0989 or P0990
P0990 | Transmission Fluid Pressure (TFP) Switch 5 Circuit High Voltage | TCM | DTC P0989 or P0990
P1011 | Intake Camshaft Position(CMP) Acuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1012 | Exhaust Camshaft Position(CMP) Acuator Park Position Bank 1 | ECM | DTC P1011-P1014
P1013 | Intake Camshaft Position(CMP) Acuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1014 | Exhaust Camshaft Position(CMP) Acuator Park Position Bank 2 | ECM | DTC P1011-P1014
P1255 | Fuel Pump Flow Control Module Driver Overtemperature | ECM | DTC P1255 or P064A
P1258 | Engine Coolant Overtemperature - Protection Mode Active | ECM | DTC P1258
P1551 | Throttle Valve Rest Position Not Reached During Learn | ECM | DTC P1551
P1574 | Stop Lamp Switch Circuit | ECM | DTC P1574
P1629 | Theft Deterrent Fuel Enable Signal Not Recieved | ECM, TDM | DTC P1629
P1631 | Theft Deterrent Fuel Enable Signal Not Correct | ECM | DTC P1631
P167D | Control Module Ignition Coil Internal Circuit | ECM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610
P1684 | Transmission Control Module (TCM) Power Up Temperature Sensor Performance | TCM | DTC P1684-P1686
P1685 | Transmission Control Module (TCM) Power Up Temperature Sensor Circuit Low Voltage | TCM | DTC P1684-P1686
P1686 | Transmission Control Module (TCM) Power Up Temperature Sensor Circuit High Voltage | TCM | DTC P1684-P1686
P1751 | Shift Valve 1 Performance | TCM | DTC P1751
P1825 | Internal Mode Switch - Invalid Range | TCM | DTC P1825, P182E, or P1915 for the 6T70/6T75 transmission
P182E | Internal Mode Switch Invalid Range | TCM | DTC P1825, P182E, or P1915 for the 6T70/6T75 transmission
P1831 | Pressure Control (PC)/Shift Lock Solenoid Control Circuit Low Voltage | TCM | DTC P1831 or P1832
P1832 | Pressure Control (PC)/Shift Lock Solenoid Control Circuit High Voltage | TCM | DTC P1831 or P1832
P1876 | Up and Down Shift Enable Switch Circut Low Voltage | TCM | DTC P1876
P1915 | Internal Mode Switch Start/Wrong Range | TCM | DTC P1825, P182E, or P1915 for the 6T70/6T75 transmission
P2096 | Post Catalyst Fuel Trim System Low Limit Bank 1 | ECM | DTC P2096 or P2098
P2097 | Post Catalyst Fuel Trim System High Limit Bank 1 | ECM | DTC P2097 or P2099
P2098 | Post Catalyst Fuel Trim System Low Limit Bank 2 | ECM | DTC P2096 or P2098
P2099 | Post Catalyst Fuel Trim System High Limit Bank 2 | ECM | DTC P2097 or P2099
P2100 | Throttle Actuator Control (TAC) Motor Control Circut | ECM | DTC P0638, P2100, P2101, or P2119
P2101 | Throttle Actuator Position Performance | ECM | DTC P0638, P2100, P2101, or P2119
P2105 | Throttle Actuator Control (TAC) System - Forced Engine Shutdown | ECM | DTC P2105
P2119 | Throttle Closed Position Performance | ECM | DTC P0638, P2100, P2101, or P2119
P2122 | Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2123 | Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2127 | Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2128 | Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2138 | Accelerator Pedal Position (APP) Sensor 1-2 Correlation | ECM | DTC P2122, P2123, P2127, P2128, or P2138
P2146 | Injector Positive Voltage Control Circuit Group 1 | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P2149 | Injector Positive Voltage Control Circuit Group 2 | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P2152 | Injector Positive Voltage Control Circuit Group 3 | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P2155 | Injector Positive Voltage Control Circuit Group 4 | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P216A | Injector Positive Voltage Control Circuit Group 5 | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P216D | Injector Positive Voltage Control Circuit Group 6 | ECM | DTC P0201-P0206, P0261, P0262, P0264, P0265, P0267, P0268, P0270, P0271, P0273, P0274, P0276, P0277, P2146, P2149, P2152, P2155, P216A, or P216D
P2176 | Minimum Throttle Position Not Learned | ECM | DTC P2176
P2177 | Fuel Trim System Lean at Cruise or Accel Bank 1 | ECM | DTC P2177, P2179, P2187, or P2189
P2178 | Fuel Trim System Rich at Cruise or Accel Bank 1 | ECM | DTC P2178, P2180, P2188, or P2190
P2179 | Fuel Trim System Lean at Cruise or Accel Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2180 | Fuel Trim System Rich at Cruise or Accel Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2187 | Fuel Trim System Lean at Idle Bank 1 | ECM | DTC P2177, P2179, P2187, or P2189
P2188 | Fuel Trim System Rich at Idle Bank 1 | ECM | DTC P2178, P2180, P2188, or P2190
P2189 | Fuel Trim System Lean at Idle Bank 2 | ECM | DTC P2177, P2179, P2187, or P2189
P2190 | Fuel Trim System Rich at Idle Bank 2 | ECM | DTC P2178, P2180, P2188, or P2190
P2227 | Barometric Pressure (BARO) Sensor Performance | ECM | DTC P2227, P2228, or P2229
P2228 | Barometric Pressure (BARO) Sensor Circuit Low Voltage | ECM | DTC P2227, P2228, or P2229
P2229 | Barometric Pressure (BARO) Sensor Circuit High Voltage | ECM | DTC P2227, P2228, or P2229
P2232 | HO2S Signal Circuit Shorted to Heater Circuit Bank 1 Sensor 2 | ECM | DTC P2232 or P2235
P2235 | HO2S Signal Circuit Shorted to Heater Circuit Bank 2 Sensor 2 | ECM | DTC P2232 or P2235
P2270 | HO2S Signal Stuck Lean Bank 1 Sensor 2 | ECM | DTC P2270 or P2272
P2271 | HO2S Signal Stuck Rich Bank 1 Sensor 2 | ECM | DTC P2271 or P2273
P2272 | HO2S Signal Stuck Lean Bank 2 Sensor 2 | ECM | DTC P2270 or P2272
P2273 | HO2S Signal Stuck Rich Bank 2 Sensor 2 | ECM | DTC P2271 or P2273
P2300 | Ignition Coil 1 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2301 | Ignition Coil 1 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2303 | Ignition Coil 2 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2304 | Ignition Coil 2 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2306 | Ignition Coil 3 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2307 | Ignition Coil 3 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2309 | Ignition Coil 4 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2310 | Ignition Coil 4 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2312 | Ignition Coil 5 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2313 | Ignition Coil 5 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2315 | Ignition Coil 6 Control Circuit Low Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2316 | Ignition Coil 6 Control Circuit High Voltage | ECM | DTC P0351-P0356, P2300, P2301, P2303, P2304, P2306, P2307, P2309, P2310, P2312, P2313, P2315, or P2316
P2534 | Ignition 1 Switch Circuit Low Voltage | TCM | DTC P0562, P0563, or P2534
ECM | DTC P2534
P2544 | Transmission Torque Request Circuit | ECM, TCM | DTC P2544
P2610 | Control Module Ignition Off Timer Performance | ECM | DTC P0601-P0604, P0606, P0607, P062B, P0167D, P2107, or P2610
P2635 | Fuel Pump Flow Performance | FPCM | DTC P2635
P2714 | Clutch Pressure Control (PC) Solenoid 4 - Stuck Off | TCM | DTC P2714 or P2715
P2715 | Clutch Pressure Control (PC) Solenoid 4 - Stuck On | TCM | DTC P2714 or P2715
P2719 | Clutch Pressure Control (PC) Solenoid 4 System Performance | TCM | DTC P2719-P2721
P2720 | Clutch Pressure Control (PC) Solenoid 4 Control Circuit Low Voltage | TCM | DTC P2719-P2721
P2721 | Clutch Pressure Control (PC) Solenoid 4 Control Circuit High Voltage | TCM | DTC P2719-P2721
P2723 | Clutch Pressure Control (PC) Solenoid 5 - Stuck Off | TCM | DTC P2723 or P2724
P2724 | Clutch Pressure Control (PC) Solenoid 5 - Stuck On | TCM | DTC P2723 or P2724
P2728 | Clutch Pressure Control (PC) Solenoid 5 System Performance | TCM | DTC P2728-P2730
P2729 | Clutch Pressure Control (PC) Solenoid 5 Control Circuit Low Voltage | TCM | DTC P2728-P2730
P2730 | Clutch Pressure Control (PC) Solenoid 5 Control Circuit High Voltage | TCM | DTC P2728-P2730
P2762 | Torque Converter Clutch (TCC) Pressure Control Solenoid System Performance | TCM | DTC P2762, P2763, or P2764
P2763 | Torque Converter Clutch (TCC) Pressure Control Solenoid Control Circuit Low Voltage | TCM | DTC P2762, P2763, or P2764
P2764 | Torque Converter Clutch (TCC) Pressure Control Solenoid Control Circuit High Voltage | TCM | DTC P2762, P2763, or P2764
U0020 | Low Speed CAN Communication Bus Performance | RCDLR,ROS,SDM,TDM | DTC U0020
U0073 | Control Module Communication Bus Off | DDM, DRR, ECM, EBCM, HVAC, IPC, MSM, PLGM, PPS, Radio, RCDLR, ROS, RSA, TCM, TDM, UPA, VCIM | DTC U0073 or U2100
U0100-0299 | Lost Communication With XXX Control Module | -- | DTC U0100-U0299
U1500 | Inter-Device Dedicated Bus 1 Short to Battery | DDM, FPDM | DTC U1500, U1511, U1512, or U1513
U1511 | Inter-device Dedicated Bus Lost Communication With Device 1 | DDM, FPDM | DTC U1500, U1511, U1512, or U1513
U1512 | Inter-device Dedicated Bus Lost Communication With Device 2 | DDM, FPDM | DTC U1500, U1511, U1512, or U1513
U1814 | Powertrain High Speed Communication Enable Circuit | BCM | DTC U1814
U2099 | High Speed Communication Enable Circuit | BCM | DTC U2099
U2100 | Controller Area Network (CAN) Bus Communication | DDM, DRR, ECM, EBCM, HVAC, IPC, MSM, PLGM, PPS, Radio, RCDLR, ROS, RSA, TCM, TDM, UPA, VCIM | DTC U0073 or U2100
U2105- 2199 | Lost Communications With Yaw Rate Sensor (YRS) | EBCM | DTC U2105-U2199