For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Seat Belt Anchor Finish Cover
2 | Front Seat Adjuster Switch Mounting Plate

#### Procedure

1. Using a non-metallic flat-bladed tool, release the retainer tabs starting at the rear edge and working forward while pulling outward on the mounting plate.
2. Disconnect the electrical connectors from the switch assemblies.

3 | Front Seat Outer Recliner Finish Cover Screw (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
4 | Front Seat Outer Recliner Finish Cover