For 1990-2009 cars

## Front Fog Lamp Bulb Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.
2. Disconnect the electrical connector from the fog lamp bulb socket.

1 | Front Fog Lamp Bulb Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

Twist the bulb socket counterclockwise and remove the fog lamp bulb.

## Front Fog Lamp Bulb Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Front Fog Lamp Bulb Socket Electrical Connector

#### Procedure

Disengage the electrical connector from the fog lamp bulb socket.

2 | Front Fog Lamp Bulb Socket Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

Rotate the bulb socket counterclockwise and remove from the fog lamp assembly.

## Front Fog Lamp Bulb Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front wheelhouse liner in order to access the fog lamp bulb. Refer to Front Wheelhouse Front Liner Replacement.
2. Disconnect the fog lamp bulb socket electrical connectors.

1 | Front Fog Lamp Bulb (Qty: 2) Tip Rotate the bulb sockets and remove.