For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Seat Adjuster Handle Finish Cover

#### Procedure

Insert a non-metallic flat-bladed tool at the top edge of the cover and carefully push downward and outward to remove the cover.

2 | Front Seat Adjuster Handle Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
3 | Front Seat Adjuster Handle