For 1990-2009 cars

Connector 1: | A/C Compressor Clutch
Connector 2: | A/C Refrigerant Pressure Sensor
Connector 3: | Accelerator Pedal Position (APP) Sensor
Connector 4: | Accessory AC/DC Power Control Module X1 (KV1)
Connector 5: | Accessory AC/DC Power Control Module X2 (KV1)
Connector 6: | Accessory Power Outlet - 110V AC (KV1)
Connector 7: | Accessory Power Outlet - Center Console
Connector 8: | Accessory Power Outlet - I/P
Connector 9: | Accessory Power Outlet - Rear
Connector 10: | Accessory Power Outlet - Rear Console (DK1)
Connector 11: | Adaptive Forward Lighting (AFL) Motor - Left (TSH)
Connector 12: | Adaptive Forward Lighting (AFL) Motor - Right (TSH)
Connector 13: | Air Temperature Actuator - Auxiliary
Connector 14: | Air Temperature Actuator - Left (CJ2)
Connector 15: | Air Temperature Actuator - Right (CJ2)
Connector 16: | Air Temperature Actuator (C67)
Connector 17: | Air Temperature Sensor - Lower Left (CJ2)
Connector 18: | Air Temperature Sensor - Lower Right (CJ2)
Connector 19: | Air Temperature Sensor - Upper Left (CJ2)
Connector 20: | Air Temperature Sensor - Upper Right (CJ2)
Connector 21: | Ambient Light Sensor (C67)
Connector 22: | Ambient Temperature Sensor
Connector 23: | Audio Amplifier X1 (UQA or UQS)
Connector 24: | Audio Amplifier X2 (UQA or UQS)
Connector 25: | Audio Amplifier X3 (UQA or UQS)
Connector 26: | Audio/Video Adapter (U42)
Connector 27: | Automatic Transmission
Connector 28: | Automatic Transmission Internal Mode Switch (IMS)
Connector 29: | Automatic Transmission Manual Shift Switch
Connector 30: | Back Up Lamp - Left (W49)
Connector 31: | Back Up Lamp - Left (WDA)
Connector 32: | Back Up Lamp - Left (Z88)
Connector 33: | Back Up Lamp - Right (W49)
Connector 34: | Back Up Lamp - Right (WDA)
Connector 35: | Back Up Lamp - Right (Z88)
Connector 36: | Battery (-)
Connector 37: | Battery (+)
Connector 38: | Battery Current Sensor
Connector 39: | Blower Motor
Connector 40: | Blower Motor - Auxiliary
Connector 41: | Blower Motor Control Module - Auxiliary X1
Connector 42: | Blower Motor Control Module - Auxiliary X2
Connector 43: | Blower Motor Control Module X1
Connector 44: | Blower Motor Control Module X2
Connector 45: | Body Control Module (BCM) X1
Connector 46: | Body Control Module (BCM) X2
Connector 47: | Body Control Module (BCM) X3
Connector 48: | Body Control Module (BCM) X4
Connector 49: | Body Control Module (BCM) X5
Connector 50: | Body Control Module (BCM) X6
Connector 51: | Body Control Module (BCM) X7
Connector 52: | Brake Booster Pump - Auxiliary
Connector 53: | Brake Booster Vacuum Sensor
Connector 54: | Brake Fluid Level Switch
Connector 55: | Brake Pedal Position Sensor
Connector 56: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Exhaust (LLT)
Connector 57: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Exhaust (LLT)
Connector 58: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Intake (LLT)
Connector 59: | Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Intake (LLT)
Connector 60: | Camshaft Position (CMP) Sensor - Bank 1 Exhaust (LLT)
Connector 61: | Camshaft Position (CMP) Sensor - Bank 2 Exhaust (LLT)
Connector 62: | Camshaft Position (CMP) Sensor - Bank 1 Intake (LLT)
Connector 63: | Camshaft Position (CMP) Sensor - Bank 2 Intake (LLT)
Connector 64: | Cellular Telephone Microphone (UE1)
Connector 65: | Center High Mounted Stop Lamp (CHMSL) (W49)
Connector 66: | Center High Mounted Stop Lamp (CHMSL) (without W49)
Connector 67: | Clock (W49)
Connector 68: | Console Flood Lamp
Connector 69: | Courtesy/Reading Lamps - 2nd Row (without U42)
Connector 70: | Courtesy/Reading Lamps - 2nd Row X1 (C3U with U42)
Connector 71: | Courtesy/Reading Lamps - 2nd Row X2 (C3U with U42)
Connector 72: | Crankshaft Position (CKP) Sensor (LLT)
Connector 73: | Data Link Connector (DLC)
Connector 74: | Data Link Resistor (without MH6)
Connector 75: | Daytime Running Lamp (DRL) - Left (W49 or Z88 with T61)
Connector 76: | Daytime Running Lamp (DRL) - Left (WDA with T61)
Connector 77: | Daytime Running Lamp (DRL) - Right (W49 or Z88 with T61)
Connector 78: | Daytime Running Lamp (DRL) - Right (WDA with T61)
Connector 79: | Digital Radio Receiver (U2K or UBS)
Connector 80: | Digital Video Disc (DVD) Display (U42)
Connector 81: | Door Control Module - Passenger X1 (AXC or AXE)
Connector 82: | Door Control Module - Passenger X2 (AXC or AXE)
Connector 83: | Door Control Module - Passenger X3 (AXC or AXE)
Connector 84: | Door Control Module - Passenger X4 (AXC or AXE)
Connector 85: | Door Control Module - Passenger X7 (AXC or AXE)
Connector 86: | Door Latch - Driver
Connector 87: | Door Latch - Left Rear
Connector 88: | Door Latch - Passenger
Connector 89: | Door Latch - Right Rear
Connector 90: | Door Lock Switch - Driver (without AXC or AXE)
Connector 91: | Door Lock Switch - Passenger (without AXC or AXE)
Connector 92: | Driver Door Module (DDM) X1 (AXC or AXE)
Connector 93: | Driver Door Module (DDM) X2 (AXC or AXE)
Connector 94: | Driver Door Module (DDM) X3 (AXC or AXE)
Connector 95: | Driver Door Module (DDM) X4 (AXC or AXE)
Connector 96: | Driver Door Module (DDM) X7 (AXC or AXE)
Connector 97: | Driver Information Center (DIC) Switch (UH9)
Connector 98: | Electronic Brake Control Module (EBCM)
Connector 99: | Electronic Compass Module (U80)
Connector 100: | Engine Control Module (ECM) X1 (LLT)
Connector 101: | Engine Control Module (ECM) X2 (LLT)
Connector 102: | Engine Coolant Temperature (ECT) Sensor (LLT)
Connector 103: | Engine Cooling Fan - Left and Engine Cooling Fan - Right
Connector 104: | Engine Oil Pressure (EOP) Switch (LLT)
Connector 105: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LLT)
Connector 106: | Evaporative Emissions (EVAP) Canister Vent Solenoid Valve (LLT)
Connector 107: | Evaporator Temperature Sensor
Connector 108: | Fog Lamp - Left Front (W49 or WDA with T96)
Connector 109: | Fog Lamp - Left Front (Z88)
Connector 110: | Fog Lamp - Right Front (W49 or WDA with T96)
Connector 111: | Fog Lamp - Right Front (Z88)
Connector 112: | Fuel Injector 1 (LLT)
Connector 113: | Fuel Injector 2 (LLT)
Connector 114: | Fuel Injector 3 (LLT)
Connector 115: | Fuel Injector 4 (LLT)
Connector 116: | Fuel Injector 5 (LLT)
Connector 117: | Fuel Injector 6 (LLT)
Connector 118: | Fuel Pump and Sender Assembly (LLT)
Connector 119: | Fuel Pump Flow Control Module (LLT)
Connector 120: | Fuel Pressure Sensor (LLT)
Connector 121: | Fuel Rail Pressure (FRP) Sensor (LLT)
Connector 122: | Fuel Tank Pressure (FTP) Sensor (LLT)
Connector 123: | Garage Door Opener (UG1)
Connector 124: | Generator X1
Connector 125: | Generator X2
Connector 126: | Hazard Switch
Connector 127: | Head Up Display (HUD) (UV6)
Connector 128: | Head Up Display (HUD) Switch (UV6)
Connector 129: | Headlamp - Left (WDA with TVD)
Connector 130: | Headlamp - Left (Z88 with TVD or W49)
Connector 131: | Headlamp - Left High Beam (WDA without TVD)
Connector 132: | Headlamp - Left High Beam (X88)
Connector 133: | Headlamp - Left High Beam (Z88 without TVD)
Connector 134: | Headlamp - Left High Beam Solenoid (W49)
Connector 135: | Headlamp - Left High Beam Solenoid (WDA with TVD)
Connector 136: | Headlamp - Left High Beam Solenoid (Z88 with TVD)
Connector 137: | Headlamp - Left Low Beam (WDA without TVD)
Connector 138: | Headlamp - Left Low Beam (X88 or Z88 without TVD)
Connector 139: | Headlamp - Right (WDA with TVD)
Connector 140: | Headlamp - Right (Z88 with TVD or W49)
Connector 141: | Headlamp - Right High Beam (WDA without TVD)
Connector 142: | Headlamp - Right High Beam (X88)
Connector 143: | Headlamp - Right High Beam (Z88 without TVD)
Connector 144: | Headlamp - Right High Beam Solenoid (W49)
Connector 145: | Headlamp - Right High Beam Solenoid (WDA with TVD)
Connector 146: | Headlamp - Right High Beam Solenoid (Z88 with TVD)
Connector 147: | Headlamp - Right Low Beam (WDA without TVD)
Connector 148: | Headlamp - Right Low Beam (X88 or Z88 without TVD)
Connector 149: | Headlamp Control Module - Left High Beam (W49)
Connector 150: | Headlamp Control Module - Right High Beam (W49)
Connector 151: | Headlamp Control Module (TSH)
Connector 152: | Headlamp Switch
Connector 153: | Heated and Cooled Seat Switch - Driver (KB6)
Connector 154: | Heated and Cooled Seat Switch - Passenger (KB6)
Connector 155: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LLT)
Connector 156: | Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LLT)
Connector 157: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LLT)
Connector 158: | Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LLT)
Connector 159: | Heated Seat Control Module - Driver X1 (KA1 without AG3)
Connector 160: | Heated Seat Control Module - Driver X2 (KA1 without AG3)
Connector 161: | Heated Seat Control Module - Driver X3 (KA1 without AG3)
Connector 162: | Heated Seat Control Module - Driver X4 (KA1 without AG3)
Connector 163: | Heated Seat Element - Driver Back (KA1)
Connector 164: | Heated Seat Element - Driver Back (KB6)
Connector 165: | Heated Seat Element - Driver Cushion (KA1)
Connector 166: | Heated Seat Element - Driver Cushion (KB6)
Connector 167: | Heated Seat Element - Passenger Back (KA1)
Connector 168: | Heated Seat Element - Passenger Back (KB6)
Connector 169: | Heated Seat Element - Passenger Cushion (KA1)
Connector 170: | Heated Seat Element - Passenger Cushion (KB6)
Connector 171: | Heated Seat Switch - Driver (KA1)
Connector 172: | Heated Seat Switch - Passenger (KA1)
Connector 173: | High Pressure Fuel Pump (LLT)
Connector 174: | Hood Ajar Switch (BTV)
Connector 175: | Horn - High Note
Connector 176: | Horn - Low Note
Connector 177: | Horn Switch X1
Connector 178: | Horn Switch X2
Connector 179: | HVAC Control Assembly - Auxiliary (without UK6)
Connector 180: | HVAC Control Module X1
Connector 181: | HVAC Control Module X2 (C67)
Connector 182: | HVAC Control Module X2 (CJ2)
Connector 183: | HVAC Control Module X3
Connector 184: | HVAC Control Module X4
Connector 185: | I/P Switch Assembly
Connector 186: | Ignition Coil 1 (LLT)
Connector 187: | Ignition Coil 2 (LLT)
Connector 188: | Ignition Coil 3 (LLT)
Connector 189: | Ignition Coil 4 (LLT)
Connector 190: | Ignition Coil 5 (LLT)
Connector 191: | Ignition Coil 6 (LLT)
Connector 192: | Ignition Lock Cylinder Control Actuator
Connector 193: | Ignition Switch
Connector 194: | Inflatable Restraint Front End Sensor - Left
Connector 195: | Inflatable Restraint Front End Sensor - Right
Connector 196: | Inflatable Restraint Front Passenger Presence System (PPS) Sensor
Connector 197: | Inflatable Restraint I/P Module
Connector 198: | Inflatable Restraint I/P Module Indicator
Connector 199: | Inflatable Restraint Roof Rail Module - Driver
Connector 200: | Inflatable Restraint Roof Rail Module - Passenger
Connector 201: | Inflatable Restraint Sensing and Diagnostic Module (SDM)
Connector 202: | Inflatable Restraint Side Impact Module - Left
Connector 203: | Inflatable Restraint Side Impact Module - Right
Connector 204: | Inflatable Restraint Side Impact Sensor (SIS) - Left Front
Connector 205: | Inflatable Restraint Side Impact Sensor (SIS) - Left Rear
Connector 206: | Inflatable Restraint Side Impact Sensor (SIS) - Right Front
Connector 207: | Inflatable Restraint Side Impact Sensor (SIS) - Right Rear
Connector 208: | Inflatable Restraint Steering Wheel Module Coil X1
Connector 209: | Inflatable Restraint Steering Wheel Module Coil X2
Connector 210: | Inflatable Restraint Steering Wheel Module Coil X3
Connector 211: | Inflatable Restraint Steering Wheel Module X1
Connector 212: | Inflatable Restraint Steering Wheel Module X2
Connector 213: | Inflatable Restraint Vehicle Rollover Sensor
Connector 214: | Infrared Transmitter (U42)
Connector 215: | Input Speed Sensor (ISS)
Connector 216: | Inside Air Temperature Sensor (CJ2)
Connector 217: | Inside Rearview Mirror
Connector 218: | Instrument Panel Cluster (IPC)
Connector 219: | Knock Sensor (KS) 1 (LLT)
Connector 220: | Knock Sensor (KS) 2 (LLT)
Connector 221: | License Lamp - Left
Connector 222: | License Lamp - Right
Connector 223: | Liftgate Control Switch - Exterior
Connector 224: | Liftgate Control Switch - Interior (TB5)
Connector 225: | Liftgate Courtesy Lamp - Left
Connector 226: | Liftgate Courtesy Lamp - Right
Connector 227: | Liftgate Latch Assembly (TB4)
Connector 228: | Liftgate Latch Assembly (TB5)
Connector 229: | Liftgate Module (LGM) X1 (TB5)
Connector 230: | Liftgate Module (LGM) X2 (TB5)
Connector 231: | Liftgate Module (LGM) X3 (TB5)
Connector 232: | Liftgate Motor Assembly X1 (TB5)
Connector 233: | Liftgate Motor Assembly X2 (TB5)
Connector 234: | Liftgate Object Sensor - Left (TB5)
Connector 235: | Liftgate Object Sensor - Right (TB5)
Connector 236: | Marker Lamp - Left Front (W49 or Z88)
Connector 237: | Marker Lamp - Left Front (WDA)
Connector 238: | Marker Lamp - Left Front (X88)
Connector 239: | Marker Lamp - Left Rear (W49)
Connector 240: | Marker Lamp - Left Rear (WDA)
Connector 241: | Marker Lamp - Left Rear (X88)
Connector 242: | Marker Lamp - Right Front (W49 or Z88)
Connector 243: | Marker Lamp - Right Front (WDA)
Connector 244: | Marker Lamp - Right Front (X88)
Connector 245: | Marker Lamp - Right Rear (W49)
Connector 246: | Marker Lamp - Right Rear (WDA)
Connector 247: | Marker Lamp - Right Rear (X88)
Connector 248: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LLT)
Connector 249: | Memory Seat Adjuster Switch - Driver (AG3)
Connector 250: | Memory Seat Module (MSM) X1 (AG3)
Connector 251: | Memory Seat Module (MSM) X2 (AG3)
Connector 252: | Memory Seat Module X3 (MSM) (AG3)
Connector 253: | Memory Seat Module (MSM) X4 (AG3)
Connector 254: | Memory Seat Module (MSM) X5 (AG3)
Connector 255: | Memory Seat Module (MSM) X6 (AG3)
Connector 256: | Memory Seat Module (MSM) X7 (AG3)
Connector 257: | Mode Actuator
Connector 258: | Mode Actuator - Auxiliary
Connector 259: | Object Alarm Module X1 (UD7)
Connector 260: | Object Alarm Module X2 (UD7)
Connector 261: | Object Alarm Sensor - Left Rear Corner (UD7)
Connector 262: | Object Alarm Sensor - Left Rear Middle (UD7)
Connector 263: | Object Alarm Sensor - Right Rear Corner (UD7)
Connector 264: | Object Alarm Sensor - Right Rear Middle (UD7)
Connector 265: | Output Speed Sensor (OSS)
Connector 266: | Outside Rearview Mirror - Driver (DL6 or DS3)
Connector 267: | Outside Rearview Mirror - Driver X1 (DNP or DNT)
Connector 268: | Outside Rearview Mirror - Driver X2 (DNP or DNT)
Connector 269: | Outside Rearview Mirror - Passenger (DL6 or DS3)
Connector 270: | Outside Rearview Mirror - Passenger X1 (DNP or DNT)
Connector 271: | Outside Rearview Mirror - Passenger X2 (DNP or DNT)
Connector 272: | Outside Rearview Mirror Switch (DL6 or DS3)
Connector 273: | Overhead Console Courtesy/Reading Lamps - Front
Connector 274: | Overhead Console Courtesy/Reading Lamps - Rear
Connector 275: | Park Brake Switch
Connector 276: | Park Lamp - Left Rear (W49)
Connector 277: | Park Lamp - Left Rear (Z88)
Connector 278: | Park Lamp - Right Rear (W49)
Connector 279: | Park Lamp - Right Rear (Z88)
Connector 280: | Park/Turn Signal Lamp - Left (X88)
Connector 281: | Park/Turn Signal Lamp - Right (X88)
Connector 282: | PRNDL Lamp
Connector 283: | Radio X1
Connector 284: | Radio X2
Connector 285: | Radio X3 (U42)
Connector 286: | Radio X4 (U3R or UVB or UZR)
Connector 287: | Radio/HVAC Control - Auxiliary X1 (UK6)
Connector 288: | Radio/HVAC Control - Auxiliary X2 (UK6)
Connector 289: | Rear Differential Clutch Control Module X1 (MH6)
Connector 290: | Rear Differential Clutch Control Module X2 (MH6)
Connector 291: | Rear Parking Assist (RPA) Display (UD7)
Connector 292: | Rear Seat Audio (RSA) Control (RCA)
Connector 293: | Rear Window Defogger Grid X1
Connector 294: | Rear Window Defogger Grid X2
Connector 295: | Rear Window Washer Fluid Pump
Connector 296: | Rear Window Wiper Motor (without X88)
Connector 297: | Rear Window Wiper Motor (X88)
Connector 298: | Rearview Camera (UVC)
Connector 299: | Recirculation Actuator
Connector 300: | Remote Control Door Lock Receiver (RCDLR)
Connector 301: | Seat Adjuster Switch - Driver (AG1)
Connector 302: | Seat Adjuster Switch - Driver (AG3)
Connector 303: | Seat Adjuster Switch - Driver (AH5)
Connector 304: | Seat Adjuster Switch - Passenger (AAQ)
Connector 305: | Seat Adjuster Switch - Passenger (AG2)
Connector 306: | Seat Back Ventilation Heating and Cooling Module -- Driver (KB6)
Connector 307: | Seat Back Ventilation Heating and Cooling Module -- Passenger (KB6)
Connector 308: | Seat Belt Buckle - Driver
Connector 309: | Seat Belt Buckle - Passenger
Connector 310: | Seat Belt Buckle Pretensioner - Driver
Connector 311: | Seat Belt Buckle Pretensioner - Passenger
Connector 312: | Seat Belt Retractor Pretensioner - Driver
Connector 313: | Seat Belt Retractor Pretensioner - Passenger
Connector 314: | Seat Cushion Ventilation Heating and Cooling Module -- Driver (KB6)
Connector 315: | Seat Cushion Ventilation Heating and Cooling Module -- Passenger (KB6)
Connector 316: | Seat Front Vertical Motor - Driver (AG1 or AG3 or AH5)
Connector 317: | Seat Front Vertical Motor Position Sensor - Driver (AG3)
Connector 318: | Seat Horizontal Motor - Driver (AG1 or AG3 or AH5)
Connector 319: | Seat Horizontal Motor - Passenger (AAQ or AG2)
Connector 320: | Seat Horizontal Motor Position Sensor - Driver (AG3)
Connector 321: | Seat Lumbar Horizontal Motor - Driver (AG3 or AH5)
Connector 322: | Seat Lumbar Horizontal Motor - Passenger (AAQ)
Connector 323: | Seat Lumbar Switch - Driver (AG3 or AH5)
Connector 324: | Seat Lumbar Switch - Passenger (AAQ)
Connector 325: | Seat Rear Vertical Motor - Driver (AG1 or AG3 or AH5)
Connector 326: | Seat Rear Vertical Motor Position Sensor - Driver (AG3)
Connector 327: | Seat Recline Motor - Driver (AG3 or AH5)
Connector 328: | Seat Recline Motor - Passenger (AAQ)
Connector 329: | Seat Recline Position Sensor - Driver (AG3)
Connector 330: | Speaker - Center I/P (UQA or UQS)
Connector 331: | Speaker - Left Front (UQA or UQS)
Connector 332: | Speaker - Left Front (UQF)
Connector 333: | Speaker - Left Front Tweeter
Connector 334: | Speaker - Left Rear (UQA or UQS without W49)
Connector 335: | Speaker - Left Rear (UQA or UQS with W49)
Connector 336: | Speaker - Left Rear (UQF)
Connector 337: | Speaker - Left Rear Compartment (UQA or UQS)
Connector 338: | Speaker - Right Front (UQA or UQS)
Connector 339: | Speaker - Right Front (UQF)
Connector 340: | Speaker - Right Front Tweeter
Connector 341: | Speaker - Right Rear (UQA or UQS without W49)
Connector 342: | Speaker - Right Rear (UQA or UQS with W49)
Connector 343: | Speaker - Right Rear (UQF)
Connector 344: | Speaker - Right Rear Compartment (UQA or UQS)
Connector 345: | Speaker - Subwoofer (UQA or UQS)
Connector 346: | Starter Motor X1 (LLT)
Connector 347: | Starter Motor X2 (LLT)
Connector 348: | Steering Column Tilt/Telescope Actuator X1 (N38)
Connector 349: | Steering Column Tilt/Telescope Actuator X2 (N38)
Connector 350: | Steering Wheel Control Switch - Left
Connector 351: | Steering Wheel Control Switch - Right (UK3)
Connector 352: | Steering Wheel Speed Position Sensor
Connector 353: | Steering Wheel/Column Tilt/Telescope Switch (N38)
Connector 354: | Sunload Sensor (CJ2)
Connector 355: | Sunroof Control Module (C3U)
Connector 356: | Sunroof Shade Module (C3U)
Connector 357: | Sunroof Shade Switch (C3U)
Connector 358: | Sunroof Switch (C3U)
Connector 359: | Sunshade - Left (DH6)
Connector 360: | Sunshade - Right (DH6)
Connector 361: | Tail Lamp - Left (Z88)
Connector 362: | Tail Lamp - Right (Z88)
Connector 363: | Tail/Stop and Turn Signal Lamp - Left (W49 or WDA or X88)
Connector 364: | Tail/Stop and Turn Signal Lamp - Right (W49 or WDA or X88)
Connector 365: | Theft Deterrent Module (TDM)
Connector 366: | Throttle Body (LLT)
Connector 367: | Trailer Connector (V92)
Connector 368: | Turn Signal Lamp - Left Front (W49 or Z88)
Connector 369: | Turn Signal Lamp - Lower Left Front (WDA)
Connector 370: | Turn Signal Lamp - Lower Right Front (WDA)
Connector 371: | Turn Signal Lamp - Right Front (W49 or Z88)
Connector 372: | Turn Signal Lamp - Upper Left Front (WDA)
Connector 373: | Turn Signal Lamp - Upper Right Front (WDA)
Connector 374: | Turn Signal/Multifunction Switch X1
Connector 375: | Turn Signal/Multifunction Switch X2
Connector 376: | Variable Effort Steering Actuator (NV7)
Connector 377: | Vehicle Communications Interface Module (VCIM) X1 (UE1)
Connector 378: | Vehicle Communications Interface Module (VCIM) X2 (UE1)
Connector 379: | Vehicle Communications Interface Module (VCIM) X3 (UE1)
Connector 380: | Wheel Speed Sensor (WSS) - Left Front
Connector 381: | Wheel Speed Sensor (WSS) - Left Rear
Connector 382: | Wheel Speed Sensor (WSS) - Right Front
Connector 383: | Wheel Speed Sensor (WSS) - Right Rear
Connector 384: | Window Motor - Driver (AXC or AXE)
Connector 385: | Window Motor - Driver (without AXC or AXE)
Connector 386: | Window Motor - Left Rear
Connector 387: | Window Motor - Passenger (AXC)
Connector 388: | Window Motor - Passenger (without AXC)
Connector 389: | Window Motor - Right Rear
Connector 390: | Window Switch - Driver X1 (without AXC or AXE)
Connector 391: | Window Switch - Driver X2 (without AXC or AXE)
Connector 392: | Window Switch - Left Rear
Connector 393: | Window Switch - Passenger (without AXC or AXE)
Connector 394: | Window Switch - Right Rear
Connector 395: | Windshield Washer Fluid Level Switch
Connector 396: | Windshield Washer Fluid Pump
Connector 397: | Windshield Washer Solvent Heater X1 (XA7)
Connector 398: | Windshield Washer Solvent Heater X2 (XA7)
Connector 399: | Windshield Wiper Motor
Connector 400: | Yaw and Lateral Accelerometer Sensor

### A/C Compressor Clutch

#### Connector Part Information

- OEM: 7282-5548-30
- Service: 88953303
- Description: 2-Way M YESC Weather Pack (BK)

#### Terminal Part Information

- Terminal/Tray: 7114-4103-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-3 (GY)

#### A/C Compressor Clutch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 59 | A/C Compressor Clutch Voltage
2 | 1 BK | 1050 | Ground

### A/C Refrigerant Pressure Sensor

#### Connector Part Information

- OEM: 15477863
- Service: 88988301
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### A/C Refrigerant Pressure Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 5514 | Low Reference
2 | 0.5 GY | 2700 | 5-Volt Reference
3 | 0.5 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal

### Accelerator Pedal Position (APP) Sensor

#### Connector Part Information

- OEM: 19177553
- Service: 88988944
- Description: 6-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Accelerator Pedal Position (APP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU | 1272 | Low Reference
B | 0.35 L-BU | 1162 | APP Sensor 2 Signal
C | 0.35 TN | 1274 | 5-Volt Reference
D | 0.35 BN | 1271 | Low Reference
E | 0.35 D-BU | 1161 | APP Sensor 1 Signal
F | 0.35 WH/BK | 1164 | 5-Volt Reference

### Accessory AC/DC Power Control Module X1 (KV1)

#### Connector Part Information

- OEM: 6098-4542
- Service: See Catalog
- Description: 6-Way F 2.8 Series (OG)

#### Terminal Part Information

- Terminal/Tray: 8100-4444/22
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

#### Accessory AC/DC Power Control Module X1 (KV1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.8 D-BU | 6807 | 120 VAC Inverter Control
3 | -- | -- | Not Used
4 | 0.8 RD | 5684 | 120 VAC Phase B
5 | -- | -- | Not Used
6 | 0.8 BK | 5683 | 120 VAC Phase A

### Accessory AC/DC Power Control Module X2 (KV1)

#### Connector Part Information

- OEM: 6098-4539
- Service: 88987988
- Description: 2-Way F Receptacle 6.3 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4122-02/10
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Accessory AC/DC Power Control Module X2 (KV1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 BK | 650 | Ground
2 | 3 RD/WH | 2740 | Battery Positive Voltage

### Accessory Power Outlet - 110V AC (KV1)

#### Connector Part Information

- OEM: 6098-4536
- Service: See Catalog
- Description: 6-Way F 1.5 (OG)

#### Terminal Part Information

- Pins: 1, 3, 6
- Terminal/Tray: 8240-0128/22
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 4
- Terminal/Tray: 8240-0127/22
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Accessory Power Outlet - 110V AC (KV1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 D-BU | 6807 | 120 VAC Inverter Control
2 | -- | -- | Not Used
3 | 0.8 RD | 5684 | 120 VAC Phase B
4 | 0.35 YE | 43 | Ignition Voltage
5 | -- | -- | Not Used
6 | 0.8 BK | 5683 | 120 VAC Phase A

### Accessory Power Outlet - Center Console

#### Connector Part Information

- OEM: 12176836
- Service: 15305923
- Description: 3-Way F Metri-Pack 280 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Accessory Power Outlet - Center Console

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 RD/WH | 2540 | Battery Positive Voltage
B | -- | -- | Not Used
C | 1 BK | 750 | Ground

### Accessory Power Outlet - I/P

#### Connector Part Information

- OEM: 12176836
- Service: 15305923
- Description: 3-Way F Metri-Pack 280 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Accessory Power Outlet - I/P

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 RD/WH | 2540 | Battery Positive Voltage
B | -- | -- | Not Used
C | 1 BK | 750 | Ground

### Accessory Power Outlet - Rear

#### Connector Part Information

- OEM: 12176836
- Service: 15305923
- Description: 3-Way F Metri-Pack 280 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Accessory Power Outlet - Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 RD/WH | 140 | Battery Positive Voltage
B | -- | -- | Not Used
C | 1 BK | 650 | Ground

### Accessory Power Outlet - Rear Console (DK1)

#### Connector Part Information

- OEM: 12176836
- Service: 15305923
- Description: 3-Way F Metri-Pack 280 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Accessory Power Outlet - Rear Console (DK1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 RD/WH | 140 | Battery Positive Voltage
B | -- | -- | Not Used
C | 1 BK | 750 | Ground

### Adaptive Forward Lighting (AFL) Motor - Left (TSH)

#### Connector Part Information

- OEM: XAP-10V
- Service: See Catalog
- Description: 10-Way F XA Series (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Adaptive Forward Lighting (AFL) Motor - Left (TSH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | -- | Left Headlamp High Beam Voltage
2 | 0.35 BK | -- | Ground
3 | 0.35 RD | -- | Battery Positive Voltage
4 | 0.35 BK | -- | Ground
5 | 0.35 OG | -- | Linear Interconnect Network (LIN)
6-10 | -- | -- | Not Used

### Adaptive Forward Lighting (AFL) Motor - Right (TSH)

#### Connector Part Information

- OEM: XAP-10V
- Service: See Catalog
- Description: 10-Way F XA Series (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Adaptive Forward Lighting (AFL) Motor - Right (TSH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | -- | Right Headlamp High Beam Voltage
2 | 0.35 BK | -- | Ground
3 | 0.35 RD | -- | Battery Positive Voltage
4 | 0.35 BK | -- | Ground
5 | 0.35 OG | -- | Linear Interconnect Network (LIN)
6-10 | -- | -- | Not Used

### Air Temperature Actuator - Auxiliary

#### Connector Part Information

- OEM: 12064993
- Service: 12102485
- Description: 6-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Air Temperature Actuator - Auxiliary

Pin | Wire | Circuit | Function
--- | --- | --- | ---
5 | 0.35 GY | 2614 | Auxiliary Air Temperature Door Control
6 | 0.35 BN | 6555 | Auxiliary Temperature Motor Voltage
7 | -- | -- | Not Used
8 | 0.35 GY/BK | 1798 | Low Reference
9 | 0.35 PK | 2145 | Auxiliary Air Temperature Door Position Signal
10 | 0.35 GY | 596 | 5-Volt Reference

### Air Temperature Actuator - Left (CJ2)

#### Connector Part Information

- OEM: 12064993
- Service: 12102485
- Description: 6-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Air Temperature Actuator - Left (CJ2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
5 | 0.35 D-BU | 1199 | Air Temperature Door Control
6 | 0.35 L-GN | 2210 | Air Temperature Door Control
7 | -- | -- | Not Used
8 | 0.35 YE | 1791 | Low Reference
9 | 0.35 L-BU | 733 | Air Temperature Door Position Signal
10 | 0.35 GY | 598 | 5-Volt Reference

### Air Temperature Actuator - Right (CJ2)

#### Connector Part Information

- OEM: 12064993
- Service: 12102485
- Description: 6-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Air Temperature Actuator - Right (CJ2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
5 | 0.35 WH/BK | 1236 | Auxiliary Air Temperature Door Control
6 | 0.35 GY/BK | 2778 | Right Air Temperature Door Control A
7 | -- | -- | Not Used
8 | 0.35 YE | 1791 | Low Reference
9 | 0.35 D-BU | 1646 | Auxiliary Air Temperature Door Position Signal
10 | 0.35 GY | 598 | 5-Volt Reference

### Air Temperature Actuator (C67)

#### Connector Part Information

- OEM: 12064993
- Service: 12102485
- Description: 6-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Air Temperature Actuator (C67)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
5 | 0.35 WH/BK | 1236 | Auxiliary Air Temperature Door Control
6 | 0.35 GY/BK | 2778 | Right Air Temperature Door Control A
7 | -- | -- | Not Used
8 | 0.35 YE | 1791 | Low Reference
9 | 0.35 D-BU | 1646 | Auxiliary Air Temperature Door Position Signal
10 | 0.35 GY | 598 | 5-Volt Reference

### Air Temperature Sensor - Lower Left (CJ2)

#### Connector Part Information

- OEM: 1-968704-1
- Service: See Catalog
- Description: 2-Way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: 928999-5/15
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Air Temperature Sensor - Lower Left (CJ2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 518 | Lower Left Air Temperature Sensor Signal
2 | 0.35 TN | 552 | Low Reference

### Air Temperature Sensor - Lower Right (CJ2)

#### Connector Part Information

- OEM: 1-968704-1
- Service: See Catalog
- Description: 2-Way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: 928999-5/15
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Air Temperature Sensor - Lower Right (CJ2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 520 | Lower Right Air Temperature Sensor Signal
2 | 0.35 TN | 552 | Low Reference

### Air Temperature Sensor - Upper Left (CJ2)

#### Connector Part Information

- OEM: 1-968704-1
- Service: See Catalog
- Description: 2-Way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: 928999-5/15
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Air Temperature Sensor - Upper Left (CJ2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 516 | Upper Left Air Temperature Sensor Signal
2 | 0.35 YE | 61 | Low Reference

### Air Temperature Sensor - Upper Right (CJ2)

#### Connector Part Information

- OEM: 1-968704-1
- Service: See Catalog
- Description: 2-Way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: 928999-5/15
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Air Temperature Sensor - Upper Right (CJ2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 517 | Upper Right Air Temperature Sensor Signal
2 | 0.35 YE | 61 | Low Reference

### Ambient Light Sensor (C67)

#### Connector Part Information

- OEM: 12047662
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Ambient Light Sensor (C67)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN/BK | 1137 | DRL Ambient Light Sensor Signal
B | 0.35 BK/WH | 1551 | Ground

### Ambient Temperature Sensor

#### Connector Part Information

- OEM: 13543521
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Ambient Temperature Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
B | 0.35 YE | 61 | Low Reference

### Audio Amplifier X1 (UQA or UQS)

#### Connector Part Information

- OEM: 89047379
- Service: 19115652
- Description: 8-Way F Unsealed (L-GY)

#### Terminal Part Information

- Pins: 1, 3, 5, 7
- Terminal/Tray: 8100-4444/22
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

- Pins: 4, 8
- Terminal/Tray: 8100-4445/22
- Core/Insulation Crimp: Pins 4 - 4/4
- Core/Insulation Crimp: Pins 8 - F/D
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

#### Audio Amplifier X1 (UQA or UQS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 GY | 118 | Left Front Speaker Output (-)
3 | 1 L-GN/BK | 1794 | Subwoofer Speaker Output (-)
4 | 2 RD/WH | 2040 | Battery Positive Voltage
5 | 1 TN | 201 | Left Front Speaker Output (+)
6 | -- | -- | Not Used
7 | 1 D-BU/WH | 346 | Subwoofer Speaker Output (+)
8 | 3 BK/WH | 351 | Ground

### Audio Amplifier X2 (UQA or UQS)

#### Connector Part Information

- OEM: 15134091
- Service: See Catalog
- Description: 16-Way F 1.5 Series (BK)

#### Terminal Part Information

- Pins: 1, 2, 7, 8, 15, 16
- Terminal/Tray: 8240-0128/22
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 3-6
- Terminal/Tray: 8240-0127/22
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Audio Amplifier X2 (UQA or UQS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 L-BU | 115 | Right Rear Speaker Output (-)
2 | 0.8 D-BU | 46 | Right Rear Speaker Output (+)
3 | 0.35 L-BU | 1960 | Front Center Speaker Output (-)
4 | 0.35 YE | 1860 | Front Center Speaker Output (+)
5 | 0.5 WH | 1959 | Left Rear Midrange Speaker Output (-)
6 | 0.5 TN | 1859 | Left Rear Midrange Speaker Output (+)
7 | 1 D-GN | 117 | Right Front Speaker Output (-)
8 | 1 L-GN | 200 | Right Front Speaker Output (+)
9-14 | -- | -- | Not Used
15 | 0.8 BN | 199 | Left Rear Speaker Output (+)
16 | 0.8 YE | 116 | Left Rear Speaker Output (-)

### Audio Amplifier X3 (UQA or UQS)

#### Connector Part Information

- OEM: 15136073
- Service: See Catalog
- Description: 16-Way F Kaizen 0.64 (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Audio Amplifier X3 (UQA or UQS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 WH | 6763 | Subwoofer Low Level Audio Signal (UQS)
2 | 0.5 OG | 6761 | Center Channel Low Level Audio Signal (-) (UQS)
3 | 0.5 D-BU | 6760 | Center Channel Low Level Audio Signal (UQS)
4 | 0.5 TN | 1946 | Right Rear Low Level Audio Signal (-) (without UK6)
0.5 TN/WH | 5830 | Right Rear Low Level Audio Signal (-) (UK6)
5 | 0.5 BN | 5314 | Left Rear Low Level Audio Signal (-) (UK6)
0.5 BN | 1999 | Left Rear Low Level Audio Signal (-) (without UK6)
6 | 0.5 L-GN | 1948 | Right Front Low Level Audio Signal (-)
7 | 0.5 D-GN | 1947 | Left Front Low Level Audio Signal (-)
8 | 0.35 WH | 7066 | Entertainment Remote Enable Signal
9 | 0.5 PK | 6762 | Subwoofer Low Level Audio (-) (UQS)
10 | -- | -- | Not Used
11 | 0.35 OG | 5748 | Radio Audio Mute Signal
12 | 0.5 D-BU | 546 | Right Rear Low Level Audio Signal (+) (without UK6)
0.5 L-GN | 5313 | Right Rear Low Level Audio Signal (+) (UK6)
13 | 0.5 BN/WH | 599 | Left Rear Low Level Audio Signal (+) (without UK6)
0.5 L-BU | 5312 | Left Rear Low Level Audio Signal (+) (UK6)
14 | 0.5 L-GN/WH | 512 | Right Front Low Level Audio Signal (+)
15 | 0.5 TN | 511 | Left Front Low Level Audio Signal (+)
16 | -- | -- | Not Used

### Audio/Video Adapter (U42)

#### Connector Part Information

- OEM: 15480082
- Service: 19149303
- Description: 8-Way F Micro 64 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Audio/Video Adapter (U42)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BARE | 5346 | Video Drain Wire
2 | -- | -- | Not Used
3 | 0.35 PU | 2056 | Auxiliary Video High Signal
4 | -- | -- | Not Used
5 | 0.35 WH | 2058 | Auxiliary Audio Right Signal
6 | 0.35 YE | 2059 | Auxiliary Audio Left Signal
7 | 0.35 BARE | 5345 | Auxiliary Audio Drain Wire
8 | -- | -- | Not Used

### Automatic Transmission

#### Connector Part Information

- OEM: 15476346
- Service: 19151494
- Description: 20-Way F GT 150 Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Pins: 1, 2, 5, 12-16
- Core/Insulation Crimp: E/4
- Pins: 18, 19
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Automatic Transmission

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BK/WH | 451 | Ground
2 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
3-4 | -- | -- | Not Used
5 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
6-9 | -- | -- | Not Used
10 | 0.8 RD/WH | 3640 | Battery Positive Voltage
11 | -- | -- | Not Used
12 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
13 | 0.5 PK | 1339 | Ignition Voltage
14 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
15 | 0.5 D-BU | 5985 | Ignition Voltage
16-17 | -- | -- | Not Used
18 | 0.8 BK/WH | 451 | Ground
19 | -- | -- | Not Used
20 | 0.5 OG/BK | 1786 | Park/Neutral Signal

### Automatic Transmission Internal Mode Switch (IMS)

#### Connector Part Information

- OEM: 15336500
- Service: Non-Serviceable
- Description: 6-Way F Metri-Pack 150.2 Series (GN)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Automatic Transmission Internal Mode Switch (IMS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 GY | -- | Low Reference
B | 0.5 BK | -- | Transmission Range Switch Signal P
C | 0.5 YE | -- | Transmission Range Switch Signal C
D | 0.5 RD | -- | Transmission Range Switch Signal B
E | 0.5 GN | -- | Transmission Range Switch Signal A
F | 0.5 WH | -- | Park/Neutral Switch Signal

### Automatic Transmission Manual Shift Switch

#### Connector Part Information

- OEM: 12064761
- Service: 12064761
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Automatic Transmission Manual Shift Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | GN | -- | Ignition Voltage
B | GN | -- | Tap Up/Tap Down Switch Signal
C-D | -- | -- | Not Used

### Back Up Lamp - Left (W49)

#### Connector Part Information

- OEM: 7712-5354-4WB
- Service: See Catalog
- Description: 2-Way F Lamp Socket, Axial (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Back Up Lamp - Left (W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | -- | Backup Lamp Voltage
B | 0.5 BK | -- | Ground

### Back Up Lamp - Left (WDA)

#### Connector Part Information

- OEM: 1-1438608-1
- Service: 19149296
- Description: 2-Way F MQS Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 962885-5/15
- Core/Insulation Crimp: 6/6
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Back Up Lamp - Left (WDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 24 | Backup Lamp Voltage
2 | 0.5 BK | 650 | Ground

### Back Up Lamp - Left (Z88)

#### Connector Part Information

- OEM: 1-1438608-2
- Service: See Catalog
- Description: 2-Way F MQS Series, Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Back Up Lamp - Left (Z88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | -- | Ground
2 | 0.5 BK | -- | Backup Lamp Voltage

### Back Up Lamp - Right (W49)

#### Connector Part Information

- OEM: 7712-5354-4WB
- Service: See Catalog
- Description: 2-Way F Lamp Socket, Axial (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Back Up Lamp - Right (W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | -- | Backup Lamp Voltage
B | 0.5 BK | -- | Ground

### Back Up Lamp - Right (WDA)

#### Connector Part Information

- OEM: 1-1438608-1
- Service: 19149296
- Description: 2-Way F MQS Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 962885-5/15
- Core/Insulation Crimp: 6/6
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Back Up Lamp - Right (WDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 24 | Backup Lamp Voltage
2 | 0.5 BK | 650 | Ground

### Back Up Lamp - Right (Z88)

#### Connector Part Information

- OEM: 1-1438608-2
- Service: See Catalog
- Description: 2-Way F MQS Series, Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Back Up Lamp - Right (Z88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | -- | Ground
2 | 0.5 BK | -- | Backup Lamp Voltage

### Battery (-)

#### Terminal Part Information

- Terminal: R61014-002
- Core/Insulation Crimp: N/A
- Description: Battery Terminal

#### Battery (-)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
- | 32 BK | 50 | Ground
10 BK | 50 | Ground

### Battery (+)

#### Terminal Part Information

- Terminal: R3311-033
- Core/Insulation Crimp: N/A
- Description: Battery Terminal

#### Battery (+)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
+ | 40 RD | 1 | Battery Positive Voltage
1 RD | 1 | Battery Positive Voltage (UE1)

### Battery Current Sensor

#### Connector Part Information

- OEM: 19177527
- Service: See Catalog
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Battery Current Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK | 5076 | Current Sensor Voltage
B | 0.35 BN | 5077 | Low Reference
C | 0.35 WH | 5075 | Current Sensor Signal

### Blower Motor

#### Connector Part Information

- OEM: 12084957
- Service: 12126461
- Description: 2-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Blower Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 PU | 65 | Blower Motor Voltage
B | 3.0 BK | 5987 | Low Reference

### Blower Motor - Auxiliary

#### Connector Part Information

- OEM: 12064749
- Service: 12064749
- Description: 2-Way F Metri-Pack 480 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Blower Motor - Auxiliary

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3.0 RD/WH | 65 | Blower Motor Voltage
B | 3.0 OG | 5988 | Low Reference

### Blower Motor Control Module - Auxiliary X1

#### Connector Part Information

- OEM: 15226103
- Service: 88988507
- Description: 2-Way F Receptacle 6.3 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Blower Motor Control Module - Auxiliary X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 RD/WH | 65 | Blower Motor Voltage
2 | 3.0 OG | 5988 | Low Reference

### Blower Motor Control Module - Auxiliary X2

#### Connector Part Information

- OEM: 15226104
- Service: 88988512
- Description: 6-Way F YESC Kaizen Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7114-4122-02/9
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

#### Blower Motor Control Module - Auxiliary X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.35 D-GN | 2211 | Auxiliary Blower Motor Speed Control
4 | -- | -- | Not Used
5 | 3.0 BK | 850 | Ground
6 | 3.0 RD/WH | 2640 | Battery Positive Voltage

### Blower Motor Control Module X1

#### Connector Part Information

- OEM: 15226103
- Service: 88988507
- Description: 2-Way F Receptacle 6.3 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Blower Motor Control Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3.0 PU | 65 | Blower Motor Voltage
2 | 3.0 BK | 5987 | Low Reference

### Blower Motor Control Module X2

#### Connector Part Information

- OEM: 15226104
- Service: 88988512
- Description: 6-Way F YESC Kaizen Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7114-4122-02/9
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-43 (RD)

#### Blower Motor Control Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.35 GY/BK | 754 | Blower Motor Speed Control
4 | -- | -- | Not Used
5 | 3.0 BK | 450 | Ground
6 | 3.0 RD/BK | 442 | Battery Positive Voltage

### Body Control Module (BCM) X1

#### Connector Part Information

- OEM: 15482789
- Service: 88988838
- Description: 27-Way F HIT Series (L-GN)

#### Terminal Part Information

- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 WH | 1390 | Ignition II/III/Key in Ignition
3 | 0.35 GY | 1884 | Cruise Control Switch Signal
4 | 0.35 WH/BK | 1073 | Ignition Key Resistor Signal
5 | 0.35 L-GN | 1715 | Windshield Wiper Switch High Signal
6 | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
7 | -- | -- | Not Used
8 | 0.35 TN/BK | 6009 | Low Reference
9 | 0.35 L-BU | 1714 | Windshield Wiper Switch Low Signal
10-12 | -- | -- | Not Used
13 | 0.35 L-GN | 1011 | Remote Radio Control Signal (RCA)
14 | 0.35 PK | 3 | Ignition Voltage
15 | 0.35 L-BU/WH | 1414 | Left Turn Signal Switch Signal
16 | 0.35 D-BU/WH | 1415 | Right Turn Signal Switch Signal
17 | 0.35 PU | 1375 | 12-Volt Reference
18 | 0.35 PU | 524 | Headlamp Dimmer Switch High Beam Signal
19 | 0.35 TN | 2144 | Hazard Switch Signal
20 | 0.35 PU | 5526 | Tap Up/Tap Down Switch Signal
21 | 0.35 BN | 4 | Ignition Voltage
22 | -- | -- | Not Used
23 | 0.35 L-BU | 553 | Tow/Haul Switch Signal
24 | 0.35 PK | 94 | Windshield Washer Switch Signal
25 | 0.35 BN | 1356 | Flash To Pass Switch Signal
26-27 | -- | -- | Not Used

### Body Control Module (BCM) X2

#### Connector Part Information

- OEM: 15482790
- Service: 88988839
- Description: 25-Way F HIT Series (WH)

#### Terminal Part Information

- Pins: 1, 2, 3, 5
- Terminal/Tray: SNAC-A061T-M2.8/20
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-4A (PU)

- Pins: 8, 11, 12, 17, 18, 20, 21, 22, 25
- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 OG | 1732 | Courtesy Lamps Voltage
2 | 0.8 RD/WH | 1240 | Battery Positive Voltage
3 | 0.8 GY | 8 | Instrument Panel Lamp Voltage
4 | -- | -- | Not Used
5 | 0.8 GY/BK | 690 | Courtesy Lamp High Control
6-7 | -- | -- | Not Used
8 | 0.35 BN/WH | 301 | Rear Park Lamps Voltage
9-10 | -- | -- | Not Used
11 | 0.35 L-GN/BK | 1137 | DRL Ambient Light Sensor Signal
12 | 0.35 WH | 103 | Headlamp Switch Headlamps On Signal
13-16 | -- | -- | Not Used
17 | 0.35 D-GN | 306 | Headlamp Switch Headlamps Off Signal
18 | 0.35 PK/BK | 1597 | Courtesy Lamps Switch On Signal
19 | -- | -- | Not Used
20 | 0.5 PU | 5357 | Right Tail Lamp Outage Detection Signal (Z88)
21 | 0.35 BN/WH | 1571 | Traction Control Switch Signal
22 | 0.35 D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Voltage
23-24 | -- | -- | Not Used
25 | 0.35 PU | 328 | Interior Lamp Switch Signal

### Body Control Module (BCM) X3

#### Connector Part Information

- OEM: 15482791
- Service: 88988840
- Description: 25-Way F HIT Series (L-BU)

#### Terminal Part Information

- Pins: 1-3, 5
- Terminal/Tray: SNAC-A061T-M2.8/20
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-4A (PU)

- Pins: 8-19, 21, 22
- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BK/WH | 1551 | Ground
2 | 0.8 RD/WH | 1640 | Battery Positive Voltage
3 | 0.8 RD/WH | 4540 | Battery Positive Voltage
4 | -- | -- | Not Used
5 | 0.8 BK/WH | 1551 | Ground
6-7 | -- | -- | Not Used
8 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
9 | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus-
10 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
11 | 0.35 D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal
12 | 0.35 OG/WH | 812 | 12-Volt Reference
13 | 0.35 L-GN | 526 | Stop Lamp Switch Signal
14 | 0.35 TN | 552 | Low Reference
15 | 0.35 GY | 598 | 5-Volt Reference
16 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
17 | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus-
18 | 0.35 PU/WH | 1382 | LED Dimming Signal
19 | 0.35 L-BU | 5986 | Communication Enable
20 | -- | -- | Not Used
21 | 0.35 OG | 192 | Fog Lamps Enable (T96)
22 | 0.35 GN/WH | 7158 | Cruise Control Indicator Dimming Signal
23-25 | -- | -- | Not Used

### Body Control Module (BCM) X4

#### Connector Part Information

- OEM: 15482792
- Service: 88988841
- Description: 25-Way F HIT Series (BK)

#### Terminal Part Information

- Pins: 7, 9-13, 15-17, 19, 21-23
- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

- Pins: 1-5
- Terminal/Tray: SNAC-A061T-M2.8/20
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-4A (PU)

#### Body Control Module (BCM) X4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 RD/WH | 340 | Battery Positive Voltage (Z88 or W49)
1 RD/WH | 340 | Battery Positive Voltage (WDA)
2 | 1 RD/WH | 240 | Battery Positive Voltage
3 | 1 RD/WH | 440 | Battery Positive Voltage
4 | 0.8 RD/WH | 2140 | Battery Positive Voltage
5 | 1 D-BU/WH | 1315 | Right Turn Signal Indicator Lamp Voltage
6 | -- | -- | Not Used
7 | 0.35 YE | 196 | Windshield Wiper Motor Park Switch Signal
8 | -- | -- | Not Used
9 | 0.35 BK | 50 | Ground
10 | 0.35 RD/WH | 2440 | Battery Positive Voltage
11 | 0.35 D-GN/WH | 1317 | Fog Lamp Relay Control (T96)
12 | 0.5 YE | 5187 | Right Trailer Turn Signal Lamp (V92)
13 | 0.5 OG | 5186 | Left Trailer Turn Signal Lamp (V92)
14 | -- | -- | Not Used
15 | 0.35 OG | 2268 | Windshield Washer Relay Control
16 | 0.35 TN/WH | 1969 | Headlamp Relay Control (W49 or WDA or Z88 with TVD)
17 | 0.35 PK/BK | 109 | Hood Ajar Switch Signal (BTV)
18 | -- | -- | Not Used
19 | 0.35 D-BU | 5985 | Ignition Voltage
20 | -- | -- | Not Used
21 | 0.35 PK | 1439 | Ignition Voltage
22 | 0.35 YE | 5704 | Liftgate Latch Relay Coil Control (TB4)
23 | 0.35 PU | 544 | Headlamp Low Beam Voltage (W49 or WDA or Z88 with TVD)
24-25 | -- | -- | Not Used

### Body Control Module (BCM) X5

#### Connector Part Information

- OEM: 15480179
- Service: 88988837
- Description: 25-Way F HIT Series (BN)

#### Terminal Part Information

- Pins: 6, 8-11, 13-18, 20, 21, 23, 24
- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

- Pins: 1-5
- Terminal/Tray: SNAC-A061T-M2.8/20
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-4A (PU)

#### Body Control Module (BCM) X5

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 YE | 18 | Left Rear Stop/Turn Lamp Voltage
2 | 0.8 D-GN | 19 | Right Rear Stop/Turn Lamp Voltage
3 | -- | -- | Not Used
4 | 0.8 L-BU/WH | 1314 | Left Turn Signal Indicator Lamp Voltage
5 | 0.8 L-BU | 1320 | Stop Lamp Voltage
6 | 0.5 WH | 17 | Stop Lamp Voltage
7 | -- | -- | Not Used
8 | 0.35 PK | 5076 | Current Sensor Voltage
9 | 0.35 WH | 5075 | Current Sensor Signal
10 | 0.35 BN | 5077 | Low Reference
11 | 0.35 D-GN | 5706 | Liftgate Relay High Control (TB4)
12 | -- | -- | Not Used
13 | 0.35 OG | 300 | Power Mode
14 | 0.35 WH | 2283 | Rear Wiper/Washer Switch Voltage
15 | 0.35 PU | 5531 | Hood Closed Switch Signal (BTV)
16 | 0.5 OG/BK | 233 | Park Brake Switch Signal
17 | 0.5 YE/BK | 5356 | Left Tail Lamp Outage Detection Signal (Z88)
18 | 0.35 TN | 28 | Horn Relay Control
19 | -- | -- | Not Used
20 | 0.35 GY | 91 | Windshield Wiper Switch Signal 2
21 | 0.35 TN | 860 | Front Windshield Wiper Switch High Signal
22 | -- | -- | Not Used
23 | 0.35 PK/WH | 1970 | Headlamp Low Beam Relay Control (W49 or WDA or Z88 with TVD)
24 | 0.35 WH | 1080 | Park Lamp Relay Control
25 | -- | -- | Not Used

### Body Control Module (BCM) X6

#### Connector Part Information

- OEM: 15482793
- Service: 88988842
- Description: 25-Way F Receptacle 0.64 2.8 (PK)

#### Terminal Part Information

- Pins: 1-3
- Terminal/Tray: SNAC-A061T-M2.8/20
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-4A (PU)

- Pins: 8-10, 12, 14-16, 18, 20-23
- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X6

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.8 L-GN | 24 | Backup Lamp Voltage
3 | 0.8 GY | 8 | Instrument Panel Lamp Voltage
4-7 | -- | -- | Not Used
8 | 0.35 TN/WH | 746 | Right Front Door Ajar Switch Signal (without AXC or AXE)
9 | 0.35 D-BU | 245 | Passenger Door Lock Switch Unlock (without AXC or AXE)
10 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal (without AXC or AXE)
11 | -- | -- | Not Used
12 | 0.35 PK/BK | 1303 | Liftgate Ajar Switch Signal (TB4)
13 | -- | -- | Not Used
14 | 0.35 L-GN/BK | 748 | Right Rear Door Ajar Switch Signal
15 | 0.35 L-BU/BK | 747 | Left Rear Door Ajar Switch Signal
16-17 | -- | -- | Not Used
18 | 0.35 L-BU | 244 | Passenger Door Lock Switch Lock (without AXC or AXE)
19-20 | -- | -- | Not Used
21 | 0.35 PU/WH | 1382 | LED Dimming Signal
22 | 0.35 L-GN | 5926 | Rear Access Open Switch Signal (TB4)
23 | 0.35 GY | 5797 | Rear Closure Handle Switch Open Signal (TB4)
24-25 | -- | -- | Not Used

### Body Control Module (BCM) X7

#### Connector Part Information

- OEM: 15466053
- Service: 88988806
- Description: 28-Way F HIT Series (GY)

#### Terminal Part Information

- Terminal/Tray: SNAC3-A021T-M0.64/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Body Control Module (BCM) X7

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 YE | 43 | Ignition Voltage
3-5 | -- | -- | Not Used
6 | 0.35 YE | 356 | Driver Door Lock Relay Unlock Control (without AXC or AXE)
7 | 0.35 L-GN | 1391 | Driver Door Unlock Relay Control
8 | 0.35 D-BU | 545 | DRL Voltage (TVD with Z88)
9 | 0.35 L-BU | 5921 | Driver Door Unlock Relay Control
10 | -- | -- | Not Used
11 | 0.35 OG/BK | 781 | Driver Door Lock Switch Unlock Signal (without AXC or AXE)
12 | 0.35 PK/BK | 780 | Driver Door Lock Switch Lock Signal (without AXC or AXE)
13 | 0.35 D-BU | 38 | Backup Lamp Relay Control (V92)
14-17 | -- | -- | Not Used
18 | 0.35 L-GN | 170 | Power Window Master Switch Right Rear Up Signal (AXC or AXE)
19 | 0.35 PU | 169 | Power Window Master Switch Left Rear Down Signal (AXC or AXE)
20 | -- | -- | Not Used
21 | 0.35 D-BU | 1307 | Power Window Master Switch Lockout Signal (AXC or AXE)
22-24 | -- | -- | Not Used
25 | 0.35 PU/WH | 6816 | Heated Seat Indicator Dimming (KA1 without A45)
26 | 0.35 PU | 171 | Power Window Master Switch Right Rear Down Signal (AXC or AXE)
27 | 0.35 L-BU/WH | 280 | Power Window Master Switch Lockout Right Rear Signal (AXC or AXE)
28 | 0.35 D-GN | 168 | Power Window Master Switch Left Rear Up Signal (AXC or AXE)

### Brake Booster Pump - Auxiliary

#### Connector Part Information

- OEM: 7282-5575-10
- Service: See Catalog
- Description: 2-Way M 2.8 Series Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4151-02/9
- Core/Insulation Crimp: C/1
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### Brake Booster Pump - Auxiliary

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 OG | 1470 | Brake Booster Pump Motor Voltage
2 | 1 BK | 451 | Ground

### Brake Booster Vacuum Sensor

#### Connector Part Information

- OEM: 7283569110
- Service: See Catalog
- Description: 3-Way F 1.5 Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Brake Booster Vacuum Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG | 6030 | Brake Vacuum Sensor Signal
2 | 0.5 YE/BK | 6032 | Low Reference
3 | 0.5 GY | 6031 | 5-Volt Reference

### Brake Fluid Level Switch

#### Connector Part Information

- OEM: 12162193
- Service: 88987993
- Description: 2-Way F Metri-Pack 150.2 Series, Sealed, Pull To Seat (BK)

#### Terminal Part Information

- Terminal/Tray: 12124075/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12180559-1/J-35616-14 (GN)

#### Brake Fluid Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK/WH | 1551 | Ground
B | 0.35 TN/WH | 33 | Brake Warning Indicator Control

### Brake Pedal Position Sensor

#### Connector Part Information

- OEM: 88953336
- Service: 88953364
- Description: 3-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Brake Pedal Position Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 598 | 5-Volt Reference
B | 0.35 L-GN | 526 | Stop Lamp Switch Signal
C | 0.35 TN | 552 | Low Reference

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Exhaust (LLT)

#### Connector Part Information

- OEM: 7283752630
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Exhaust (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply
2 | 0.5 L-GN | 5282 | Camshaft Phaser Exhaust Solenoid

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Exhaust (LLT)

#### Connector Part Information

- OEM: 7283752630
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Exhaust (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply
2 | 0.5 WH/BK | 5283 | Camshaft Phaser Exhaust Solenoid

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Intake (LLT)

#### Connector Part Information

- OEM: 7283752630
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 1 Intake (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply
2 | 0.5 PU | 5284 | Camshaft Phaser Intake Solenoid

### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Intake (LLT)

#### Connector Part Information

- OEM: 7283752630
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4026/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15313892/J-35616-18 (BK)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Bank 2 Intake (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply
2 | 0.5 OG/BK | 5272 | Camshaft Phaser Intake Solenoid

### Camshaft Position (CMP) Sensor - Bank 1 Exhaust (LLT)

#### Connector Part Information

- OEM: 1-928-403-968
- Service: See Catalog
- Description: 3-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Camshaft Position (CMP) Sensor - Bank 1 Exhaust (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 552 | Low Reference
2 | 0.5 D-GN | 5273 | Camshaft Position Exhaust Sensor
3 | 0.5 GY | 705 | 5-Volt Reference 2

### Camshaft Position (CMP) Sensor - Bank 2 Exhaust (LLT)

#### Connector Part Information

- OEM: 1-928-403-968
- Service: See Catalog
- Description: 3-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Camshaft Position (CMP) Sensor - Bank 2 Exhaust (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 552 | Low Reference
2 | 0.5 PU | 5274 | Camshaft Position Exhaust Sensor
3 | 0.5 GY | 705 | 5-Volt Reference 2

### Camshaft Position (CMP) Sensor - Bank 1 Intake (LLT)

#### Connector Part Information

- OEM: 1-928-403-968
- Service: See Catalog
- Description: 3-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Camshaft Position (CMP) Sensor - Bank 1 Intake (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 552 | Low Reference
2 | 0.5 OG | 5275 | Camshaft Position Intake Sensor
3 | 0.5 GY | 705 | 5-Volt Reference 2

### Camshaft Position (CMP) Sensor - Bank 2 Intake (LLT)

#### Connector Part Information

- OEM: 1-928-403-968
- Service: See Catalog
- Description: 3-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Camshaft Position (CMP) Sensor - Bank 2 Intake (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 552 | Low Reference
2 | 0.5 YE | 5276 | Camshaft Position Intake Sensor
3 | 0.5 GY | 705 | 5-Volt Reference 2

### Cellular Telephone Microphone (UE1)

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Cellular Telephone Microphone (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BARE | 514 | Ground
B | 0.35 GY | 655 | Cellular Microphone Signal

### Center High Mounted Stop Lamp (CHMSL) (W49)

#### Connector Part Information

- OEM: 13575577
- Service: See Catalog
- Description: 2-Way F 090 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-1420/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Center High Mounted Stop Lamp (CHMSL) (W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 650 | Ground
2 | 0.5 L-BU | 1320 | Stop Lamp Voltage

### Center High Mounted Stop Lamp (CHMSL) (without W49)

#### Connector Part Information

- OEM: 7223-1324
- Service: 88988460
- Description: 2-Way F 090 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-1420/11
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 15315247/J-35616-18 (BK)

#### Center High Mounted Stop Lamp (CHMSL) (without W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 650 | Ground
2 | 0.5 L-BU | 1320 | Stop Lamp Voltage

### Clock (W49)

#### Connector Part Information

- OEM: 15368694
- Service: 88953272
- Description: 3-Way F Multilock 070 Series (WH)

#### Terminal Part Information

- Terminal/Tray: 173630-7/7
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-33 (YE)

#### Clock (W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1840 | Battery Positive Voltage
2 | 0.35 BK | 1450 | Ground
3 | 0.35 PU/WH | 1382 | LED Dimming Signal

### Console Flood Lamp

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Console Flood Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 850 | Ground
B | 0.35 PU/WH | 1382 | LED Dimming Signal

### Courtesy/Reading Lamps - 2nd Row (without U42)

#### Connector Part Information

- OEM: 12047781
- Service: 12101864
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Courtesy/Reading Lamps - 2nd Row (without U42)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG | 1732 | Courtesy Lamps Voltage
B | 0.5 BK | 850 | Ground
C | 0.5 GY/BK | 690 | Courtesy Lamp High Control

### Courtesy/Reading Lamps - 2nd Row X1 (C3U with U42)

#### Connector Part Information

- OEM: 12047781
- Service: 12101864
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Courtesy/Reading Lamps - 2nd Row X1 (C3U with U42)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG | 1732 | Courtesy Lamps Voltage
B | 0.5 BK | 850 | Ground
C | 0.5 GY/BK | 690 | Courtesy Lamp High Control

### Courtesy/Reading Lamps - 2nd Row X2 (C3U with U42)

#### Connector Part Information

- OEM: 12047781
- Service: 12101864
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Courtesy/Reading Lamps - 2nd Row X2 (C3U with U42)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG | 1732 | Courtesy Lamps Voltage
B | 0.5 BK | 850 | Ground
C | 0.5 GY/BK | 690 | Courtesy Lamp High Control

### Crankshaft Position (CKP) Sensor (LLT)

#### Connector Part Information

- OEM: 31403-3710
- Service: 88988337
- Description: 3-Way F 064 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 33468-0003/23
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Crankshaft Position (CKP) Sensor (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 452 | Low Reference
2 | 0.5 YE | 573 | CKP Sensor Signal
3 | 0.5 GY | 605 | 5-Volt Reference 3

### Data Link Connector (DLC)

#### Connector Part Information

- OEM: 19177614
- Service: See Catalog
- Description: 16-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12129484/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Data Link Connector (DLC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
2-3 | -- | -- | Not Used
4 | 0.5 BK | 750 | Ground
5 | 0.35 BK/WH | 1551 | Ground
6 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
7-13 | -- | -- | Not Used
14 | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus-
15 | -- | -- | Not Used
16 | 0.35 RD/WH | 1840 | Battery Positive Voltage

### Data Link Resistor (without MH6)

#### Connector Part Information

- OEM: 19177503
- Service: 15306156
- Description: 2-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 15326427/5
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Data Link Resistor (without MH6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
B | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus-

### Daytime Running Lamp (DRL) - Left (W49 or Z88 with T61)

#### Connector Part Information

- OEM: 7900-1486-004
- Service: See Catalog
- Description: 3-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Daytime Running Lamp (DRL) - Left (W49 or Z88 with T61)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 OG | -- | Left DRL/Turn Voltage (Z88)
0.8 L-BU/WH | -- | Left DRL/Turn Voltage (W49)
2 | -- | -- | Not Used
3 | 0.8 BK | -- | Ground

### Daytime Running Lamp (DRL) - Left (WDA with T61)

#### Connector Part Information

- OEM: 1-967644-1
- Service: See Catalog
- Description: 2-Way F TYCO Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Daytime Running Lamp (DRL) - Left (WDA with T61)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | -- | Ground
2 | 0.5 PU | -- | Left DRL/Turn Voltage

### Daytime Running Lamp (DRL) - Right (W49 or Z88 with T61)

#### Connector Part Information

- OEM: 7900-1486-004
- Service: See Catalog
- Description: 3-Way F Lamp Socket Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Daytime Running Lamp (DRL) - Right (W49 or Z88 with T61)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 OG | -- | Right DRL/Turn Voltage (Z88)
0.8 L-BU/WH | -- | Right DRL/Turn Voltage (W49)
2 | -- | -- | Not Used
3 | 0.8 BK | -- | Ground

### Daytime Running Lamp (DRL) - Right (WDA with T61)

#### Connector Part Information

- OEM: 1-967644-1
- Service: See Catalog
- Description: 2-Way F TYCO Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Daytime Running Lamp (DRL) - Right (WDA with T61)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | -- | Ground
2 | 0.5 PU | -- | Right DRL/Turn Voltage

### Digital Radio Receiver (U2K or UBS)

#### Connector Part Information

- OEM: 15394150
- Service: See Catalog
- Description: 16-Way F Micro-Pack 064 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Digital Radio Receiver (U2K or UBS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN/WH | 372 | Left Audio Signal (-)
2 | 0.5 BN/WH | 367 | Left Audio Signal (+)
3 | 0.5 D-GN/WH | 368 | Right Audio Signal (+)
4 | 0.5 GY | 388 | Right Audio Signal (-)
5 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
6-8 | -- | -- | Not Used
9 | 0.5 BK/WH | 351 | Ground
10-15 | -- | -- | Not Used
16 | 0.5 RD/WH | 2340 | Battery Positive Voltage

### Digital Video Disc (DVD) Display (U42)

#### Connector Part Information

- OEM: 15490628
- Service: See Catalog
- Description: 10-Way F Kaizen 0.64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Digital Video Disc (DVD) Display (U42)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 6975 | DVD Video Signal (+)
2 | 0.35 WH/BK | 5335 | DVD Video Signal (-)
3-5 | -- | -- | Not Used
6 | 0.5 BK/WH | 351 | Ground
7 | 0.5 RD/WH | 2340 | Battery Positive Voltage
8 | 0.35 WH | 7066 | Entertainment Remote Enable Signal
9 | 0.35 PK/BK | 5844 | Video Bright Control
10 | 0.35 L-GN/BK | 5845 | Video Mode Signal

### Door Control Module - Passenger X1 (AXC or AXE)

#### Connector Part Information

- OEM: 6098-4607
- Service: 88988497
- Description: 6-Way F 2.8mm PBT (BK)

#### Terminal Part Information

- Pins: 1-3, 5
- Terminal/Tray: 8100-4445/22
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

- Pins: 4
- Terminal/Tray: 8100-4444/22
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

#### Door Control Module - Passenger X1 (AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 BN | 667 | Power Window Motor Right Front Down Control (AXE)
2 | 2 RD/WH | 3340 | Battery Positive Voltage (AXE)
3 | 2 D-BU | 666 | Power Window Motor Right Front Up Control (AXE)
4 | 0.8 RD/WH | 840 | Battery Positive Voltage (AXC or AXE)
5 | 2 BK | 750 | Ground (AXC or AXE)
6 | -- | -- | Not Used

### Door Control Module - Passenger X2 (AXC or AXE)

#### Connector Part Information

- OEM: 7283-9078-80
- Service: See Catalog
- Description: 16-Way F Kaizen 0.64 Series (BN)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Door Control Module - Passenger X2 (AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.35 D-BU | 6133 | Linear Interconnect Network Bus (AXC)
4 | -- | -- | Not Used
5 | 0.5 YE | 5943 | Low Reference
6 | -- | -- | Not Used
7 | 0.5 GY | 295 | Door Lock Actuator Lock Control
8 | 0.5 TN | 294 | Door Lock Actuator Unlock Control
9 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
10-12 | -- | -- | Not Used
13 | 0.5 TN/WH | 746 | Right Front Door Ajar Switch Signal
14-16 | -- | -- | Not Used

### Door Control Module - Passenger X3 (AXC or AXE)

#### Connector Part Information

- OEM: 7283-9040-30
- Service: See Catalog
- Description: 10-Way F YESC Kaizen Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Door Control Module - Passenger X3 (AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 OG/BK | 6162 | Outside Right Mirror Right Front Up Control (A45 with DNP or DNT or DS3)
2 | 0.35 GY/BK | 6161 | Outside Right Mirror Horizontal Position Control (A45 with DNP or DNT or DS3)
3 | 0.5 D-GN | 628 | Low Reference (A45 with DNP or DNT or DS3)
4-5 | -- | -- | Not Used
6 | 0.35 WH | 7196 | Outside Right Mirror Drive Motor Common (A45 with DNP or DNT or DS3)
7 | 0.5 OG | 2267 | Mirror Heating Element Voltage (A45 with DNP or DNT or DS3)
8 | 0.35 PK/BK | 5862 | Low Reference (UFT)
9-10 | -- | -- | Not Used

### Door Control Module - Passenger X4 (AXC or AXE)

#### Connector Part Information

- OEM: 7283-9065-40
- Service: See Catalog
- Description: 14-Way F Kaizen 0.64 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Door Control Module - Passenger X4 (AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control (A45 with KA1 or KB6)
2 | 0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control (A45 with KA1 or KB6)
3 | 0.35 GY | 6182 | Low Reference (A45 with KB6)
4-5 | -- | -- | Not Used
6 | 0.35 D-BU | 6180 | Low Reference (A45 with KA1 or KB6)
7 | 0.35 GY | 6182 | Low Reference (A45 with KA1)
8 | -- | -- | Not Used
9 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control (A45 with KA1 or KB6)
10 | 0.35 BN | 6179 | 5-Volt Reference (A45 with KA1 or KB6)
11 | 0.35 PU | 6181 | 5-Volt Reference (A45 with KA1)
12 | 0.35 PU | 6181 | 5-Volt Reference (A45 with KB6)
13-14 | -- | -- | Not Used

### Door Control Module - Passenger X7 (AXC or AXE)

#### Connector Part Information

- OEM: 7283-9045
- Service: See Catalog
- Description: 10-Way F 064 Series Unsealed (WH)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Door Control Module - Passenger X7 (AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 6804 | Driver Mirror Motor Down Control (DNP or DNT)
2 | 0.35 L-BU | 6805 | Right Extend Motor Retract/Unfold Control (DNP or DNT)
3 | -- | -- | Not Used
4 | 0.35 BN | 787 | Passenger Mirror Vertical Position Sensor Signal (A45 with DNP or DNT or DS3)
5 | 0.35 L-BU/BK | 785 | Passenger Mirror Horizontal Position Sensor Signal (A45 with DNP or DNT or DS3)
6 | -- | -- | Not Used
7 | 0.35 YE | 674 | 5-Volt Reference (A45 with DNP or DNT or DS3)
8 | 0.35 PK | 5861 | Passenger Side Object Detection LED Signal (UFT)
9 | -- | -- | Not Used
10 | 0.35 L-GN | 675 | Low Reference (A45 with DNP or DS3)

### Door Latch - Driver

#### Connector Part Information

- OEM: 6-1355688-1
- Service: See Catalog
- Description: 10-Way F 1.2 Micro III Timer (BK)

#### Terminal Part Information

- Terminal/Tray: 4-969005-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-560/J-35616-33 (YE)

#### Door Latch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.8 TN | 694 | Driver Door Lock Actuator Unlock Control (without AXC or AXE)
0.5 TN | 694 | Driver Door Lock Actuator Unlock Control (AXC or AXE)
3 | 0.8 GY | 295 | Door Lock Actuator Lock Control (without AXC or AXE)
0.5 GY | 295 | Door Lock Actuator Lock Control (AXC or AXE)
4-5 | -- | -- | Not Used
6 | 0.5 GY/BK | 745 | Left Front Door Ajar Switch Signal
7 | -- | -- | Not Used
8 | 0.5 YE | 5942 | Low Reference (AXC or AXE)
0.35 BK | 550 | Ground (without AXC or AXE)
9-10 | -- | -- | Not Used

### Door Latch - Left Rear

#### Connector Part Information

- OEM: 6-1355683-1
- Service: 88986251
- Description: 6-Way F Sealed Series (BK)

#### Terminal Part Information

- Pins: 2-6
- Terminal/Tray: 4-969005-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-560/J-35616-33 (YE)

#### Door Latch - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.8 TN | 294 | Door Lock Actuator Unlock Control
3 | 0.8 GY | 295 | Door Lock Actuator Lock Control
4 | 0.5 L-BU/BK | 747 | Left Rear Door Ajar Switch Signal
5 | -- | -- | Not Used
6 | 0.5 BK | 550 | Ground

### Door Latch - Passenger

#### Connector Part Information

- OEM: 6-1355683-1
- Service: 88986251
- Description: 6-Way F Sealed Series (BK)

#### Terminal Part Information

- Terminal/Tray: 4-969005-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-560/J-35616-33 (YE)

#### Door Latch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN/WH | 746 | Right Front Door Ajar Switch Signal
2 | -- | -- | Not Used
3 | 0.5 YE | 5943 | Low Reference (AXC or AXE)
0.35 BK | 750 | Ground (without AXC or AXE)
4 | -- | -- | Not Used
5 | 0.5 TN | 294 | Door Lock Actuator Unlock Control (AXC or AXE)
0.8 TN | 294 | Door Lock Actuator Unlock Control (without AXC or AXE)
6 | 0.8 GY | 295 | Door Lock Actuator Lock Control (without AXC or AXE)
0.5 GY | 295 | Door Lock Actuator Lock Control (AXC or AXE)

### Door Latch - Right Rear

#### Connector Part Information

- OEM: 6-1355683-1
- Service: 88986251
- Description: 6-Way F Sealed Series (BK)

#### Terminal Part Information

- Pins: 1-3, 5, 6
- Terminal/Tray: 964274-2/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-560/J-35616-33 (YE)

#### Door Latch - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN/BK | 748 | Right Rear Door Ajar Switch Signal
2 | -- | -- | Not Used
3 | 0.5 BK | 750 | Ground
4 | -- | -- | Not Used
5 | 0.8 TN | 294 | Door Lock Actuator Unlock Control
6 | 0.8 GY | 295 | Door Lock Actuator Lock Control

### Door Lock Switch - Driver (without AXC or AXE)

#### Connector Part Information

- OEM: 12124997
- Service: 12167130
- Description: 5-Way F Metri-Pack 150 Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12103359/18
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Door Lock Switch - Driver (without AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 8 | Instrument Panel Lamp Voltage
B | 0.35 BK | 550 | Ground
C | -- | -- | Not Used
D | 0.5 OG/BK | 781 | Driver Door Lock Switch Unlock Signal (WDA)
0.5 PK/BK | 780 | Driver Door Lock Switch Lock Signal (Z88)
E | 0.5 PK/BK | 780 | Driver Door Lock Switch Lock Signal (WDA)
0.5 OG/BK | 781 | Driver Door Lock Switch Unlock Signal (Z88)

### Door Lock Switch - Passenger (without AXC or AXE)

#### Connector Part Information

- OEM: 12124997
- Service: 12167130
- Description: 5-Way F Metri-Pack 150 Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12103359/18
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Door Lock Switch - Passenger (without AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 8 | Instrument Panel Lamp Voltage
B | 0.35 BK | 750 | Ground
C | -- | -- | Not Used
D | 0.5 D-BU | 245 | Passenger Door Lock Switch Unlock
E | 0.5 L-BU | 244 | Passenger Door Lock Switch Lock

### Driver Door Module (DDM) X1 (AXC or AXE)

#### Connector Part Information

- OEM: 6098-4607
- Service: 88988497
- Description: 6-Way F 2.8mm PBT (BK)

#### Terminal Part Information

- Pins: 4
- Terminal/Tray: 8100-4444/22
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

- Pins: 5
- Terminal/Tray: 8100-4445/22
- Core/Insulation Crimp: 4/4
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

#### Driver Door Module (DDM) X1 (AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | 1 RD/WH | 3240 | Battery Positive Voltage
5 | 2 BK | 550 | Ground
6 | -- | -- | Not Used

### Driver Door Module (DDM) X2 (AXC or AXE)

#### Connector Part Information

- OEM: 7283-9078-80
- Service: See Catalog
- Description: 16-Way F Kaizen 0.64 Series (BN)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Driver Door Module (DDM) X2 (AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.35 BN | 6132 | Linear Interconnect Network Bus
4 | -- | -- | Not Used
5 | 0.5 YE | 5942 | Low Reference
6 | -- | -- | Not Used
7 | 0.5 GY | 295 | Door Lock Actuator Lock Control
8 | 0.5 TN | 294 | Door Lock Actuator Unlock Control
9 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
10-12 | -- | -- | Not Used
13 | 0.5 GY/BK | 745 | Left Front Door Ajar Switch Signal
14-16 | -- | -- | Not Used

### Driver Door Module (DDM) X3 (AXC or AXE)

#### Connector Part Information

- OEM: 7283-9040-30
- Service: See Catalog
- Description: 10-Way F YESC Kaizen Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Driver Door Module (DDM) X3 (AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-BU/WH | 6160 | Outside Left Mirror Vertical Position Control
2 | 0.35 D-GN/WH | 6159 | Outside Left Mirror Horizontal Position Control
3 | 0.5 L-GN | 627 | Low Reference
4-5 | -- | -- | Not Used
6 | 0.35 WH | 7197 | Outside Left Mirror Drive Motor Common
7 | 0.5 OG | 2267 | Mirror Heating Element Voltage
8 | 0.35 PK/BK | 5855 | Low Reference (UFT)
9-10 | -- | -- | Not Used

### Driver Door Module (DDM) X4 (AXC or AXE)

#### Connector Part Information

- OEM: 7283-9065-40
- Service: See Catalog
- Description: 14-Way F Kaizen 0.64 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Driver Door Module (DDM) X4 (AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control (A45 with KA1 or KB6)
2 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control (A45 with KA1 or KB6)
3 | -- | -- | Not Used
4 | 0.35 D-BU/WH | 5978 | Low Reference (AG3)
5 | 0.35 OG | 614 | Memory Set Switch Signal (AG3)
6 | 0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal (A45 with KA1 or KB6)
7 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal (A45 with KA1)
8 | -- | -- | Not Used
9 | 0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control (A45 with KA1 or KB6)
10 | 0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED (A45 with KA1 or KB6)
11 | 0.35 PU | 6174 | Driver Heated Seat Switch Back LED (A45 with KA1)
12 | 0.35 PU | 6174 | Driver Heated Seat Switch Back LED (A45 with KB6)
13 | 0.35 BN/WH | 6064 | Memory Switch Dimming Control (AG3)
14 | 0.35 GY/BK | 5979 | Memory Seat Switch Exit Signal (AG3)

### Driver Door Module (DDM) X7 (AXC or AXE)

#### Connector Part Information

- OEM: 7283-9045
- Service: See Catalog
- Description: 10-Way F 064 Series Unsealed (WH)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Driver Door Module (DDM) X7 (AXC or AXE)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 6802 | Left Extend/Fold Mirror Motor Extend Control (DNP or DNT)
2 | 0.35 L-BU | 6803 | Passenger Mirror Motor Down Control (DNP or DNT)
3 | -- | -- | Not Used
4 | 0.35 D-GN | 784 | Driver Mirror Vertical Position Sensor Signal (A45 with DNP or DNT or DS3)
5 | 0.35 GY | 786 | Driver Mirror Horizontal Position Sensor Signal (A45 with DNP or DNT or DS3)
6 | -- | -- | Not Used
7 | 0.35 D-BU | 672 | 5-Volt Reference (A45 with DNP or DNT or DS3)
8 | 0.35 PK | 5853 | Low Reference (UFT)
9 | -- | -- | Not Used
10 | 0.35 BN | 673 | Low Reference (A45 with DNP or DNT or DS3)

### Driver Information Center (DIC) Switch (UH9)

#### Connector Part Information

- OEM: 15491277
- Service: 88988747
- Description: 5-Way F HCM 5PA Series (BK)

#### Terminal Part Information

- Terminal/Tray: SHCM-A03T-P025/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Driver Information Center (DIC) Switch (UH9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN/WH | 1358 | DIC Switch Signal
2 | 0.35 BN | 897 | Low Reference
3 | 0.35 PK | 893 | DIC Select Menu Switch Signal
4 | 0.35 PU/WH | 1382 | LED Dimming Signal
5 | 0.35 BK | 1450 | Ground

### Electronic Brake Control Module (EBCM)

#### Connector Part Information

- OEM: 31381-1005
- Service: See Catalog
- Description: 38-Way F 2.8 Series, Sealed (BK)

#### Terminal Part Information

- Pins: 1, 13, 25, 38
- Terminal/Tray: 15304720/19
- Core/Insulation Crimp: 4/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 2, 3, 5, 6, 10-12, 14-16, 18-20, 21, 24, 26-28, 31-35, 37
- Terminal/Tray: 7116-3703-02/14
- Core/Insulation Crimp: 9/9
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Electronic Brake Control Module (EBCM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 RD/BK | 142 | Battery Positive Voltage
2 | 0.5 GY | 6031 | 5-Volt Reference
3 | 0.5 WH | 320 | Engine Mount Solenoid Control (W49)
4 | -- | -- | Not Used
5 | 0.5 WH | 1294 | Variable Effort Steering Actuator Voltage (NV7)
6 | 0.5 TN | 833 | Low Reference
7-9 | -- | -- | Not Used
10 | 0.5 OG | 6030 | Brake Vacuum Sensor Signal
11 | 0.5 D-GN/WH | 817 | Vehicle Speed Signal (U3R or UZR or UVB)
12 | 0.5 L-BU | 2088 | Low Reference
13 | 3 BK/WH | 251 | Ground
14 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
15 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
16 | 0.5 YE/BK | 6032 | Low Reference
17 | -- | -- | Not Used
18 | 0.5 D-GN | 872 | Right Front Wheel Speed Sensor Signal
19 | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
20 | 0.5 OG | 885 | Low Reference
21 | 0.5 L-BU | 830 | Left Front Wheel Speed Sensor Signal
22-23 | -- | -- | Not Used
24 | 0.5 L-GN/BK | 6432 | CAN Bus Low Serial Data
25 | 2 RD/WH | 3540 | Battery Positive Voltage
26 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
27 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
28 | 0.5 BN | 1295 | Variable Effort Steering Actuator Control (NV7)
29-30 | -- | -- | Not Used
31 | 0.5 WH | 883 | Low Reference
32 | 0.5 D-GN | 2087 | 12-Volt Reference
33 | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal
34 | 0.5 YE | 873 | Low Reference
35 | 0.5 L-BU | 5986 | Communication Enable
36 | -- | -- | Not Used
37 | 0.5 TN/WH | 6433 | CAN Bus High Serial Data
38 | 2 BK/WH | 251 | Ground

### Electronic Compass Module (U80)

#### Connector Part Information

- OEM: 88988900
- Service: See Catalog
- Description: 4-Way F AIT2PB-04A-1 AKAIT II Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Electronic Compass Module (U80)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 OG | 300 | Ignition 3 Voltage
2 | 0.35 BK | 850 | Ground
3 | 0.35 D-GN | 6135 | Linear Interconnect Network Bus
4 | -- | -- | Not Used

### Engine Control Module (ECM) X1 (LLT)

#### Connector Part Information

- OEM: 1928404927
- Service: 19153157
- Description: 96-Way F 1.2 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498135/19
- Core/Insulation Crimp: Pins 1,2, 6, 7, 9, 10, 14, 15, 18, 24, 25, 30, 33-36, 38-46, 48, 49, 55-57, 59-61, 67, 70, 72, 73, 76, 77, 79-84, 88-90, 92, 93, 96 - J/J
- Core/Insulation Crimp: Pins 3-5, 26-29, 50-53, 74, 75 - K/K
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Engine Control Module (ECM) X1 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 5282 | Camshaft Phaser Exhaust Solenoid (1)
2 | 0.5 PU | 5284 | Camshaft Phaser Intake Solenoid (1)
3 | 1 PU/WH | 4906 | Direct Fuel Injector (DFI) High Voltage Cylinder 6
4 | 1 PU | 4806 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 6
5 | 1 YE | 7301 | High Pressure Fuel Pump Actuator High Control
6 | 0.5 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control
7 | 0.5 OG | 5275 | Camshaft Position Intake Sensor (1)
8 | -- | -- | Not Used
9 | 0.5 PU | 5274 | Camshaft Position Exhaust Sensor (2)
10 | 0.5 OG | 225 | Generator Turn On Signal
11-14 | -- | -- | Not Used
15 | 0.5 GY | 705 | 5-Volt Reference 2
16 | -- | -- | Not Used
17 | 0.5 TN/BK | 231 | Oil Pressure Switch Signal
18 | 0.35 BN | 7448 | Vacuum Assist Pump Relay Coil Control
19-23 | -- | -- | Not Used
24 | 0.75 YE | 581 | TAC Motor Control - 1
25 | 0.5 WH/BK | 5283 | Camshaft Phaser Exhaust Solenoid (2)
26 | 1 D-GN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
27 | 1 D-GN/WH | 4903 | Direct Fuel Injector (DFI) High Voltage Cylinder 3
28 | 1 L-GN | 4805 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 5
29 | 1 L-GN/WH | 4905 | Direct Fuel Injector (DFI) High Voltage Cylinder 5
30 | 0.5 GY | 23 | Generator Field Duty Cycle Signal
31-32 | -- | -- | Not Used
33 | 0.5 YE | 5276 | Camshaft Position Intake Sensor (2)
34 | 0.5 D-GN | 5273 | Camshaft Position Exhaust Sensor (1)
35 | 0.5 YE | 573 | CKP Sensor Signal
36 | 0.5 YE | 2918 | FRP Sensor Signal
37 | -- | -- | Not Used
38 | 0.5 GY | 598 | 5-Volt Reference 1
39 | 0.5 GY | 2701 | 5-Volt Reference 3
40 | -- | -- | Not Used
41 | 0.5 TN | 552 | Low Reference
42 | 0.5 TN | 808 | Low Reference
43 | -- | -- | Not Used
44 | 0.5 TN | 476 | Low Reference
45 | 0.5 GY | 605 | 5-Volt Reference 3
46 | 0.5 TN | 452 | Low Reference
47 | -- | -- | Not Used
48 | 0.75 BN | 582 | TAC Motor Control - 2
49 | 0.5 OG/BK | 5272 | Camshaft Phaser Intake Solenoid (2)
50 | 1 L-BU | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
51 | 1 BN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
52 | 1 D-BU | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
53 | 1 D-BU/WH | 4902 | Direct Fuel Injector (DFI) High Voltage Cylinder 2
54 | 0.5 BN/WH | 419 | MIL Control
55 | 0.5 PU | 2121 | IC 1 Control
56 | 0.5 L-BU | 2123 | IC 3 Control
57 | 0.5 D-GN | 2125 | IC 5 Control
58 | -- | -- | Not Used
59 | 0.5 D-BU | 496 | Knock Sensor 1 Signal
60 | 0.5 GY | 2303 | Knock Sensor 2 Signal
61 | -- | -- | Not Used
62-63 | -- | -- | Not Used
64 | 0.5 TN | 407 | Low Reference
65-66 | -- | -- | Not Used
67 | 0.5 TN/WH | 3111 | HO2S Low Signal (Bank 1 Sensor 1)
68-69 | -- | -- | Not Used
70 | 0.5 PU/WH | 3210 | HO2S High Signal (Bank 2 Sensor 1)
71 | -- | -- | Not Used
72 | 0.5 L-GN | 3212 | HO2S Heater Low Control Bank 2 Sensor 1
73 | 1 PU | 7300 | High Pressure Fuel Pump Actuator Low Control
74 | 1 L-BU/WH | 4904 | Direct Fuel Injector (DFI) High Voltage Cylinder 4
75 | 1 BN/WH | 4901 | Direct Fuel Injector (DFI) High Voltage Cylinder 1
76 | 0.5 PK/BK | 5291 | Ignition Voltage
77 | 0.5 PK/BK | 5292 | Ignition Voltage
78 | -- | -- | Not Used
79 | 0.5 OG/WH | 2122 | IC 2 Control
80 | 0.5 D-GN/WH | 2124 | IC 4 Control
81 | 0.5 L-BU/WH | 2126 | IC 6 Control
82 | 0.5 YE | 410 | ECT Sensor Signal
83 | 0.5 GY | 1716 | Knock Sensor 1 Signal
84 | 0.5 L-BU | 1876 | Knock Sensor 2 Signal
85-87 | -- | -- | Not Used
88 | 0.5 TN | 2752 | Low Reference
89 | 0.5 PU | 486 | TP Sensor 2 Signal
90 | 0.5 D-GN | 485 | TP Sensor 1 Signal
91 | -- | -- | Not Used
92 | 0.5 PU/WH | 3110 | HO2S High Signal (Bank 1 Sensor 1)
93 | 0.5 TN/WH | 3211 | HO2S Low Signal (Bank 1 Sensor 1)
94-95 | -- | -- | Not Used
96 | 0.5 GY/WH | 3113 | HO2S Heater Low Control Bank 1 Sensor 1

### Engine Control Module (ECM) X2 (LLT)

#### Connector Part Information

- OEM: 1928404916
- Service: 19115599
- Description: 58-Way F 2.8 Series Sealed (BK)

#### Terminal Part Information

- Pins: 1-6
- Terminal/Tray: 1928498058/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

- Pins: 7, 9-11, 13-15, 17-27, 34-39, 41-52, 54-58
- Terminal/Tray: 1928498135/19
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Engine Control Module (ECM) X2 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 BK/WH | 451 | Ground
2 | 2 BK/WH | 451 | Ground
3 | 1 PK/BK | 5290 | Ignition Voltage
4 | 2 BK/WH | 451 | Ground
5 | 1 PK/BK | 5290 | Ignition Voltage
6 | 1 PK/BK | 5290 | Ignition Voltage
7 | 0.5 GY/WH | 3122 | HO2S Heater Low Control Bank 2 Sensor 1
8 | -- | -- | Not Used
9 | 0.5 TN | 2759 | Low Reference
10 | 0.5 D-GN/WH | 465 | Fuel Pump Relay Control
11 | 0.5 TN | 5514 | Low Reference
12 | -- | -- | Not Used
13 | 0.5 YE | 492 | MAF Sensor Signal
14 | 0.5 GY | 2709 | 5-Volt Reference
15 | 0.5 D-BU | 1161 | APP Sensor 1 Signal
16 | -- | -- | Not Used
17 | 0.5 OG/BK | 1786 | Park/Neutral Signal
18 | -- | -- | Not Used
19 | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control
20 | 0.5 OG/WH | 3223 | HO2S Heater Low Control (Bank 2 Sensor 2)
21 | -- | -- | Not Used
22 | 0.5 TN | 2760 | Low Reference
23 | 0.5 TN/WH | 3121 | HO2S Low Signal (Bank 1 Sensor 2)
24 | 0.5 TN | 3221 | HO2S Low Signal (Bank 2 Sensor 2)
25 | 0.5 L-BU | 1162 | APP Sensor 2 Signal
26 | -- | -- | Not Used
27 | 0.5 D-GN | 890 | Fuel Tank Pressure Sensor Signal
28-33 | -- | -- | Not Used
34 | 0.5 BN | 1271 | Low Reference
35 | 0.5 GY | 2700 | 5-Volt Reference 3
36 | 0.5 PU | 1589 | Fuel Level Sensor Signal
37 | -- | -- | Not Used
38 | 0.5 PU | 3120 | HO2S High Signal (Bank 1 Sensor 2)
39 | 0.5 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal
40 | -- | -- | Not Used
41 | 0.5 D-BU | 5985 | Accessory Wakeup Serial Data
42 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
43 | -- | -- | Not Used
44 | 0.5 D-GN/WH | 459 | A/C Compressor Clutch Relay Control
45 | 0.5 D-BU | 473 | High Speed Cooling Fan Relay Control
46 | 0.5 D-GN | 335 | Low Speed Cooling Fan Relay Control
47 | 0.5 PU | 1272 | Low Reference
48 | 0.5 TN | 1274 | 5-Volt Reference 3
49 | 0.5 WH/BK | 1164 | 5-Volt Reference 2
50 | 0.5 L-BU | 6289 | Induction Air Temperature Sensor Signal
51 | 0.5 PU | 3220 | HO2S High Signal (Bank 2 Sensor 2)
52 | 0.5 WH | 17 | Stop Lamp Switch Signal
53 | -- | -- | Not Used
54 | 0.5 PK | 439 | Ignition Voltage
55 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
56 | 0.5 RD/WH | 540 | Battery Positive Voltage
57 | 0.5 YE | 447 | Starter Relay Coil Control
58 | 0.5 YE | 5991 | Main Relay Control

### Engine Coolant Temperature (ECT) Sensor (LLT)

#### Connector Part Information

- OEM: 1928403874
- Service: 88988963
- Description: 2-Way F Kompakt 2.8 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498054/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Engine Coolant Temperature (ECT) Sensor (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 410 | ECT Sensor Signal
2 | 0.5 TN | 476 | Low Reference

### Engine Cooling Fan - Left and Engine Cooling Fan - Right

#### Connector Part Information

- OEM: 12191387
- Service: 13506139
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12129497/1
- Core/Insulation Crimp: F/5
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### Engine Cooling Fan - Left and Engine Cooling Fan - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3 BK | 250 | Right Cooling Fan Motor Ground
B | 3 L-BU | 409 | Right Cooling Fan Motor High Control
C | 3 WH | 504 | Left Cooling Fan Motor High Control
D | 3 GY | 532 | Left Cooling Fan Motor Low Control

### Engine Oil Pressure (EOP) Switch (LLT)

#### Connector Part Information

- OEM: 12065400
- Service: 12126436
- Description: 4-Way F Metri-Pack 150 Series (GN)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Engine Oil Pressure (EOP) Switch (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/BK | 231 | Oil Pressure Switch Signal
B | 0.5 TN | 407 | Low Reference
C-D | -- | -- | Not Used

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LLT)

#### Connector Part Information

- OEM: 1928404072
- Service: 88988586
- Description: 2-Way F 2.8 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 1928498056/8
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: J-38125-561/J-35616-35 (VT)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply
2 | 0.5 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control

### Evaporative Emissions (EVAP) Canister Vent Solenoid Valve (LLT)

#### Connector Part Information

- OEM: 12052643
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Evaporative Emissions (EVAP) Canister Vent Solenoid Valve (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 RD/WH | 4140 | Battery Positive Voltage
B | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control

### Evaporator Temperature Sensor

#### Connector Part Information

- OEM: 1-968704-1
- Service: See Catalog
- Description: 2-Way F MQS Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Evaporator Temperature Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 WH | 2622 | Evaporator Temperature Sensor Signal
2 | 0.35 TN | 552 | Low Reference

### Fog Lamp - Left Front (W49 or WDA with T96)

#### Connector Part Information

- OEM: 12124819
- Service: 12085498
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fog Lamp - Left Front (W49 or WDA with T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 34 | Front Fog Lamp Voltage
B | 0.5 BK | 1350 | Ground

### Fog Lamp - Left Front (Z88)

#### Connector Part Information

- OEM: 13513272
- Service: See Catalog
- Description: 2-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Pins: A
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: B
- Terminal/Tray: 15496531/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fog Lamp - Left Front (Z88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 34 | Front Fog Lamp Voltage
B | 0.35 BK | 1250 | Ground

### Fog Lamp - Right Front (W49 or WDA with T96)

#### Connector Part Information

- OEM: 12124819
- Service: 12085498
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fog Lamp - Right Front (W49 or WDA with T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 34 | Front Fog Lamp Voltage
B | 0.5 BK | 1350 | Ground

### Fog Lamp - Right Front (Z88)

#### Connector Part Information

- OEM: 13513272
- Service: See Catalog
- Description: 2-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15496531/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Fog Lamp - Right Front (Z88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 34 | Front Fog Lamp Voltage
B | 0.35 BK | 1350 | Ground

### Fuel Injector 1 (LLT)

#### Connector Part Information

- OEM: 1928403874
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 1 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 TN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
2 | 1 BK | 4901 | Direct Fuel Injector (DFI) High Voltage Cylinder 1

### Fuel Injector 2 (LLT)

#### Connector Part Information

- OEM: 1928403874
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 2 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 TN | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
2 | 1 BK | 4902 | Direct Fuel Injector (DFI) High Voltage Cylinder 2

### Fuel Injector 3 (LLT)

#### Connector Part Information

- OEM: 1928403874
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 3 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 TN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
2 | 1 BK | 4903 | Direct Fuel Injector (DFI) High Voltage Cylinder 3

### Fuel Injector 4 (LLT)

#### Connector Part Information

- OEM: 1928403874
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 4 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 TN | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
2 | 1 BK | 4904 | Direct Fuel Injector (DFI) High Voltage Cylinder 4

### Fuel Injector 5 (LLT)

#### Connector Part Information

- OEM: 1928403874
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 5 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 TN | 4805 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 5
2 | 1 BK | 4905 | Direct Fuel Injector (DFI) High Voltage Cylinder 5

### Fuel Injector 6 (LLT)

#### Connector Part Information

- OEM: 1928403874
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 6 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 TN | 4806 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 6
2 | 1 BK | 4906 | Direct Fuel Injector (DFI) High Voltage Cylinder 6

### Fuel Pump and Sender Assembly (LLT)

#### Connector Part Information

- OEM: 15127959
- Service: 15306360
- Description: 4-Way F GT 280 Series Sealed 5.8 (BK)

#### Terminal Part Information

- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: Pins A, D: 2/5
- Core/Insulation Crimp: Pins B, C: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Fuel Pump and Sender Assembly (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 PK | 1580 | Fuel Pump Motor Low Reference
B | 2 GY | 120 | Fuel Pump Voltage
C | 0.35 TN | 2759 | Low Reference
D | 0.5 PU | 1589 | Fuel Level Sensor Signal

### Fuel Pump Flow Control Module (LLT)

#### Connector Part Information

- OEM: ASGPB-47R1A-K
- Service: See Catalog
- Description: 47-Way F ASG Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Pump Flow Control Module (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 BK | 650 | Ground
2-4 | -- | -- | Not Available
5 | 0.35 GY | 7447 | Low Reference
6 | 0.35 TN | 2501 | High Speed GMLAN Serial Data -
7 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data +
8-9 | -- | -- | Not Available
10 | 0.35 PU | 7446 | Fuel Line Pressure Sensor Signal
11-12 | -- | -- | Not Available
13 | 0.35 D-GN/WH | 465 | Fuel Pump Relay Control
14 | -- | -- | Not Available
15 | 0.35 PK | 439 | Ignition Voltage
16 | 2 PK | 1580 | Low Reference
17 | 0.5 L-BU | 5986 | Serial Data Communication Enable
18-20 | -- | -- | Not Available
21 | 0.35 TN | 2501 | High Speed GMLAN Serial Data -
22 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data +
23-31 | -- | -- | Not Available
32 | 3 RD/WH | 2940 | Battery Positive Voltage
33-35 | -- | -- | Not Available
36 | 0.35 BN | 7445 | 5-Volt Reference
37-43 | -- | -- | Not Available
44 | 0.5 GY | 7443 | Drain Wire
45-46 | -- | -- | Not Available
47 | 2 GY | 120 | Fuel Pump Voltage

### Fuel Pressure Sensor (LLT)

#### Connector Part Information

- OEM: 19115173
- Service: 19168035
- Description: 3-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Pressure Sensor (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PU | 7446 | Fuel Line Pressure Sensor Signal
2 | 0.35 GY | 7447 | Fuel Line Pressure Sensor Signal
3 | 0.35 BN | 7445 | 5-Volt Reference

### Fuel Rail Pressure (FRP) Sensor (LLT)

#### Connector Part Information

- OEM: 1928403966
- Service: See Catalog
- Description: 3-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Rail Pressure (FRP) Sensor (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 808 | Low Reference
2 | 0.5 YE | 2918 | FRP Sensor Signal
3 | 0.5 GY | 598 | 5-Volt Reference 1

### Fuel Tank Pressure (FTP) Sensor (LLT)

#### Connector Part Information

- OEM: 88988720
- Service: 19149288
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Tank Pressure (FTP) Sensor (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal
2 | 0.35 TN | 2759 | Low Reference
3 | 0.35 GY | 2709 | 5-Volt Reference

### Garage Door Opener (UG1)

#### Connector Part Information

- OEM: 09016038
- Service: See Catalog
- Description: 3-Way M P/C Egdeboard (NA)

#### Terminal Part Information

- Terminal/Tray: 08-50-0115/20
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: J-38125-213/J-35616-4A (PU)

#### Garage Door Opener (UG1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 RD/WH | 3140 | Battery Positive Voltage
2 | 0.5 GY | 8 | Instrument Panel Lamp Voltage
3 | 0.5 BK | 850 | Ground

### Generator X1

#### Connector Part Information

- OEM: 1928403137
- Service: 89046837
- Description: 2-Way F 2.8 Junior Power Timer (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Generator X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG | 225 | Generator Turn On Signal
2 | 0.5 GY | 23 | Generator Field Duty Cycle Signal

### Generator X2

#### Connector Part Information

- OEM: 7003-1171-02
- Core/Insulation Crimp: N/A
- Description: Ring Terminal

#### Generator X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 19 RD/BK | 1 | Battery Positive Voltage

### Hazard Switch

#### Connector Part Information

- OEM: 12047781
- Service: 12101864
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: A
- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

- Pins: B, C
- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Hazard Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 GY | 8 | Instrument Panel Lamp Voltage
B | 0.35 BK | 750 | Ground
C | 0.35 TN | 2144 | Hazard Switch Signal

### Head Up Display (HUD) (UV6)

#### Connector Part Information

- OEM: 175964-2
- Service: 15306185
- Description: 8-Way F AMP Multilock 040 MarkII (BK)

#### Terminal Part Information

- Terminal/Tray: 173681-2/17
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Head Up Display (HUD) (UV6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
2 | -- | -- | Not Used
3 | 0.35 BN | 622 | HUD Switch Signal
4 | 0.35 BK/WH | 1551 | Ground
5 | 0.35 L-BU/BK | 5812 | HUD Off/Dimming Control
6 | 0.5 RD/WH | 4540 | Battery Positive Voltage
7 | -- | -- | Not Used
8 | 0.35 L-GN/BK | 5699 | Low Reference

### Head Up Display (HUD) Switch (UV6)

#### Connector Part Information

- OEM: 15269798
- Service: See Catalog
- Description: 6-Way F AIT II Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Head Up Display (HUD) Switch (UV6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 L-BU/BK | 5812 | HUD Off/Dimming Control
3 | 0.35 L-GN/BK | 5699 | Low Reference
4 | 0.35 BK | 1450 | Ground
5 | 0.35 PU/WH | 1382 | LED Dimming Signal
6 | 0.35 BN | 622 | HUD Switch Signal

### Headlamp - Left (WDA with TVD)

#### Connector Part Information

- OEM: 0-1418889
- Service: See Catalog
- Description: 16-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left (WDA with TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
5 | 0.8 YE | -- | Left Headlamp Low Beam Voltage
6 | 0.8 BK | -- | Ground
7 | -- | -- | Not Used
8 | 0.5 D-GN/WH | -- | Left Headlamp High Beam Voltage
9 | 0.5 BK | -- | Ground
10-21 | -- | -- | Not Used

### Headlamp - Left (Z88 with TVD or W49)

#### Connector Part Information

- OEM: VECR-07 (04)
- Service: See Catalog
- Description: 7-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left (Z88 with TVD or W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | COAX | -- | High Intensity Discharge
2 | COAX | -- | High Intensity Discharge
3 | COAX | -- | High Intensity Discharge
4-5 | -- | -- | Not Used
6 | 0.8 BK | -- | Ground
7 | 0.8 RD | -- | Left Headlamp Low Beam Voltage (Z88)
0.8 PU | -- | Left Headlamp Low Beam Voltage (W49)

### Headlamp - Left High Beam (WDA without TVD)

#### Connector Part Information

- OEM: 699707-1
- Service: See Catalog
- Description: 2-Way F Two-Position Receptacle Housing (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left High Beam (WDA without TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | -- | Ground
B | 0.5 D-GN/WH | -- | Left Headlamp High Beam Voltage

### Headlamp - Left High Beam (X88)

#### Connector Part Information

- OEM: 12059182
- Service: 12101898
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left High Beam (X88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.25 BK | -- | Ground
B | 1.25 BK | -- | Left Headlamp High Beam Voltage

### Headlamp - Left High Beam (Z88 without TVD)

#### Connector Part Information

- OEM: 1544352-1
- Service: See Catalog
- Description: 2-Way F 2-Position Receptacle Housing (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left High Beam (Z88 without TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.5 BK | -- | Ground
A | 1.5 WH | -- | Right Headlamp High Beam Voltage

### Headlamp - Left High Beam Solenoid (W49)

#### Connector Part Information

- OEM: XLP-02V
- Service: See Catalog
- Description: 2-Way F XL Series (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left High Beam Solenoid (W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | -- | Ground
2 | 0.35 GY | -- | Left Headlamp High Beam Voltage

### Headlamp - Left High Beam Solenoid (WDA with TVD)

#### Connector Part Information

- OEM: 968705-9
- Service: 88953152
- Description: 3-Way F MQS Series (L-BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left High Beam Solenoid (WDA with TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GN/WH | -- | Left Headlamp High Beam Voltage
2 | -- | -- | Not Used
3 | 0.5 BK |  | Ground

### Headlamp - Left High Beam Solenoid (Z88 with TVD)

#### Connector Part Information

- OEM: 0-925014-1-2W
- Service: See Catalog
- Description: 2-Way F 2.8 Series (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left High Beam Solenoid (Z88 with TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
I | 1.5 BK | -- | Ground
II | 1.5 WH | -- | Left Headlamp High Beam Voltage

### Headlamp - Left Low Beam (WDA without TVD)

#### Connector Part Information

- OEM: 12059183
- Service: See Catalog
- Description: 2-Way F H11 Lamp Socket

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left Low Beam (WDA without TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | -- | Ground
B | 0.5 YE | -- | Left Headlamp Low Beam Voltage

### Headlamp - Left Low Beam (X88 or Z88 without TVD)

#### Connector Part Information

- OEM: 92095787
- Service: See Catalog
- Description: 2-Way F H11 Lamp Socket

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Left Low Beam (X88 or Z88 without TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.5 RD | -- | Left Headlamp Low Beam Voltage (Z88)
1.25 RD | -- | Ground (X88)
B | 1.5 BK | -- | Ground (Z88)
1.25 RD | -- | Left Headlamp Low Beam Voltage (X88)

### Headlamp - Right (WDA with TVD)

#### Connector Part Information

- OEM: 0-1418889
- Service: See Catalog
- Description: 16-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right (WDA with TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
5 | 0.8 YE | -- | Right Headlamp Low Beam Voltage
6 | 0.8 BK | -- | Ground
7 | -- | -- | Not Used
8 | 0.5 D-GN/WH | -- | Right Headlamp High Beam Voltage
9 | 0.5 BK | -- | Ground
10-21 | -- | -- | Not Used

### Headlamp - Right (Z88 with TVD or W49)

#### Connector Part Information

- OEM: VECR-07(04)
- Service: See Catalog
- Description: 7-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right (Z88 with TVD or W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | COAX | -- | High Intensity Discharge
2 | COAX | -- | High Intensity Discharge
3 | COAX | -- | High Intensity Discharge
4-5 | -- | -- | Not Used
6 | 0.8 BK | -- | Ground
7 | 0.8 RD | -- | Right Headlamp Low Beam Voltage (Z88)
0.8 PU | -- | Right Headlamp Low Beam Voltage (W49)

### Headlamp - Right High Beam (WDA without TVD)

#### Connector Part Information

- OEM: 699707-1
- Service: See Catalog
- Description: 2-Way F 2-Position Receptacle Housing (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right High Beam (WDA without TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | -- | Ground
B | 0.5 D-GN/WH | -- | Right Headlamp High Beam Voltage

### Headlamp - Right High Beam (X88)

#### Connector Part Information

- OEM: 12059182
- Service: 12101898
- Description: 2-Way F Metri-Pack 280 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right High Beam (X88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.25 BK | -- | Ground
B | 1.25 BK | -- | Right Headlamp High Beam Voltage

### Headlamp - Right High Beam (Z88 without TVD)

#### Connector Part Information

- OEM: 1544352-1
- Service: See Catalog
- Description: 2-Way F 2-Position Receptacle Housing (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right High Beam (Z88 without TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1.5 BK | -- | Ground
A | 1.5 WH | -- | Right Headlamp High Beam Voltage

### Headlamp - Right High Beam Solenoid (W49)

#### Connector Part Information

- OEM: XLP-02V
- Service: See Catalog
- Description: 2-Way F XL Series (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right High Beam Solenoid (W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | -- | Ground
2 | 0.35 GY | -- | Right Headlamp High Beam Voltage

### Headlamp - Right High Beam Solenoid (WDA with TVD)

#### Connector Part Information

- OEM: 968705-9
- Service: 88953152
- Description: 3-Way F MQS Series (L-BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right High Beam Solenoid (WDA with TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GN/WH | -- | Right Headlamp High Beam Voltage
2 | -- | -- | Not Used
3 | 0.5 BK |  | Ground

### Headlamp - Right High Beam Solenoid (Z88 with TVD)

#### Connector Part Information

- OEM: 0-925014-1-2W
- Service: See Catalog
- Description: 2-Way F 2.8 Series (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right High Beam Solenoid (Z88 with TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
I | 1.5 BK | -- | Ground
II | 1.5 WH | -- | Right Headlamp High Beam Voltage

### Headlamp - Right Low Beam (WDA without TVD)

#### Connector Part Information

- OEM: 12059183
- Service: See Catalog
- Description: 2-Way F H11 Lamp Socket

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right Low Beam (WDA without TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | -- | Ground
B | 0.5 YE | -- | Right Headlamp Low Beam Voltage

### Headlamp - Right Low Beam (X88 or Z88 without TVD)

#### Connector Part Information

- OEM: 92095787
- Service: See Catalog
- Description: 2-Way F H11 Lamp Socket

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp - Right Low Beam (X88 or Z88 without TVD)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.5 RD | -- | Right Headlamp Low Beam Voltage (Z88)
1.25 RD | -- | Ground (X88)
B | 1.5 BK | -- | Ground (Z88)
1.25 RD | -- | Right Headlamp Low Beam Voltage (X88)

### Headlamp Control Module - Left High Beam (W49)

#### Connector Part Information

- OEM: XARP-05V
- Service: See Catalog
- Description: 5-Way F XA Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp Control Module - Left High Beam (W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | -- | Left Headlamp High Beam Voltage
2 | 0.35 BK | -- | Ground
3 | -- | -- | Not Used
4 | 0.35 BK | -- | Ground
5 | 0.35 GY | -- | Left Headlamp High Beam Voltage

### Headlamp Control Module - Right High Beam (W49)

#### Connector Part Information

- OEM: XARP-05V
- Service: See Catalog
- Description: 5-Way F XA Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp Control Module - Right High Beam (W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | -- | Right Headlamp High Beam Voltage
2 | 0.35 BK | -- | Ground
3 | -- | -- | Not Used
4 | 0.35 BK | -- | Ground
5 | 0.35 GY | -- | Right Headlamp High Beam Voltage

### Headlamp Control Module (TSH)

#### Connector Part Information

- OEM: HLP-12V
- Service: See Catalog
- Description: 12-Way F HL Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp Control Module (TSH)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD | -- | Communication Enable
2 | 0.35 WH | -- | High Speed GMLAN Serial Data Bus-
3 | 0.35 YE | -- | High Speed GMLAN Serial Data Bus+
4 | 0.35 BK | -- | Ground
5 | 0.35 OG | -- | Linear Interconnect Network (LIN)
6 | 0.35 RD | -- | Battery Positive Voltage
7 | 0.5 RD | -- | Battery Positive Voltage
8-9 | -- | -- | Not Used
10 | 0.35 BK | -- | Ground
11 | 0.35 OG | -- | Linear Interconnect Network (LIN)
12 | 0.35 RD | -- | Battery Positive Voltage

### Headlamp Switch

#### Connector Part Information

- OEM: 15416970
- Service: See Catalog
- Description: 16-Way F Micro-Pack 64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Headlamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 WH | 103 | Headlamp Switch Headlamps On Signal
2 | 0.35 BN/WH | 301 | Rear Park Lamps Voltage
3 | 0.35 D-GN | 306 | Headlamp Switch Headlamps Off Signal
4-5 | -- | -- | Not Used
6 | 0.35 OG | 192 | Fog Lamps Enable (T96)
7 | 0.35 PU/WH | 1382 | LED Dimming Signal
8 | 0.8 BK/WH | 1551 | Ground
9 | 0.35 PU | 328 | Interior Lamp Switch Signal
10 | 0.35 L-GN | 6096 | Washer Fluid Heated Control Switch Signal (XA7)
11 | -- | -- | Not Used
12 | 0.35 PK/BK | 1597 | Courtesy Lamps Switch On Signal
13 | 0.35 D-GN | 44 | Instrument Panel Lamps Dimmer Switch Signal
14 | -- | -- | Not Used
15 | 0.35 OG/WH | 812 | 12-Volt Reference
16 | -- | -- | Not Used

### Heated and Cooled Seat Switch - Driver (KB6)

#### Connector Part Information

- OEM: 30700-1100
- Service: See Catalog
- Description: 10-Way F HDAC64 DR Series (GY)

#### Terminal Part Information

- Terminal/Tray: 1393364-2/7
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Heated and Cooled Seat Switch - Driver (KB6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED
2 | -- | -- | Not Used
3 | 0.35 PU/WH | 1382 | LED Dimming Signal
4 | 0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal
5 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal
6 | 0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control
7 | 0.5 BK | 750 | Ground
8 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control
9 | 0.35 PU | 6174 | Driver Heated Seat Switch Back LED
10 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control

### Heated and Cooled Seat Switch - Passenger (KB6)

#### Connector Part Information

- OEM: 30700-1101
- Service: See Catalog
- Description: 10-Way F HDAC64 DR Series (BK)

#### Terminal Part Information

- Terminal/Tray: 1393364-2/7
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Heated and Cooled Seat Switch - Passenger (KB6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN | 6179 | Passenger Heated Seat Switch Back Cushion LED
2 | -- | -- | Not Used
3 | 0.35 PU/WH | 1382 | LED Dimming Signal
4 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal
5 | 0.35 GY | 6182 | Passenger Heated Seat Switch Back Signal
6 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control
7 | 0.5 BK | 750 | Ground
8 | 0.35 WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control
9 | 0.35 PU | 6181 | Passenger Heated Seat Switch Back LED
10 | 0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control

### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LLT)

#### Connector Part Information

- OEM: 12092839
- Service: 15305960
- Description: 5-Way M Metri-Pack 150 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 1 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 3111 | HO2S Low Signal (Bank 1 Sensor 1)
B | 0.5 PU/WH | 3110 | HO2S High Signal (Bank 1 Sensor 1)
C | -- | -- | Not Used
D | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply
E | 0.5 GY/WH | 3113 | HO2S Heater Low Control (Bank 1 Sensor 1)

### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LLT)

#### Connector Part Information

- OEM: 12092839
- Service: 15305960
- Description: 5-Way M Metri-Pack 150 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 3121 | HO2S Low Signal (Bank 1 Sensor 2)
B | 0.5 PU | 3120 | HO2S High Signal (Bank 1 Sensor 2)
C | -- | -- | Not Used
D | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply
E | 0.5 GY/WH | 3122 | HO2S Heater Low Control (Bank 1 Sensor 2)

### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LLT)

#### Connector Part Information

- OEM: 12092839
- Service: 15305960
- Description: 5-Way M Metri-Pack 150 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 1 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 3211 | HO2S Low Signal (Bank 2 Sensor 1)
B | 0.5 PU/WH | 3210 | HO2S High Signal (Bank 2 Sensor 1)
C | -- | -- | Not Used
D | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply
E | 0.5 L-GN | 3212 | HO2S Heater Low Control (Bank 2 Sensor 1)

### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LLT)

#### Connector Part Information

- OEM: 12092839
- Service: 15305960
- Description: 5-Way M Metri-Pack 150 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 3221 | HO2S Low Signal (Bank 2 Sensor 2)
B | 0.5 PU | 3220 | HO2S High Signal (Bank 2 Sensor 2)
C | -- | -- | Not Used
D | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply
E | 0.5 OG/WH | 3223 | HO2S Heater Low Control (Bank 1 Sensor 2)

### Heated Seat Control Module - Driver X1 (KA1 without AG3)

#### Connector Part Information

- OEM: 6098-4606
- Service: See Catalog
- Description: 6-Way F 2.8 Series (BN)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Control Module - Driver X1 (KA1 without AG3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 PU | 2424 | Driver Heated Seat Back Element Control
2 | 0.8 PK | 2480 | Passenger Heated Seat Cushion Element Control
3 | 0.8 BN | 2432 | Driver Heated Seat Back Element Voltage
4 | 0.8 L-BU | 2433 | Passenger Heated Seat Back Element Control
5 | 0.8 L-GN | 2078 | Heated Seat Cushion Element Control
6 | 0.8 D-BU | 2479 | Passenger Heated Seat Element Voltage

### Heated Seat Control Module - Driver X2 (KA1 without AG3)

#### Connector Part Information

- OEM: 6098-4713
- Service: 88988652
- Description: 8-Way F 2.8 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Control Module - Driver X2 (KA1 without AG3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 RD/WH | 640 | Battery Positive Voltage
2 | 1 BK | 550 | Ground
3-4 | -- | -- | Not Used
5 | 0.35 PK | 2426 | Low Reference
6 | 0.35 YE | 2080 | Low Reference
7 | 0.35 TN | 2482 | Low Reference
8 | 0.35 L-BU | 5476 | Low Reference

### Heated Seat Control Module - Driver X3 (KA1 without AG3)

#### Connector Part Information

- OEM: 7283-9040-30
- Service: See Catalog
- Description: 10-Way F YESC Kaizen Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Heated Seat Control Module - Driver X3 (KA1 without AG3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | 0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control
5 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control
6 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
7-8 | -- | -- | Not Used
9 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control
10 | 0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control

### Heated Seat Control Module - Driver X4 (KA1 without AG3)

#### Connector Part Information

- OEM: 31410-1200
- Service: See Catalog
- Description: 20-Way F 0.64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Heated Seat Control Module - Driver X4 (KA1 without AG3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal
2 | -- | -- | Not Used
3 | 0.35 GY | 6182 | Passenger Heated Seat Switch Back Signal
4-5 | -- | -- | Not Used
6 | 0.35 BN | 6185 | Passenger Heated Seat Medium Indicator Control
7 | 0.35 BN | 6179 | Passenger Heated Seat Switch Back Cushion LED
8 | -- | -- | Not Used
9 | 0.35 YE/BK | 2079 | Heated Seat Cushion Temperature Sensor Signal
10 | 0.35 TN | 2436 | Heated Seat Back Temperature Sensor Signal
11 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal
12-13 | -- | -- | Not Used
14 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal
15 | 0.35 PU | 6174 | Driver Heated Seat Switch Back LED
16 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control
17 | 0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED
18 | 0.35 PU | 6181 | Passenger Heated Seat Switch Back LED
19 | 0.35 D-BU | 2425 | Driver Heated Seat Back Temperature Sensor Signal
20 | 0.35 GY | 2434 | Passenger Heated Seat Cushion Temperature Sensor Signal

### Heated Seat Element - Driver Back (KA1)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: Pins A, B - E/A
- Core/Insulation Crimp: Pins C, D - E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Seat Element - Driver Back (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BN | 2432 | Driver Heated Seat Back Element Voltage
B | 0.8 PU | 2424 | Driver Heated Seat Back Element Control
C | 0.35 D-BU | 2425 | Driver Heated Seat Back Temperature Sensor Signal
D | 0.35 PK | 2426 | Low Reference

### Heated Seat Element - Driver Back (KB6)

#### Connector Part Information

- OEM: 12064763
- Service: 12101876
- Description: 6-Way M Metri-Pack 150 Series, Unsealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: Pins A, F- E/A
- Core/Insulation Crimp: Pins D, E - E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Seat Element - Driver Back (KB6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BN | 2432 | Driver Heated Seat Back Element Voltage
B-C | -- | -- | Not Used
D | 0.35 D-BU | 2425 | Driver Heated Seat Back Temperature Sensor Signal
E | 0.35 PK | 2426 | Low Reference
F | 0.8 PU | 2424 | Driver Heated Seat Back Element Control

### Heated Seat Element - Driver Cushion (KA1)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: Pins A, B - E/A
- Core/Insulation Crimp: Pins C, D - E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Seat Element - Driver Cushion (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BN | 2432 | Driver Heated Seat Back Element Voltage
B | 0.8 L-GN | 2078 | Heated Seat Cushion Element Control
C | 0.35 YE/BK | 2079 | Heated Seat Cushion Temperature Sensor Signal
D | 0.35 YE | 2080 | Low Reference

### Heated Seat Element - Driver Cushion (KB6)

#### Connector Part Information

- OEM: 12064763
- Service: 12101876
- Description: 6-Way M Metri-Pack 150 Series, Unsealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: Pins A, F- E/A
- Core/Insulation Crimp: Pins B-E - E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Seat Element - Driver Cushion (KB6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 PU | 2424 | Driver Heated Seat Back Element Control
B | 0.35 D-BU | 2079 | Driver Heated Seat Temperature Sensor Signal 2
C | 0.35 YE | 2080 | Low Reference
D | 0.35 OG | 7018 | Seat Cushion Temperature Sensor Signal
E | 0.35 OG/WH | 7019 | Low Reference
F | 0.8 L-GN | 2078 | Heated Seat Cushion Element Control

### Heated Seat Element - Passenger Back (KA1)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: Pins A, B - E/A
- Core/Insulation Crimp: Pins C, D - E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Seat Element - Passenger Back (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 D-BU | 2479 | Passenger Heated Seat Element Voltage
B | 0.8 L-BU | 2433 | Passenger Heated Seat Back Element Control
C | 0.35 TN | 2436 | Heated Seat Back Temperature Sensor Signal
D | 0.35 TN | 2482 | Low Reference

### Heated Seat Element - Passenger Back (KB6)

#### Connector Part Information

- OEM: 12064763
- Service: 12101876
- Description: 6-Way M Metri-Pack 150 Series, Unsealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: Pins A, F- E/A
- Core/Insulation Crimp: Pins D, E - E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Seat Element - Passenger Back (KB6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 D-BU | 2479 | Passenger Heated Seat Element Voltage
B-C | -- | -- | Not Used
D | 0.35 TN | 2436 | Heated Seat Back Temperature Sensor Signal
E | 0.35 TN | 2482 | Low Reference
F | 0.8 TN | 2481 | Passenger Heated Seat Back Element Control

### Heated Seat Element - Passenger Cushion (KA1)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series, Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: Pins A, B - E/A
- Core/Insulation Crimp: Pins C, D - E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Seat Element - Passenger Cushion (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 D-BU | 2479 | Passenger Heated Seat Element Voltage
B | 0.8 PK | 2480 | Passenger Heated Seat Cushion Element Control
C | 0.35 GY | 2434 | Passenger Heated Seat Cushion Temperature Sensor Signal
D | 0.35 L-BU | 5476 | Low Reference

### Heated Seat Element - Passenger Cushion (KB6)

#### Connector Part Information

- OEM: 12064763
- Service: 12101876
- Description: 6-Way M Metri-Pack 150 Series, Unsealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: Pins A, F- E/A
- Core/Insulation Crimp: Pins B-E - E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Seat Element - Passenger Cushion (KB6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 TN | 2481 | Passenger Heated Seat Back Element Control
B | 0.35 GY | 2434 | Passenger Heated Seat Temperature Sensor Signal 2
C | 0.35 L-BU | 5476 | Low Reference
D | 0.35 D-BU | 5475 | Passenger Heated Seat Temperature Sensor Signal 1
E | 0.35 PK | 2435 | Low Reference
F | 0.8 PK | 2480 | Heated Seat Cushion Element Control

### Heated Seat Switch - Driver (KA1)

#### Connector Part Information

- OEM: 30700-1100
- Service: See Catalog
- Description: 10-Way F HDAC64 DR Series (GY)

#### Terminal Part Information

- Terminal/Tray: 1393364-2/7
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Heated Seat Switch - Driver (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN | 6173 | Driver Heated Seat Switch Back Cushion LED
2 | 0.35 PU/WH | 6816 | Heated Seat Indicator Dimming
3 | 0.35 PU/WH | 1382 | LED Dimming Signal
4 | 0.35 D-BU | 6172 | Driver Heated Seat Switch Back Cushion Signal
5 | 0.35 GY | 6175 | Driver Heated Seat Switch Back Signal
6 | 0.35 L-BU | 1662 | Driver Heated Seat Low Temperature Indicator Control
7 | 0.5 BK | 750 | Ground
8 | 0.35 WH/BK | 6177 | Driver Heated Seat Medium Indicator Control
9 | 0.35 PU | 6174 | Driver Heated Seat Switch Back LED
10 | 0.35 D-GN | 1661 | Driver Heated Seat High Temperature Indicator Control

### Heated Seat Switch - Passenger (KA1)

#### Connector Part Information

- OEM: 30700-1101
- Service: See Catalog
- Description: 10-Way F HDAC64 DR Series (BK)

#### Terminal Part Information

- Terminal/Tray: 1393364-2/7
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Heated Seat Switch - Passenger (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN | 6179 | Passenger Heated Seat Switch Back Cushion LED
2 | 0.35 PU/WH | 6816 | Heated Seat Indicator Dimming
3 | 0.35 PU/WH | 1382 | LED Dimming Signal
4 | 0.35 D-BU | 6180 | Passenger Heated Seat Switch Back Cushion Signal
5 | 0.35 GY | 6182 | Passenger Heated Seat Switch Back Signal
6 | 0.35 TN | 1686 | Passenger Heated Seat Low Temperature Indicator Control
7 | 0.5 BK | 750 | Ground
8 | 0.35 WH/BK | 6185 | Passenger Heated Seat Medium Indicator Control
9 | 0.35 PU | 6181 | Passenger Heated Seat Switch Back LED
10 | 0.35 YE | 1685 | Passenger Heated Seat High Temperature Indicator Control

### High Pressure Fuel Pump (LLT)

#### Connector Part Information

- OEM: 1-928-403-874
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### High Pressure Fuel Pump (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 PU | 7300 | High Pressure Fuel Pump Actuator Low Control
2 | 1 YE | 7301 | High Pressure Fuel Pump Actuator High Control

### Hood Ajar Switch (BTV)

#### Connector Part Information

- OEM: 19177527
- Service: See Catalog
- Description: 3-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Hood Ajar Switch (BTV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK/BK | 109 | Hood Ajar Switch Signal
B | 0.35 PU | 5531 | Hood Closed Switch Signal
C | 0.35 BK | 1250 | Ground

### Horn - High Note

#### Connector Part Information

- OEM: 88988434
- Service: 88988313
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A - E/A
- Core/Insulation Crimp: Pins B - 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Horn - High Note

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 1250 | Ground
B | 0.8 D-GN | 1329 | Horn Fuse Voltage

### Horn - Low Note

#### Connector Part Information

- OEM: 88988434
- Service: 88988313
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A - E/A
- Core/Insulation Crimp: Pins B - 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Horn - Low Note

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 1250 | Ground
B | 0.8 D-GN | 1329 | Horn Fuse Voltage

### Horn Switch X1

#### Connector Part Information

- OEM: 2-521102-2
- Service: See Catalog
- Description: 1-Way F 4.75 Series (RD)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Horn Switch X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 29 | Horn Control

### Horn Switch X2

#### Connector Part Information

- OEM: 2-520128-2
- Service: See Catalog
- Description: 1-Way F 6.35 Series (RD)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Horn Switch X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK/WH | 1550 | Ground

### HVAC Control Assembly - Auxiliary (without UK6)

#### Connector Part Information

- OEM: 89047355
- Service: See Catalog
- Description: 10-Way F 0.64 Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### HVAC Control Assembly - Auxiliary (without UK6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 8 | Instrument Panel Lamp Voltage
2 | 0.5 BK | 750 | Ground
3 | 0.5 GY | 596 | 5-Volt Reference
4 | 0.5 GY/BK | 1798 | Low Reference
5-6 | -- | -- | Not Used
7 | 0.5 PU/WH | 760 | Auxiliary Blower Motor Speed Control
8 | 0.5 YE | 2214 | Auxiliary Air Temperature Door Control
9 | -- | -- | Not Used
10 | 0.5 OG | 2615 | Auxiliary Mode Door Control

### HVAC Control Module X1

#### Connector Part Information

- OEM: 15126709
- Service: See Catalog
- Description: 20-Way F USCAR 0.64 Series (BN)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### HVAC Control Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | 0.35 D-GN | 734 | Inside Air Temperature Sensor Signal (CJ2)
5 | 0.35 GY | 1548 | Passenger Sunload Sensor Signal (CJ2)
6-7 | -- | -- | Not Used
8 | 0.5 PK | 2145 | Air Temperature Switch Signal - Right (C67)
0.5 PU/WH | 760 | Auxiliary Blower Motor Speed Control (CJ2 without UK6)
9 | 0.5 OG | 2615 | Auxiliary Mode Door Control (without UK6)
10 | 0.5 YE | 2214 | Auxiliary Air Temperature Door Control (without UK6)
11-14 | -- | -- | Not Used
15 | 0.35 L-BU/BK | 590 | Driver Sunload Sensor Signal (CJ2)
16 | 0.35 TN | 516 | Upper Left Air Temperature Sensor Signal (CJ2)
17 | 0.35 TN | 517 | Upper Right Air Temperature Sensor Signal (CJ2)
18 | 0.5 GY | 2599 | Auxiliary Mode Door Control (C67)
0.5 PK | 2145 | Air Temperature Switch Signal - Right (CJ2)
19 | 0.5 PU/WH | 760 | Auxiliary Blower Motor Speed Control (C67 without UK6)
0.5 GY | 2599 | Auxiliary Mode Door Control (CJ2)
20 | -- | -- | Not Used

### HVAC Control Module X2 (C67)

#### Connector Part Information

- OEM: 7283-9080-90
- Service: See Catalog
- Description: 16-Way F USCAR 0.64 Series (BU)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### HVAC Control Module X2 (C67)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PU/WH | 1382 | LED Dimming Signal
2 | 0.35 OG | 300 | Power Mode
3 | 0.35 BK/WH | 1551 | Ground
4 | 0.5 RD/WH | 4540 | Battery Positive Voltage
5 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
6-7 | -- | -- | Not Used
8 | 0.35 WH | 193 | Rear Defog Relay Control
9 | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
10 | 0.35 BK | 1450 | Ground
11 | -- | -- | Not Used
12 | 0.35 YE | 61 | Low Reference
13-16 | -- | -- | Not Used

### HVAC Control Module X2 (CJ2)

#### Connector Part Information

- OEM: 7283-9076-30
- Service: See Catalog
- Description: 16-Way F Kaizen 0.64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### HVAC Control Module X2 (CJ2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 RD/WH | 4540 | Battery Positive Voltage
2-3 | -- | -- | Not Used
4 | 0.35 L-GN/BK | 735 | Ambient Air Temperature Sensor Signal
5 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
6-7 | -- | -- | Not Used
8 | 0.35 BK/WH | 1551 | Ground
9 | 0.35 OG | 300 | Power Mode
10 | 0.35 WH | 193 | Rear Defog Relay Control
11-15 | -- | -- | Not Used
16 | 0.35 YE | 61 | Low Reference

### HVAC Control Module X3

#### Connector Part Information

- OEM: 15126710
- Service: 15126710
- Description: 20-Way F (GY)

#### Terminal Part Information

- Terminal/Tray: SAIT-A03T-M064/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215A/J35616-64B (L-BU)

#### HVAC Control Module X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 518 | Lower Left Air Temperature Sensor Signal (CJ2)
2 | 0.35 L-GN | 2275 | Mode Door Position Signal
3 | 0.35 PU | 1838 | Recirculation Door Position Signal
4 | 0.35 GY/BK | 754 | Blower Motor Speed Control
5 | 0.35 TN | 2273 | Mode Door Control
6 | 0.35 D-BU | 1199 | Air Temperature Door Control (CJ2)
7 | 0.35 D-GN | 1614 | Recirculation Door Control B
8 | 0.35 WH/BK | 1236 | Auxiliary Air Temperature Door Control
9 | -- | -- | Not Used
10 | 0.35 GY | 598 | 5-Volt Reference
11 | 0.35 TN | 520 | Lower Right Air Temperature Sensor Signal (CJ2)
12 | 0.35 L-BU | 733 | Air Temperature Door Position Signal (CJ2)
13 | 0.35 D-BU | 1646 | Auxiliary Air Temperature Door Position Signal
14 | 0.35 WH | 2622 | Evaporator Temperature Sensor Signal
15 | 0.35 WH | 119 | Mode Door Control
16 | 0.35 L-GN | 2210 | Air Temperature Door Control (CJ2)
17 | 0.35 TN/BK | 2274 | Recirculation Door Control A
18 | 0.35 GY/BK | 2778 | Right Air Temperature Door Control A
19 | 0.35 TN | 552 | Low Reference
20 | 0.35 YE | 1791 | Low Reference

### HVAC Control Module X4

#### Connector Part Information

- OEM: 7283-9079-60
- Service: See Catalog
- Description: 16-Way F 064 Series Unsealed (GN)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### HVAC Control Module X4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 GY | 596 | 5-Volt Reference
3 | 0.5 L-GN/WH | 5729 | Auxiliary Mode Motor Voltage
4 | 0.5 BN | 6555 | Auxiliary Temperature Motor Voltage
5 | 0.5 GY/BK | 1798 | Low Reference (C67)
6 | 0.5 GY/BK | 1798 | Low Reference
7-9 | -- | -- | Not Used
10 | 0.5 D-GN | 2211 | Auxiliary Blower Motor Speed Control
11 | 0.5 OG | 2215 | Auxiliary Mode Door Control
12 | 0.5 GY | 2614 | Auxiliary Air Temperature Door Control
13-16 | -- | -- | Not Used

### I/P Switch Assembly

#### Connector Part Information

- OEM: 31410-1120
- Service: See Catalog
- Description: 12-Way F 0.64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### I/P Switch Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN/WH | 1571 | Traction Control Switch Signal
2 | -- | -- | Not Used
3 | 0.35 BK | 750 | Ground
4 | 0.35 PU/WH | 1382 | LED Dimming Signal
5 | 0.35 GY | 391 | Rear Window Wiper Switch Signal (W49)
6 | 0.35 WH | 2283 | Rear Wiper/Washer Switch Voltage (W49)
7 | 0.35 D-GN/WH | 5800 | Liftgate Open/Close Switch Signal (TB5)
8 | 0.35 D-GN | 6112 | Power Liftgate On/Off Switch Signal (TB5)
9-10 | -- | -- | Not Used
11 | 0.35 L-BU | 553 | Tow/Haul Switch Signal
12 | 0.35 L-GN | 2270 | Rear Window Washer Relay Control (W49)

### Ignition Coil 1 (LLT)

#### Connector Part Information

- OEM: 1928403441
- Service: 88988582
- Description: 4-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Ignition Coil 1 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PU | 2121 | IC 1 Control
2 | 1 PK/BK | 5291 | Ignition 1 Voltage
3 | 1 BK | 2550 | Ground
4 | 1 BK | 2550 | Ground

### Ignition Coil 2 (LLT)

#### Connector Part Information

- OEM: 1928403441
- Service: 88988582
- Description: 4-Way F Sealed (BK)

#### Terminal Part Information

- Pins: 1, 2
- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Ignition Coil 2 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG/WH | 2122 | IC 2 Control
2 | 1 PK/BK | 5292 | Ignition 1 Voltage
3 | 1 BK | 2650 | Ground
4 | 1 BK | 2650 | Ground

### Ignition Coil 3 (LLT)

#### Connector Part Information

- OEM: 1928403441
- Service: 88988582
- Description: 4-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Ignition Coil 3 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU | 2123 | IC 3 Control
2 | 1 PK/BK | 5291 | Ignition 1 Voltage
3 | 1 BK | 2550 | Ground
4 | 1 BK | 2550 | Ground

### Ignition Coil 4 (LLT)

#### Connector Part Information

- OEM: 1928403441
- Service: 88988582
- Description: 4-Way F Sealed (BK)

#### Terminal Part Information

- Pins: 1, 2
- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Ignition Coil 4 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN/WH | 2124 | IC 4 Control
2 | 1 PK/BK | 5292 | Ignition 1 Voltage
3 | 1 BK | 2650 | Ground
4 | 1 BK | 2650 | Ground

### Ignition Coil 5 (LLT)

#### Connector Part Information

- OEM: 1928403441
- Service: 88988582
- Description: 4-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Ignition Coil 5 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 2125 | IC 5 Control
2 | 1 PK/BK | 5291 | Ignition 1 Voltage
3 | 1 BK | 2550 | Ground
4 | 1 BK | 2550 | Ground

### Ignition Coil 6 (LLT)

#### Connector Part Information

- OEM: 1928403441
- Service: 88988582
- Description: 4-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Ignition Coil 6 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU/WH | 2126 | IC 6 Control
2 | 1 PK/BK | 5292 | Ignition 1 Voltage
3 | 1 BK | 2650 | Ground
4 | 1 BK | 2650 | Ground

### Ignition Lock Cylinder Control Actuator

#### Connector Part Information

- OEM: 7283725830
- Service: See Catalog
- Description: 2-Way F GT 150 Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Lock Cylinder Control Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK | 1450 | Ground
2 | 0.35 PU/WH | 1630 | Steering Column Key Cylinder Lock Solenoid Control

### Ignition Switch

#### Connector Part Information

- OEM: HCMPBC06K
- Service: See Catalog
- Description: 6-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: SHCM-A03T-P025/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Ignition Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PK | 3 | Ignition Voltage
2 | 0.35 RD/WH | 1040 | Battery Positive Voltage
3 | 0.35 BN | 4 | Accessory Voltage
4 | 0.35 WH | 1390 | Off/Run/Crank Voltage
5 | -- | -- | Not Used
6 | 0.35 WH/BK | 1073 | Ignition Key Resistor Signal

### Inflatable Restraint Front End Sensor - Left

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front End Sensor - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN/OG | 5045 | Low Reference
B | 0.35 YE | 354 | Discriminating Sensor - Signal

### Inflatable Restraint Front End Sensor - Right

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front End Sensor - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 5600 | Low Reference
B | 0.35 D-GN | 1409 | Discriminating Sensor - Right - Signal

### Inflatable Restraint Front Passenger Presence System (PPS) Sensor

#### Connector Part Information

- OEM: 6098-5519
- Service: 19153764
- Description: 4-Way M Low Profile 1.5 Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: N/A

#### Inflatable Restraint Front Passenger Presence System (PPS) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
2 | -- | -- | Not Used
3 | 0.35 RD/WH | 1340 | Battery Positive Voltage
4 | 0.35 BK/WH | 1751 | Ground

### Inflatable Restraint I/P Module

#### Connector Part Information

- OEM: SNAPB-05UN-1FYS
- Service: 19153434
- Service Caution: The connector at the Inflatable Restraint Module cannot be disconnected or removed without damage to the module. If the connector is removed from the module, the entire module with harness must be replaced.
- Description: 5-Way F 0.64 Series Unsealed (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint I/P Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 YE | 3025 | I/P Module - Stage 1 - High Control
2 | 0.35 OG | 3024 | I/P Module - Stage 1 - Low Control
3 | -- | -- | Not Used
4 | 0.35 GY | 3027 | I/P Module - Stage 2 - High Control
5 | 0.35 PU | 3026 | I/P Module - Stage 2 - Low Control

### Inflatable Restraint I/P Module Indicator

#### Connector Part Information

- OEM: 15398877
- Service: See Catalog
- Description: 5-Way F HCM Series (WH)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Inflatable Restraint I/P Module Indicator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-BU | 2307 | Passenger Air Bag On Indicator Control
2 | 0.35 BK | 1450 | Ground
3 | 0.35 D-GN | 2308 | Passenger Air Bag Off Indicator Control
4 | 0.35 PK | 1139 | Ignition Voltage
5 | 0.35 PU | 5234 | Passenger Seat Belt Indicator

### Inflatable Restraint Roof Rail Module - Driver

#### Connector Part Information

- OEM: 12186799
- Service: 15306012
- Service Caution: The connector at the Inflatable Restraint Module cannot be disconnected or removed without damage to the module. If the connector is removed from the module, the entire module with harness must be replaced.
- Description: 2-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: 12066337/18
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-5 (PU)

#### Inflatable Restraint Roof Rail Module - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU/WH | 5019 | Roof Rail Module - Left - High Control
B | 0.35 PK | 5020 | Roof Rail Module - Left - Low Control

### Inflatable Restraint Roof Rail Module - Passenger

#### Connector Part Information

- OEM: 12186799
- Service: 15306012
- Service Caution: The connector at the Inflatable Restraint Module cannot be disconnected or removed without damage to the module. If the connector is removed from the module, the entire module with harness must be replaced.
- Description: 2-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: 12066337/18
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-5 (PU)

#### Inflatable Restraint Roof Rail Module - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE/BK | 5021 | Roof Rail Module - Right - High Control
B | 0.35 WH/BK | 5022 | Roof Rail Module - Right - Low Control

### Inflatable Restraint Sensing and Diagnostic Module (SDM)

#### Connector Part Information

- OEM: 6-184464-5
- Service: See Catalog
- Description: 60-Way F GET Series (YE)

#### Terminal Part Information

- Terminal/Tray: Service With Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Inflatable Restraint Sensing and Diagnostic Module (SDM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK/WH | 1751 | Ground
2 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
3 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
4 | 0.35 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control
5 | 0.35 WH | 3023 | Steering Wheel Module - Stage 2 - High Control
6 | 0.35 GY | 3027 | I/P Module - Stage 2 - High Control
7 | 0.35 PU | 3026 | I/P Module - Stage 2 - Low Control
8 | 0.35 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
9 | 0.35 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
10 | 0.35 YE | 3025 | I/P Module - Stage 1 - High Control
11 | 0.35 OG | 3024 | I/P Module - Stage 1 - Low Control
12 | 0.5 YE/BK | 2138 | Side Impact Module - Left Front - Low Control
13 | 0.5 BN | 2137 | Side Impact Module - Left Front - High Control
14 | 0.5 TN/WH | 2135 | Side Impact Module - Right Front - High Control
15 | 0.5 L-GN | 2136 | Side Impact Module - Right Front - Low Control
16 | 0.5 YE/BK | 3065 | Seat Belt Buckle Pretensioner - Left - Low Control
17 | 0.5 WH | 3064 | Seat Belt Buckle Pretensioner - Left - High Control
18 | 0.5 TN | 3062 | Seat Belt Buckle Pretensioner - Right - High Control
19 | 0.5 L-BU/BK | 3063 | Seat Belt Buckle Pretensioner - Right - Low Control
20 | 0.5 PK | 5020 | Roof Rail Module - Left - Low Control
21 | 0.5 PU/WH | 5019 | Roof Rail Module - Left - High Control
22 | 0.5 YE/BK | 5021 | Roof Rail Module - Right - High Control
23 | 0.5 WH/BK | 5022 | Roof Rail Module - Right - Low Control
24 | 0.5 OG/BK | 2119 | Seat Belt Retractor Pretensioner - Left - Low Control
25 | 0.5 TN/WH | 2118 | Seat Belt Retractor Pretensioner - Left - High Control
26 | 0.5 L-GN | 2116 | Seat Belt Retractor Pretensioner - Right - High Control
27 | 0.5 OG | 2117 | Seat Belt Retractor Pretensioner - Right - Low Control
28 | 0.35 PK | 5057 | Low Reference
29 | -- | -- | Not Used
30 | 0.35 L-BU | 5056 | Seat Position Sensor - Right - Signal (W49)
31 | 0.35 RD/WH | 1340 | Battery Positive Voltage
32 | 0.5 PK | 1139 | Ignition Voltage
33-35 | -- | -- | Not Used
36 | 0.35 YE | 354 | Discriminating Sensor - Signal
37 | 0.35 D-GN | 1409 | Discriminating Sensor - Right - Signal
38 | 0.35 TN/OG | 5045 | Front End Sensor - Signal
39 | 0.35 GY | 5600 | Low Reference
40 | 0.35 PU/WH | 6628 | Low Reference
41 | 0.35 WH/BK | 6629 | Low Reference
42 | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal
43 | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal
44 | 0.35 L-BU | 6622 | Left Rear Side Impact Sensing Module Signal
45 | 0.35 L-BU/WH | 6626 | Right Rear Side Impact Sensing Module Signal
46 | 0.35 L-GN/BK | 6623 | Low Reference
47 | 0.35 PK/BK | 6627 | Low Reference
48-57 | -- | -- | Not Used
58 | 0.35 YE/BK | 5229 | Roll Over Sensor High Signal
59 | 0.35 D-GN | 5016 | Seat Belt Switch - Left - Signal
60 | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal

### Inflatable Restraint Side Impact Module - Left

#### Connector Part Information

- OEM: SNAPB-02UN-1FYS
- Service: 19153427
- Service Caution: The connector at the Inflatable Restraint Module cannot be disconnected or removed without damage to the module. If the connector is removed from the module, the entire module with harness must be replaced.
- Description: 2-Way F 0.64 Series Unsealed (YE)

#### Terminal Part Information

- Terminal/Tray: See Catalog
- Core/Insulation Crimp: See Catalog
- Release Tool/Test Probe: See Catalog

#### Inflatable Restraint Side Impact Module - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 2137 | Side Impact Module - Left Front - High Control
2 | 0.5 YE/BK | 2138 | Side Impact Module - Left Front - Low Control

### Inflatable Restraint Side Impact Module - Right

#### Connector Part Information

- OEM: SNAPB-02UN-1FYS
- Service: 19153427
- Service Caution: The connector at the Inflatable Restraint Module cannot be disconnected or removed without damage to the module. If the connector is removed from the module, the entire module with harness must be replaced.
- Description: 2-Way F 0.64 Series Unsealed (YE)

#### Terminal Part Information

- Terminal/Tray: See Catalog
- Core/Insulation Crimp: See Catalog
- Release Tool/Test Probe: See Catalog

#### Inflatable Restraint Side Impact Module - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN/WH | 2135 | Side Impact Module - Right Front - High Control
2 | 0.5 L-GN | 2136 | Side Impact Module - Right Front - Low Control

### Inflatable Restraint Side Impact Sensor (SIS) - Left Front

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Side Impact Sensor (SIS) - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU/WH | 6628 | Low Reference
B | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal

### Inflatable Restraint Side Impact Sensor (SIS) - Left Rear

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Side Impact Sensor (SIS) - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN/BK | 6623 | Low Reference
B | 0.35 L-BU | 6622 | Left Rear Side Impact Sensing Module Signal

### Inflatable Restraint Side Impact Sensor (SIS) - Right Front

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Side Impact Sensor (SIS) - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH/BK | 6629 | Low Reference
B | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal

### Inflatable Restraint Side Impact Sensor (SIS) - Right Rear

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Sealed 4.0 (YE)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Side Impact Sensor (SIS) - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK/BK | 6627 | Low Reference
B | 0.35 L-BU/WH | 6626 | Right Rear Side Impact Sensing Module Signal

### Inflatable Restraint Steering Wheel Module Coil X1

#### Connector Part Information

- OEM: 15269795
- Service: See Catalog
- Description: 10-Way F AIT II Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service With Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 28 | Horn Relay Control
2 | 0.35 PU | 1375 | 12-Volt Reference
3 | 0.35 PU/WH | 7005 | LED Dimming Signal
4 | 0.35 BK/WH | 1551 | Ground
5 | 0.35 GY | 1884 | Cruise Control Switch Signal
6 | 0.35 GN/WH | 7158 | Cruise Control Indicator Dimming Signal
7 | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
8-10 | -- | -- | Not Used

### Inflatable Restraint Steering Wheel Module Coil X2

#### Connector Part Information

- OEM: 15269795
- Service: See Catalog
- Description: 10-Way F AIT II Series (BK)

#### Terminal Part Information

- Terminal/Tray: Service With Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-3 | -- | -- | Not Used
4 | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
5 | 0.35 GN/WH | 7158 | Cruise Control Indicator Dimming Signal
6 | 0.35 GY | 1884 | Cruise Control Switch Signal
7 | 0.35 BK/WH | 1551 | Ground
8 | 0.35 PU/WH | 7005 | LED Dimming Signal
9 | 0.35 PU | 1375 | 12-Volt Reference
10 | 0.35 D-GN | 29 | Horn Control

### Inflatable Restraint Steering Wheel Module Coil X3

#### Connector Part Information

- OEM: 15393421
- Service: 88987853
- Description: 4-Way F Micro-Pack 064 Series (YE)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
2 | 0.35 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
3 | 0.35 WH | 3023 | Steering Wheel Module - Stage 2 - High Control
4 | 0.35 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control

### Inflatable Restraint Steering Wheel Module X1

#### Connector Part Information

- OEM: 54560236
- Service: See Catalog
- Description: 2-Way F (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
2 | 0.35 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control

### Inflatable Restraint Steering Wheel Module X2

#### Connector Part Information

- OEM: 54560222
- Service: See Catalog
- Description: 2-Way F (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 WH | 3023 | Steering Wheel Module - Stage 2 - High Control
2 | 0.35 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control

### Inflatable Restraint Vehicle Rollover Sensor

#### Connector Part Information

- OEM: 6189-7001
- Service: See Catalog
- Description: 6-Way F 0.64 Series, Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service With Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Inflatable Restraint Vehicle Rollover Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1340 | Battery Positive Voltage
2 | -- | -- | Not Used
3 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
4 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
5 | 0.35 YE/BK | 5229 | Roll Over Sensor High Signal
6 | 0.5 BK/WH | 1751 | Ground

### Infrared Transmitter (U42)

#### Connector Part Information

- OEM: 7283-9078-80
- Service: See Catalog
- Description: 16-Way F Kaizen 0.64 Series (BN)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Infrared Transmitter (U42)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-BU | 5826 | Left DVD Audio Signal (+)
2 | 0.35 PU | 6979 | DVD Audio Common (-)
3 | 0.35 WH | 5828 | Right DVD Audio Signal (+)
4 | 0.5 PK | 5829 | Infrared Module Voltage
5-7 | -- | -- | Not Used
8 | 0.35 OG/BK | 5831 | Remote Infrared Signal (+)
9 | 0.35 OG/BK | 5329 | Left Infrared Audio Signal (+)
10 | 0.35 BN/WH | 5331 | Infrared Audio Low Reference
11 | 0.35 PU/WH | 5330 | Right Infrared Audio Signal (+)
12 | 0.5 BK/WH | 351 | Ground
13-15 | -- | -- | Not Used
16 | 0.35 TN/WH | 5830 | Remote Infrared Signal (-)

### Input Speed Sensor (ISS)

#### Connector Part Information

- OEM: 15467085
- Service: Non-Serviceable
- Description: 2-Way F M/P 150.2 Series P2S (L-GY)

#### Terminal Part Information

- Terminal/Tray: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Input Speed Sensor (ISS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | -- | ISS High Signal
B | 0.5 BK | -- | ISS Low Signal

### Inside Air Temperature Sensor (CJ2)

#### Connector Part Information

- OEM: 12059252
- Service: 12102749
- Description: 2-Way M Metri-Pack 150 Series (RD)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Inside Air Temperature Sensor (CJ2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 734 | Inside Air Temperature Sensor Signal
B | 0.35 YE | 61 | Low Reference

### Inside Rearview Mirror

#### Connector Part Information

- OEM: 917981-2
- Service: 15306351
- Description: 16-Way F 0.040/0.070 HYBRID I/O (BK)

#### Terminal Part Information

- Terminal/Tray: 175266-5/15
- Core/Insulation Crimp: Pins 5, 13, 15, 16 - J/J
- Core/Insulation Crimp: Pins 8, 9, 11, 12, 14 - K/K
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Inside Rearview Mirror

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-4 | -- | -- | Not Used
5 | 0.35 GY | 1690 | Automatic Day/Night Mirror Signal (DNP)
6-7 | -- | -- | Not Used
8 | 0.5 BK | 850 | Ground (UE1 or DD8)
9 | 0.5 BK/WH | 24 | Backup Lamp Voltage (DD8)
10 | -- | -- | Not Used
11 | 0.5 BK/GN | 2514 | Keypad Signal (UE1)
12 | 0.5 BK/L-GN | 2515 | Keypad Voltage (UE1)
13 | 0.35 BK/YE | 43 | Ignition Voltage (DD8)
14 | 0.5 BK/GY | 2516 | Keypad Green LED Signal (UE1)
15 | 0.35 BN/WH | 2517 | Keypad Red LED Signal (UE1)
16 | 0.35 BK/RD | 1691 | Low Reference (DNP)

### Instrument Panel Cluster (IPC)

#### Connector Part Information

- OEM: 15126711
- Service: See Catalog
- Description: 20-Way F 0.64 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Instrument Panel Cluster (IPC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1840 | Battery Positive Voltage
2 | 0.35 BK/WH | 1551 | Ground
3 | 0.35 PK | 1139 | Ignition Voltage
4 | 0.35 BN/WH | 419 | MIL Control
5 | -- | -- | Not Used
6 | 0.35 PK | 893 | DIC Select Menu Switch Signal (UH9)
7 | 0.35 D-GN/WH | 1358 | DIC Switch Signal (UH9)
8 | -- | -- | Not Used
9 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
10 | -- | -- | Not Used
11 | 0.35 PU | 5234 | Passenger Seat Belt Indicator
12 | 0.35 D-BU | 2307 | Passenger Air Bag On Indicator Control
13 | 0.35 D-GN | 2308 | Passenger Air Bag Off Indicator Control
14 | 0.35 TN | 185 | Low Washer Fluid Indicator Control
15 | 0.35 D-BU/WH | 5970 | Washer Fluid Heated Control Switch LED Voltage (XA7)
16-17 | -- | -- | Not Used
18 | 0.35 TN/WH | 33 | Brake Warning Indicator Control
19 | 0.35 BN | 897 | Low Reference (UH9)
20 | -- | -- | Not Used

### Knock Sensor (KS) 1 (LLT)

#### Connector Part Information

- OEM: 88986864
- Service: See Catalog
- Description: 2-Way F GT 150 Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Knock Sensor (KS) 1 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | 496 | Knock Sensor 1 Signal
B | 0.5 GY | 1716 | Knock Sensor 1 Signal

### Knock Sensor (KS) 2 (LLT)

#### Connector Part Information

- OEM: 88986864
- Service: See Catalog
- Description: 2-Way F GT 150 Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Knock Sensor (KS) 2 (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 1876 | Knock Sensor 2 Signal
B | 0.5 GY | 2303 | Knock Sensor 2 Signal

### License Lamp - Left

#### Connector Part Information

- OEM: V10170
- Service: See Catalog
- Description: 2-Way F Molded Wedge Base Lamp Socket (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### License Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | -- | Left Park Lamp Voltage (WDA or Z88)
0.5 BK | -- | Left Park Lamp Voltage (W49)
0.5 PU | 709 | Left Park Lamp Voltage (X88)
B | 0.5 BK | -- | Ground (WDA or Z88)
0.5 WH | -- | Ground (W49)
0.5 BK | 650 | Ground (X88)

### License Lamp - Right

#### Connector Part Information

- OEM: V10170
- Service: See Catalog
- Description: 2-Way F Molded Wedge Base Lamp Socket (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### License Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 WH | -- | Left Park Lamp Voltage (WDA or Z88)
0.5 BK | -- | Left Park Lamp Voltage (W49)
0.5 PU | 709 | Left Park Lamp Voltage (X88)
B | 0.5 BK | -- | Ground (WDA or Z88)
0.5 WH | -- | Ground (W49)
0.5 BK | 650 | Ground (X88)

### Liftgate Control Switch - Exterior

#### Connector Part Information

- OEM: 7282-6444-60
- Service: See Catalog
- Description: 2-Way M 1.5 Series (GN)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### Liftgate Control Switch - Exterior

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 5797 | Rear Closure Handle Switch Open Signal (TB4)
0.35 GY/BK | 6113 | Rear Liftgate Open/Close Switch Signal (TB5)
2 | 0.35 BK | 650 | Ground (TB4)
0.35 PU/WH | 5801 | Low Reference (TB5)

### Liftgate Control Switch - Interior (TB5)

#### Connector Part Information

- OEM: 7282-6443-40
- Service: See Catalog
- Description: 2-Way M 1.5 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: 7114-4100-08/9
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### Liftgate Control Switch - Interior (TB5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY/BK | 6113 | Rear Liftgate Open/Close Switch Signal
2 | 0.35 PU/WH | 5801 | Low Reference

### Liftgate Courtesy Lamp - Left

#### Connector Part Information

- OEM: 12186713
- Service: See Catalog
- Description: 2-Way F Faston (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Liftgate Courtesy Lamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 650 | Ground
2 | 0.5 GY/BK | 690 | Courtesy Lamp High Control

### Liftgate Courtesy Lamp - Right

#### Connector Part Information

- OEM: 12186713
- Service: See Catalog
- Description: 2-Way F Faston (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Liftgate Courtesy Lamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | 650 | Ground
2 | 0.5 GY/BK | 690 | Courtesy Lamp High Control

### Liftgate Latch Assembly (TB4)

#### Connector Part Information

- OEM: 15476199
- Service: 88988358
- Description: 6-Way F GT 280 Series, Sealed (GN)

#### Terminal Part Information

- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Liftgate Latch Assembly (TB4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU | 6128 | Ground
2 | -- | -- | Not Used
3 | 0.5 BK | 650 | Ground
4 | 0.5 L-GN | 5926 | Rear Access Open Switch Signal
5 | 0.35 BK | 650 | Ground
6 | 0.5 PK/BK | 1303 | Liftgate Ajar Switch Signal

### Liftgate Latch Assembly (TB5)

#### Connector Part Information

- OEM: 15476196
- Service: 88988498
- Description: 6-Way F GT 280 Series, Sealed (BK)

#### Terminal Part Information

- Pins: 1, 3
- Terminal/Tray: 15304720/19
- Core/Insulation Crimp: 4/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: 2, 4-6
- Terminal/Tray: 15304719/19
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Liftgate Latch Assembly (TB5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 BN | 5790 | Liftgate Cinch Latch Motor Open Control
2 | 0.35 PU/WH | 5801 | Low Reference
3 | 2 L-BU | 5791 | Liftgate Cinch Latch Motor Close Control
4 | 0.35 D-GN | 5512 | Latch Sector Switch Signal
5 | 0.35 GY | 7000 | Latch Pawl Switch Signal
6 | 0.35 PK/BK | 6000 | Latch Ratchet Switch Signal

### Liftgate Module (LGM) X1 (TB5)

#### Connector Part Information

- OEM: 15136073
- Service: See Catalog
- Description: 16-Way F Kaizen 0.64 (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4618-02/14
- Core/Insulation Crimp: P/P
- Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Liftgate Module (LGM) X1 (TB5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 6112 | Power Liftgate On/Off Switch Signal
2-3 | -- | -- | Not Used
4 | 0.35 D-GN | 5512 | Latch Sector Switch Signal
5 | 0.35 PK/BK | 6000 | Latch Ratchet Switch Signal
6 | 0.35 GY | 7000 | Latch Pawl Switch Signal
7 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
8 | 0.35 WH/BK | 6126 | Liftgate Object Sensor 2 Signal
9-11 | -- | -- | Not Used
12 | 0.35 D-GN/WH | 5800 | Liftgate Open/Close Switch Signal
13 | -- | -- | Not Used
14 | 0.35 GY/BK | 6113 | Rear Liftgate Open/Close Switch Signal
15 | -- | -- | Not Used
16 | 0.35 PU/WH | 5801 | Low Reference

### Liftgate Module (LGM) X2 (TB5)

#### Connector Part Information

- OEM: 15134094
- Service: 88988497
- Description: 6-Way F 2.8 Series (BK)

#### Terminal Part Information

- Pins: 4
- Terminal/Tray: 8100-4443/22
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

- Pins: 1-3, 6
- Terminal/Tray: 8100-4445/22
- Core/Insulation Crimp: Pins 1, 2, 6 - 4/4
- Core/Insulation Crimp: Pins 3 - F/D
- Release Tool/Test Probe: 15315247/J-35616-35 (VT)

#### Liftgate Module (LGM) X2 (TB5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 BN | 5790 | Liftgate Cinch Latch Motor Open Control
2 | 2 L-BU | 5791 | Liftgate Cinch Latch Motor Close Control
3 | 3 RD | 1342 | Battery Positive Voltage
4 | 0.5 RD/WH | 1840 | Battery Positive Voltage
5 | -- | -- | Not Used
6 | 3 BK | 650 | Ground

### Liftgate Module (LGM) X3 (TB5)

#### Connector Part Information

- OEM: 7283-8398-40
- Service: See Catalog
- Description: 14-Way F 0.64 2.8 YESC Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Liftgate Module (LGM) X3 (TB5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 WH | 5798 | Liftgate Open/Close Motor Open Control
2 | 2 BN/WH | 5799 | Liftgate Open/Close Motor Close Control
3 | 0.35 TN | 5794 | Liftgate Engage/Disengage Motor Engage Control
4 | 0.35 D-BU | 5795 | Liftgate Engage/Disengage Motor Disengage Control
5 | 0.35 D-BU/WH | 5796 | Liftgate Full Open Switch Signal
6 | 0.35 OG | 5804 | Low Reference
7 | -- | -- | Not Used
8 | 0.35 BK/TN | 5803 | Liftgate Position Sensor Voltage Reference
9 | 0.35 L-BU/WH | 5805 | Liftgate Position Sensor Signal (1)
10 | 0.35 PU | 5806 | Liftgate Position Sensor Signal (2)
11 | 0.35 D-GN/WH | 5804 | Low Reference
12-14 | -- | -- | Not Used

### Liftgate Motor Assembly X1 (TB5)

#### Connector Part Information

- OEM: 15316639
- Service: 15306434
- Description: 2-Way F 040 Multilock Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Liftgate Motor Assembly X1 (TB5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 5794 | Liftgate Engage/Disengage Motor Engage Control
2 | 0.35 D-BU | 5795 | Liftgate Engage/Disengage Motor Disengage Control

### Liftgate Motor Assembly X2 (TB5)

#### Connector Part Information

- OEM: 15316639
- Service: 15306434
- Description: 2-Way F 040 Multilock Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Liftgate Motor Assembly X2 (TB5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 OG | 5804 | Low Reference
2 | 0.35 D-BU/WH | 5796 | Liftgate Full Open Switch Signal

### Liftgate Object Sensor - Left (TB5)

#### Connector Part Information

- OEM: 12048457
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Liftgate Object Sensor - Left (TB5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU/WH | 5801 | Low Reference
B | 0.35 PK/BK | 5802 | Liftgate Object Sensor Signal

### Liftgate Object Sensor - Right (TB5)

#### Connector Part Information

- OEM: 12048457
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Liftgate Object Sensor - Right (TB5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK/BK | 5802 | Liftgate Object Sensor Signal
B | 0.35 WH/BK | 6126 | Liftgate Object Sensor 2 Signal

### Marker Lamp - Left Front (W49 or Z88)

#### Connector Part Information

- OEM: 7712-5354-4WB
- Service: See Catalog
- Description: 2-Way F Lamp Socket, Axial (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Left Front (W49 or Z88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BU | -- | Left Park Lamp Voltage
B | 0.5 BK | -- | Ground

### Marker Lamp - Left Front (WDA)

#### Connector Part Information

- OEM: 12146418
- Service: See Catalog
- Description: 2-Way F Lamp Socket (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Left Front (WDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | -- | Ground
2 | 0.5 PU | -- | Left Park Lamp Voltage

### Marker Lamp - Left Front (X88)

#### Connector Part Information

- OEM: 6341
- Service: See Catalog
- Description: 2-Way F Lamp Socket (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Left Front (X88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 RD | -- | Left Park Lamp Voltage
B | 0.8 BK | -- | Ground

### Marker Lamp - Left Rear (W49)

#### Connector Part Information

- OEM: 7712-5354-4WB
- Service: See Catalog
- Description: 2-Way F Lamp Socket, Axial (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Left Rear (W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | -- | Left Park Lamp Voltage
B | 0.5 BK | -- | Ground

### Marker Lamp - Left Rear (WDA)

#### Connector Part Information

- OEM: 12146418
- Service: See Catalog
- Description: 2-Way F Lamp Socket (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Left Rear (WDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | -- | Left Park Lamp Voltage
B | 0.8 BK | -- | Ground

### Marker Lamp - Left Rear (X88)

#### Connector Part Information

- OEM: 12110053
- Service: See Catalog
- Description: 2-Way F Lamp Socket (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Left Rear (X88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | -- | Left Park Lamp Voltage
B | 0.8 BK | -- | Ground

### Marker Lamp - Right Front (W49 or Z88)

#### Connector Part Information

- OEM: 7712-5354-4WB
- Service: See Catalog
- Description: 2-Way F Lamp Socket, Axial (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Right Front (W49 or Z88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BU | -- | Right Park Lamp Voltage
B | 0.5 BK | -- | Ground

### Marker Lamp - Right Front (WDA)

#### Connector Part Information

- OEM: 12146418
- Service: See Catalog
- Description: 2-Way F Lamp Socket (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Right Front (WDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK | -- | Ground
2 | 0.5 PU | -- | Right Park Lamp Voltage

### Marker Lamp - Right Front (X88)

#### Connector Part Information

- OEM: 6341
- Service: See Catalog
- Description: 2-Way F Lamp Socket (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Right Front (X88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 RD | -- | Right Park Lamp Voltage
B | 0.8 BK | -- | Ground

### Marker Lamp - Right Rear (W49)

#### Connector Part Information

- OEM: 7712-5354-4WB
- Service: See Catalog
- Description: 2-Way F Lamp Socket, Axial (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Right Rear (W49)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | -- | Left Park Lamp Voltage
B | 0.5 BK | -- | Ground

### Marker Lamp - Right Rear (WDA)

#### Connector Part Information

- OEM: 12146418
- Service: See Catalog
- Description: 2-Way F Lamp Socket (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Right Rear (WDA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | -- | Right Park Lamp Voltage
B | 0.8 BK | -- | Ground

### Marker Lamp - Right Rear (X88)

#### Connector Part Information

- OEM: 12110053
- Service: See Catalog
- Description: 2-Way F Lamp Socket (D-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Right Rear (X88)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | -- | Right Park Lamp Voltage
B | 0.8 BK | -- | Ground

### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LLT)

#### Connector Part Information

OEM: 13520906
Service: 19151493
Description: 5-Way F GT 150 Sealed 4.0 (BK)

#### Terminal Part Information

Pins: C
Terminal/Tray: 12191812/19
Core/Insulation Crimp: C/A
Release Tool/Test Probe: 15315247/J-35616-2A (GY)

Terminal/Tray: 12191819/8
Core/Insulation Crimp: Pins A, B, D, E - E/A
Core/Insulation Crimp: Pins C - 2/A
Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LLT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 492 | MAF Sensor Signal
B | 0.5 PK | 439 | Ignition 1 Voltage
C | 0.5 BK/WH | 451 | Ground
D | 0.5 L-BU | 6289 | Induction Air Temperature Sensor Signal
E | 0.5 TN | 2760 | Low Reference

### Memory Seat Adjuster Switch - Driver (AG3)

#### Connector Part Information

OEM: 7282-6560-40
Service: See Catalog
Description: 4-Way M 064 YESC Series (L-GY)

#### Terminal Part Information

Terminal/Tray: 7114-4720-02/14
Core/Insulation Crimp: J/J
Release Tool/Test Probe: 15315247/J-35616-65B (L-BU)

#### Memory Seat Adjuster Switch - Driver (AG3)
Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 OG | 614 | Memory Set Switch Signal
2 | 0.35 GY/BK | 5979 | Memory Seat Switch Exit Signal
3 | 0.35 D-BU/WH | 5978 | Low Reference
4 | 0.35 BN/WH | 6064 | Memory Switch Dimming Control

### Memory Seat Module (MSM) X1 (AG3)

#### Connector Part Information

OEM: 6098-4611
Service: See Catalog
Description: 16-Way F 1.5 Series, Unsealed (BK)

#### Terminal Part Information

Terminal/Tray: 8240-0128/22
Core/Insulation Crimp: C/A
Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Memory Seat Module (MSM) X1 (AG3)
Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 PU | 2424 | Driver Heated Seat Back Element Control
2-3 | -- | -- | Not Used
4 | 0.8 L-BU | 2433 | Passenger Heated Seat Back Element Control
5 | -- | -- | Not Used
6 | 0.8 BN | 2432 | Driver Heated Seat Back Element Voltage (KA1)
0.8 L-GN | 2078 | Heated Seat Cushion Element Control (KB6)
7 | 1 TN | 2110 | Steering Column Telescope Motor Control - Reverse (N38)
8 | 1 OG | 2098 | Steering Column Telescope Motor Forward (N38)
9 | 1 TN | 285 | Driver Seat Horizontal Motor Forward Control
10 | 1 L-GN | 284 | Driver Seat Horizontal Motor Rearward Control
11 | 0.8 L-GN | 2078 | Heated Seat Cushion Element Control (KA1)
0.8 BN | 2432 | Driver Heated Seat Back Element Voltage (KB6)
12 | 1 D-GN | 286 | Driver Seat Front Vertical Motor Up Control
13 | 1 D-BU | 287 | Driver Seat Front Vertical Motor Down Control
14 | 0.8 D-BU | 2479 | Passenger Heated Seat Element Voltage (KA1)
0.8 PK | 2480 | Passenger Heated Seat Cushion Element Control (KB6)
15 | 1 YE | 282 | Driver Seat Rear Vertical Motor Up Control
16 | 1 L-BU | 283 | Driver Seat Rear Vertical Motor Down Control

### Memory Seat Module (MSM) X2 (AG3)

#### Connector Part Information

OEM: 6098-4607
Service: 88988497
Description: 6-Way F 2.8mm PBT (BK)

#### Terminal Part Information

Terminal/Tray: 8100-4443/22
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 15315247/J-35616-35 (VT)

#### Memory Seat Module (MSM) X2 (AG3)

Pin

Wire

Circuit

Function

1

0.35 GY

6206

Low Reference

2

0.35 PK

2426

Low Reference

3

0.35 YE

2080

Low Reference

4

--

--

Not Used

5

0.35 TN

2482

Low Reference

6

0.35 L-BU

5476

Low Reference

### Memory Seat Module X3 (MSM) (AG3)

#### Connector Part Information

OEM: 6098-4606
Service: See Catalog
Description: 6-Way F 2.8 Series (BN)

#### Terminal Part Information

Pins: 3, 6
Terminal/Tray: 8100-4443/22
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 15315247/J-35616-35 (VT)

Pins: 1, 2, 4, 5
Terminal/Tray: 8100-4445/22
Core/Insulation Crimp: Pins 1, 2, 4 - 4/4
Core/Insulation Crimp: Pins 5 - F/D
Release Tool/Test Probe: 15315247/J-35616-35 (VT)

#### Memory Seat Module (MSM) X3 (AG3)

Pin

Wire

Circuit

Function

1

2 BK

550

Ground

2

2 RD/WH

4040

Battery Positive Voltage (N38)

3

0.35 PU/WH

6205

Driver Position Switch High Reference

4

2 BK

550

Ground

5

3 RD/WH

1140

Battery Positive Voltage

6

0.35 RD/WH

3140

Battery Positive Voltage

### Memory Seat Module (MSM) X4 (AG3)

#### Connector Part Information

OEM: 6098-4610
Service: See Catalog
Description: 16-Way F 1.5 Series, Unsealed (GN)

#### Terminal Part Information

Terminal/Tray: 8240-0128/22
Core/Insulation Crimp: C/A
Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Memory Seat Module (MSM) X4 (AG3)

Pin

Wire

Circuit

Function

1-6

--

--

Not Used

7

1 BN

2112

Steering Column Tilt Motor Control - Down (N38)

8

1 PK

2111

Steering Column Tilt Motor Control - Up (N38)

9-11

--

--

Not Used

12

1 D-BU

611

Driver Seat Lumbar Motor Forward Control

13

1 PK

610

Driver Seat Lumbar Motor Rearward Control

14

0.8 PK

2480

Passenger Heated Seat Cushion Element Control (KA1)

0.8 D-BU

2479

Passenger Heated Seat Element Voltage (KB6)

15

1 L-GN

276

Driver Seat Recline Motor Forward Control

16

1 L-BU

277

Driver Seat Recline Motor Rearward Control

### Memory Seat Module (MSM) X5 (AG3)

#### Connector Part Information

OEM: 31410-1200
Service: See Catalog
Description: 20-Way F 0.64 Series (BK)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Memory Seat Module (MSM) X5 (AG3)

Pin

Wire

Circuit

Function

1

0.35 YE/BK

2079

Heated Seat Cushion Temperature Sensor Signal

2

0.35 GY

2434

Passenger Heated Seat Cushion Temperature Sensor Signal

3

0.35 TN

2436

Heated Seat Back Temperature Sensor Signal

4

0.35 D-BU

2425

Driver Heated Seat Back Temperature Sensor Signal

5-8

--

--

Not Used

9

0.35 OG

2153

Steering Column Telescope Sensor Signal (N38)

10

--

--

Not Used

11

0.35 TN

6207

5-Volt Reference

12-13

--

--

Not Used

14

0.35 BN/WH

557

Front Vertical Seat Motor Position Sensor Signal

15

0.35 TN

568

Rear Vertical Seat Motor Position Sensor Signal

16

0.35 D-GN

569

Horizontal Seat Motor Position Sensor Signal

17

0.35 WH/BK

570

Driver Seat Recline Motor Position Sensor Signal

18

--

--

Not Used

19

0.35 YE

1063

Driver Seat Lumbar Horizontal Position Sensor Signal

20

0.35 OG

2154

Steering Column Tilt Sensor Signal (N38)

### Memory Seat Module (MSM) X6 (AG3)

#### Connector Part Information

OEM: 31410-1201
Service: See Catalog
Description: 20-Way F USCAR 0.64 Series (GY)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Memory Seat Module (MSM) X6 (AG3)

Pin

Wire

Circuit

Function

1

--

--

Not Used

2

0.35 GY

5961

Right Heated/Cooled Seat Mode Signal (KB6)

3-5

--

--

Not Used

6

0.35 YE

1065

Driver Seat Lumbar Forward Switch Signal

7

--

--

Not Used

8

0.35 GY

2096

Steering Column Tilt and Telescope Up Switch Signal (N38)

9

0.35 PK

2094

Steering Column Tilt and Telescope Forward Switch Signal (N38)

10

--

--

Not Used

11

0.35 L-BU/WH

181

Left Heated/Cooled Seat Mode Signal (KB6)

12-15

--

--

Not Used

16

0.35 D-BU

1064

Driver Seat Lumbar Rearward Switch Signal

17

--

--

Not Used

18

0.35 YE

2097

Steering Column Tilt and Telescope Down Switch Signal (N38)

19

0.35 OG

2095

Steering Column Tilt and Telescope Reverse Switch Signal (N38)

20

--

--

Not Used

### Memory Seat Module (MSM) X7 (AG3)

#### Connector Part Information

OEM: 31410-1202
Service: See Catalog
Description: 20-Way F 0.64 Series (BK)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Memory Seat Module (MSM) X7 (AG3)

Pin

Wire

Circuit

Function

1-6

--

--

Not Used

7

0.35 D-GN

1518

Power Seat Front Vertical Up Switch Signal

8

0.35 YE

1519

Power Seat Rear Vertical Up Switch Signal

9

0.35 TN

1522

Power Seat Horizontal Forward Switch Signal

10

0.35 GY/BK

1269

Power Seat Recline Forward Switch Signal

11-15

--

--

Not Used

16

0.35 D-GN

5060

Low Speed GMLAN Serial Data

17

0.35 D-BU

1520

Power Seat Front Vertical Down Switch Signal

18

0.35 L-BU

1521

Power Seat Rear Vertical Down Switch Signal

19

0.35 L-GN

1523

Power Seat Horizontal Rearward Switch Signal

20

0.35 D-GN/WH

1270

Power Seat Recline Rearward Switch Signal

### Mode Actuator

#### Connector Part Information

OEM: 12064993
Service: 12102485
Description: 6-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12146447/3
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Mode Actuator

Pin

Wire

Circuit

Function

5

0.35 TN

2273

Mode Door Control

6

0.35 TN/BK

119

Mode Door Control

7

--

--

Not Used

8

0.35 YE

1791

Low Reference

9

0.35 L-GN

2275

Mode Door Position Signal

10

0.35 GY

598

5-Volt Reference

### Mode Actuator - Auxiliary

#### Connector Part Information

OEM: 12064993
Service: 12102485
Description: 6-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12146447/3
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Mode Actuator - Auxiliary

Pin

Wire

Circuit

Function

5

0.35 OG

2215

Auxiliary Mode Door Control

6

0.35 L-GN/WH

5729

Auxiliary Mode Motor Voltage

7

--

--

Not Used

8

0.35 GY/BK

1798

Low Reference

9

0.35 GY

2599

Auxiliary Mode Door Control

10

0.35 GY

596

5-Volt Reference

### Object Alarm Module X1 (UD7)

#### Connector Part Information

OEM: 89047364
Service: See Catalog
Description: 12-Way F Unsealed (BK)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Object Alarm Module X1 (UD7)

Pin

Wire

Circuit

Function

1

0.35 RD/WH

3140

Battery Positive Voltage

2

0.35 WH

2370

Telltale Assembly Voltage

3

--

--

Not Used

4

0.35 OG

2371

Left Amber Indicator Control

5

--

--

Not Used

6

0.35 D-GN

5060

Low Speed GMLAN Serial Data

7

0.35 BK

650

Ground

8

--

--

Not Used

9

0.35 D-BU

2372

Center Amber Indicator Control

10

0.35 GY

2373

Red Indicator Control

11-12

--

--

Not Used

### Object Alarm Module X2 (UD7)

#### Connector Part Information

OEM: 89047354
Service: 19115653
Description: 8-Way F Unsealed (GY)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Object Alarm Module X2 (UD7)

Pin

Wire

Circuit

Function

1

0.35 PU

2378

Right Rear Corner Object Sensor Signal

2

0.35 D-GN

2377

Right Rear Middle Object Sensor Signal

3

0.35 OG

2376

Left Rear Middle Object Sensor Signal

4

0.35 D-BU

2374

Object Sensor Voltage

5

0.35 YE

2375

Left Rear Corner Object Sensor Signal

6-7

--

--

Not Used

8

0.35 GY

2379

Low Reference

### Object Alarm Sensor - Left Rear Corner (UD7)

#### Connector Part Information

OEM: 31404-3700
Service: 88988337
Description: 3-Way F MX64 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Object Alarm Sensor - Left Rear Corner (UD7)

Pin

Wire

Circuit

Function

1

0.35 D-BU

2374

Object Sensor Voltage

2

0.35 GY

2379

Low Reference

3

0.35 YE

2375

Left Rear Corner Object Sensor Signal

### Object Alarm Sensor - Left Rear Middle (UD7)

#### Connector Part Information

OEM: 31404-3700
Service: 88988337
Description: 3-Way F MX64 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Object Alarm Sensor - Left Rear Middle (UD7)

Pin

Wire

Circuit

Function

1

0.35 D-BU

2374

Object Sensor Voltage

2

0.35 GY

2379

Low Reference

3

0.35 OG

2376

Left Rear Middle Object Sensor Signal

### Object Alarm Sensor - Right Rear Corner (UD7)

#### Connector Part Information

OEM: 31404-3700
Service: 88988337
Description: 3-Way F MX64 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Object Alarm Sensor - Right Rear Corner (UD7)

Pin

Wire

Circuit

Function

1

0.35 D-BU

2374

Object Sensor Voltage

2

0.35 GY

2379

Low Reference

3

0.35 PU

2378

Right Rear Corner Object Sensor Signal

### Object Alarm Sensor - Right Rear Middle (UD7)

#### Connector Part Information

OEM: 31404-3700
Service: 88988337
Description: 3-Way F MX64 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Object Alarm Sensor - Right Rear Middle (UD7)

Pin

Wire

Circuit

Function

1

0.35 D-BU

2374

Object Sensor Voltage

2

0.35 GY

2379

Low Reference

3

0.35 D-GN

2377

Right Rear Middle Object Sensor Signal

### Output Speed Sensor (OSS)

#### Connector Part Information

OEM: 15473844
Service: Non-Serviceable
Description: 2-Way F M/P 150.2 Series P2S (L-GN)

#### Terminal Part Information

Terminal/Tray: Non-Serviceable
Core/Insulation Crimp: Non-Serviceable
Release Tool/Test Probe: Non-Serviceable

#### Output Speed Sensor (OSS)

Pin

Wire

Circuit

Function

A

0.5 WH

--

OSS High Signal

B

0.5 BK

--

OSS Low Signal

### Outside Rearview Mirror - Driver (DL6 or DS3)

#### Connector Part Information

OEM: 7282-6455-40
Service: 88988272
Description: 10-Way M Kaizen YESC Series (L-GY)

#### Terminal Part Information

Terminal/Tray: 7114-4100-08/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### Outside Rearview Mirror - Driver (DL6 or DS3)

Pin

Wire

Circuit

Function

1

0.35 L-GN

89

Left Mirror Motor Down Control

2

0.35 WH

81

Driver Mirror Motor Right Control

3

0.35 BK

550

Ground (DS3 without W49)

0.5 L-GN

627

Ground (W49)

4

--

--

Not Used

5

0.5 L-BU/WH

1314

Left Turn Signal Indicator Lamp Voltage (DS3)

6

0.35 TN

329

Driver Mirror Motor Voltage

7

0.5 OG

2267

Mirror Heating Element Voltage (DS3)

8-9

--

--

Not Used

10

0.35 BK

550

Ground (DS3)

### Outside Rearview Mirror - Driver X1 (DNP or DNT)

#### Connector Part Information

OEM: 7282-6455-40
Service: 88988272
Description: 10-Way M Kaizen YESC Series (L-GY)

#### Terminal Part Information

Terminal/Tray: 7114-4100-08/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### Outside Rearview Mirror - Driver X1 (DNP or DNT)

Pin

Wire

Circuit

Function

1

0.35 YE

6802

Left Extend/Fold Mirror Motor Extend Control

2

0.35 L-BU

6803

Left Extend Mirror Motor Retract/Unfold Control

3

--

--

Not Used

4

0.35 D-GN

784

Driver Mirror Vertical Position Sensor Signal

5

0.35 GY

786

Driver Mirror Horizontal Position Sensor Signal

6

--

--

Not Used

7

0.35 D-BU

672

5-Volt Reference

8

0.35 PK

5853

Driver Side Object Detection LED Signal (UFT)

9

0.35 PK/BK

5855

Low Reference (UFT)

10

0.35 BN

673

Low Reference

### Outside Rearview Mirror - Driver X2 (DNP or DNT)

#### Connector Part Information

OEM: 7282-5683-60
Service: See Catalog
Description: 10-Way M YESC/USCAR Class III Series, Sealed (GN)

#### Terminal Part Information

Terminal/Tray: 7114-4100-08/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### Outside Rearview Mirror - Driver X2 (DNP or DNT)

Pin

Wire

Circuit

Function

1

0.35 D-BU/WH

6160

Left Mirror Vertical Position Control

2

0.35 D-GN/WH

6159

Left Mirror Horizontal Position Control

3

0.5 L-GN

627

Low Reference

4

0.35 PK

1691

Low Reference (DNP)

5

0.5 L-BU/WH

1314

Left Turn Signal Indicator Lamp Voltage

6

0.35 WH

7197

Left Mirror Drive Motor Common

7

0.5 OG

2267

Mirror Heating Element Voltage

8

--

--

Not Used

9

0.35 GY

1690

Automatic Day/Night Mirror Signal (DNP)

10

0.35 BK

550

Ground

### Outside Rearview Mirror - Passenger (DL6 or DS3)

#### Connector Part Information

OEM: 7282-6455-40
Service: 88988272
Description: 10-Way M Kaizen YESC Series (L-GY)

#### Terminal Part Information

Terminal/Tray: 7114-4100-08/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### Outside Rearview Mirror - Passenger (DL6 or DS3)

Pin

Wire

Circuit

Function

1

0.35 PU/WH

889

Passenger Mirror Motor Down Control

2

0.35 OG/WH

881

Passenger Mirror Motor Right Control

3

0.35 BK

750

Ground (DS3 without W49)

0.5 D-GN

628

Ground (W49)

4

--

--

Not Used

5

0.5 D-BU/WH

1315

Right Turn Signal Indicator Lamp Voltage (DS3)

6

0.35 TN/WH

330

Passenger Mirror Motor Voltage

7

0.5 OG

2267

Mirror Heating Element Voltage (DS3)

8-9

--

--

Not Used

10

0.35 BK

750

Ground (DS3)

### Outside Rearview Mirror - Passenger X1 (DNP or DNT)

#### Connector Part Information

OEM: 7282-6455-40
Service: 88988272
Description: 10-Way M Kaizen YESC Series (L-GY)

#### Terminal Part Information

Terminal/Tray: 7114-4100-08/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### Outside Rearview Mirror - Passenger X1 (DNP or DNT)

Pin

Wire

Circuit

Function

1

0.35 YE

6804

Driver Mirror Motor Down Control

2

0.35 L-BU

6805

Right Extend Motor Retract/Unfold Control

3

--

--

Not Used

4

0.35 BN

787

Passenger Mirror Vertical Position Sensor Signal

5

0.35 L-BU/BK

785

Passenger Mirror Horizontal Position Sensor Signal

6

--

--

Not Used

7

0.35 YE

674

5-Volt Reference

8

0.35 PK

5861

Passenger Side Object Detection LED Signal (UFT)

9

0.35 PK/BK

5862

Low Reference (UFT)

10

0.35 L-GN

675

Low Reference

### Outside Rearview Mirror - Passenger X2 (DNP or DNT)

#### Connector Part Information

OEM: 7282-5683-60
Service: See Catalog
Description: 10-Way M YESC/USCAR Class III Series, Sealed (GN)

#### Terminal Part Information

Terminal/Tray: 7114-4100-08/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### Outside Rearview Mirror - Passenger X2 (DNP or DNT)

Pin

Wire

Circuit

Function

1

0.35 OG/BK

6162

Outside Right Mirror Right Front Up Control

2

0.35 GY/BK

6161

Right Mirror Horizontal Position Control

3

0.5 D-GN

628

Low Reference

4

--

--

Not Used

5

0.5 D-BU/WH

1315

Right Turn Signal Indicator Lamp Voltage

6

0.35 WH

7196

Right Mirror Drive Motor Common

7

0.5 OG

2267

Mirror Heating Element Voltage

8-9

--

--

Not Used

10

0.35 BK

750

Ground

### Outside Rearview Mirror Switch (DL6 or DS3)

#### Connector Part Information

OEM: 12064769
Service: 12101762
Description: 10-Way F Metri-Pack 150 Series (NA)

#### Terminal Part Information

Terminal/Tray: 12064971/5
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Outside Rearview Mirror Switch (DL6 or DS3)

Pin

Wire

Circuit

Function

A

--

--

Not Used

B

0.5 RD/WH

1940

Battery Positive Voltage

C

0.35 TN/WH

330

Passenger Mirror Motor Voltage

D

0.35 OG/WH

881

Passenger Mirror Motor Right Control

E

0.35 GY

8

Instrument Panel Lamp Voltage

F

0.35 PU/WH

889

Passenger Mirror Motor Down Control

G

0.35 BK

550

Ground

H

0.35 TN

329

Driver Mirror Motor Voltage

J

0.35 WH

81

Driver Mirror Motor Right Control

K

0.35 L-GN

89

Driver Mirror Motor Down Control

### Overhead Console Courtesy/Reading Lamps - Front

#### Connector Part Information

OEM: 12047781
Service: 12101864
Description: 3-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

Pins: A, C
Terminal/Tray: 12047767/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

Pins: B
Terminal/Tray: 12064971/5
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Overhead Console Courtesy/Reading Lamps - Front

Pin

Wire

Circuit

Function

A

0.8 OG

1732

Courtesy Lamps Voltage

B

0.5 BK

850

Ground

C

0.8 GY/BK

690

Courtesy Lamp High Control

### Overhead Console Courtesy/Reading Lamps - Rear

#### Connector Part Information

OEM: 12047781
Service: 12101864
Description: 3-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12064971/5
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Overhead Console Courtesy/Reading Lamps - Rear

Pin

Wire

Circuit

Function

A

0.5 OG

1732

Courtesy Lamps Voltage

B

0.5 BK

850

Ground

C

0.5 GY/BK

690

Courtesy Lamp High Control

### Park Brake Switch

#### Connector Part Information

OEM: 12004267
Service: 12102561
Description: 1-Way F 56 Series Lock Type (BK)

#### Terminal Part Information

Terminal/Tray: 12124515/1
Core/Insulation Crimp: C/D
Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Park Brake Switch

Pin

Wire

Circuit

Function

A

0.5 OG/BK

233

Park Brake Switch Signal

### Park Lamp - Left Rear (W49)

#### Connector Part Information

OEM: 1011101
Service: See Catalog
Description: 2-Way F Lamp Socket, Axial (WH)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Park Lamp - Left Rear (W49)

Pin

Wire

Circuit

Function

A

0.5 BK

--

Ground

0.5 BK

--

Ground

B

0.5 BN

--

Park Lamp Voltage

### Park Lamp - Left Rear (Z88)

#### Connector Part Information

OEM: 104257-1
Service: See Catalog
Description: 2-Way F (BK)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Park Lamp - Left Rear (Z88)

Pin

Wire

Circuit

Function

1

0.5 BK

--

Left Park Lamp Voltage

2

0.5 BK

--

Ground

### Park Lamp - Right Rear (W49)

#### Connector Part Information

OEM: 1011101
Service: See Catalog
Description: 2-Way F Lamp Socket, Axial (WH)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Park Lamp - Right Rear (W49)

Pin

Wire

Circuit

Function

A

0.5 BK

--

Ground

0.5 BK

--

Ground

B

0.5 BN

--

Park Lamp Voltage

### Park Lamp - Right Rear (Z88)

#### Connector Part Information

OEM: 104257-1
Service: See Catalog
Description: 2-Way F (BK)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Park Lamp - Right Rear (Z88)

Pin

Wire

Circuit

Function

1

0.5 BK

--

Right Park Lamp Voltage

2

0.5 BK

--

Ground

### Park/Turn Signal Lamp - Left (X88)

#### Connector Part Information

OEM: 12450004
Service: See Catalog
Description: 3-Way F CIC W3 Socket (L-GY)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Park/Turn Signal Lamp - Left (X88)

Pin

Wire

Circuit

Function

A

0.8 GN

--

Left Turn Voltage

B

0.8 BK

--

Ground

0.8 BK

--

Ground

C

0.8 RD

--

Park Lamps Voltage

0.8 RD

--

Park Lamps Voltage

### Park/Turn Signal Lamp - Right (X88)

#### Connector Part Information

OEM: 12450004
Service: See Catalog
Description: 3-Way F CIC W3 Socket (L-GY)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Park/Turn Signal Lamp - Right (X88)

Pin

Wire

Circuit

Function

A

0.8 GN

--

Right Turn Voltage

B

0.8 BK

--

Ground

0.8 BK

--

Ground

C

0.8 RD

--

Park Lamps Voltage

0.8 RD

--

Park Lamps Voltage

### PRNDL Lamp

#### Connector Part Information

OEM: 12162711
Service: See Catalog
Description: 2-Way Lamp Socket Wedge Base W2 (BK)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### PRNDL Lamp

Pin

Wire

Circuit

Function

A

0.35 BU

--

Instrument Panel Lamp Voltage

B

0.35 BU

--

Ground

### Radio X1

#### Connector Part Information

OEM: 7283-9281-30
Service: See Catalog
Description: 14-Way F YESC Kaizen Series (BK)

#### Terminal Part Information

Pins: 1, 8
Terminal/Tray: 12191812/19
Core/Insulation Crimp: C/A
Release Tool/Test Probe: 15315247/J-35616-2A (GY)

Pins: 2-7, 9-11, 13
Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Radio X1

Pin

Wire

Circuit

Function

1

1 RD/WH

4240

Battery Positive Voltage

2

0.5 TN

201

Left Front Speaker Output (+) (UQF)

0.5 TN

511

Left Front Low Level Audio Signal (+) (UQA or UQS)

3

0.5 L-GN

200

Right Front Speaker Output (+) (UQF)

0.5 L-GN/WH

512

Right Front Low Level Audio Signal (+) (UQA or UQS)

4

0.35 PK

5149

Voice Recognition Audio Signal (UE1 with UZR or U3R)

5

0.35 PK/BK

5152

Low Reference (UE1 with UZR or U3R)

6

0.35 WH

7066

Entertainment Remote Enable Signal

7

0.35 PU/WH

1382

LED Dimming Signal

8

1 BK/WH

351

Ground

9

0.5 GY

118

Left Front Speaker Output (-) (UQF)

0.5 D-GN

1947

Left Front Low Level Audio Signal (-) (UQA or UQS)

10

0.5 D-GN

117

Right Front Speaker Output (-) (UQF)

0.5 L-GN

1948

Right Front Low Level Audio Signal (-) (UQA or UQS)

11

0.35 BARE

1573

Drain Wire (UQA or UQS)

12

--

--

Not Used

13

0.35 D-GN

5060

Low Speed GMLAN Serial Data

14

--

--

Not Used

### Radio X2

#### Connector Part Information

OEM: 7283-9282-30
Service: See Catalog
Description: 16-Way F YESC Kaizen Series (BK)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Radio X2

Pin

Wire

Circuit

Function

1

0.5 BN/WH

367

Left Audio Signal (+) (U2K or UBS)

2

0.5 D-GN/WH

368

Right Audio Signal (+) (U2K or UBS)

3

0.35 BARE

1574

Drain Wire (UQA or UQS)

4

--

--

Not Used

5

0.35 BN/WH

599

Left Rear Low Level Audio Signal (+) (without UQF without UK6)

0.35 BN

199

Left Rear Speaker Output (+) (UQF without UK6)

6

0.35 D-BU

46

Right Rear Speaker Output (+) (UQF without UK6)

0.35 D-BU

546

Right Rear Low Level Audio Signal (+) (without UQF without UK6)

7

0.35 OG/BK

1406

Remote Playback Device Left Audio Signal (UE1)

8

0.35 OG

5748

Radio Audio Mute Signal (without UQF)

9

0.5 TN/WH

372

Left Audio Signal (-) (U2K or UBS)

10

0.5 GY

388

Right Audio Signal (-) (U2K or UBS)

11

0.35 BARE

6131

Drain Wire (U2K or UBS)

12

--

--

Not Used

13

0.35 BN

1999

Left Rear Low Level Audio Signal (-) (UK6 without UQF)

0.35 YE

116

Left Rear Speaker Output (-) (UQF without UK6)

14

0.35 TN

1946

Right Rear Low Level Audio Signal (-) (UK6 without UQF)

0.35 L-BU

115

Right Rear Speaker Output (-) (UQF without UK6)

15

0.35 L-BU

1405

Remote Playback Device Audio Common Signal (UE1)

16

--

--

Not Used

### Radio X3 (U42)

#### Connector Part Information

OEM: 7283-9283-40
Service: See Catalog
Description: 16-Way F YESC Kaizen Series (L-GY)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Radio X3 (U42)

Pin

Wire

Circuit

Function

1

0.35 YE

2059

Auxiliary Audio Left Signal

2

0.35 WH

2058

Auxiliary Audio Right Signal

3

0.35 L-BU

5826

Left DVD Audio Signal (+)

4

0.35 WH

5828

Right DVD Audio Signal (+)

5

0.35 OG/BK

5831

Remote Infrared Signal (+)

6

0.35 PK/BK

5844

Video Bright Control

7

0.35 D-GN

6975

DVD Video Signal (+)

8

0.35 PU

2056

Auxiliary Video High Signal

9

0.35 BARE

5345

Drain Wire

10

0.35 L-GN/BK

5845

Video Module Signal

11

0.35 PU

6979

DVD Audio Common

12

0.35 BARE

6980

DVD Audio Shield

13

0.35 TN/WH

5830

Remote Infrared Signal (-)

14

0.35 BARE

6976

DVD Video Drain Wire

15

0.35 WH/BK

5335

DVD Video Signal (-)

16

0.35 BARE

5346

Drain Wire

### Radio X4 (U3R or UVB or UZR)

#### Connector Part Information

OEM: 7283-9284-80
Service: See Catalog
Description: 16-Way F YESC Kaizen Series (BN)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Radio X4 (U3R or UVB or UZR)

Pin

Wire

Circuit

Function

1-2

--

--

Not Used

3

0.5 D-BU

6760

Center Speaker High

4

0.5 WH

6763

Subwoofer Speaker High

5

0.5 D-GN/WH

817

Vehicle Speed Signal

6

0.35 PK

6972

Camera Signal 2 (+) (UVC)

7

0.35 L-BU

6973

Camera Signal 2 (UVC)

8-10

--

--

Not Used

11

0.5 OG

6761

Center Speaker Low

12

0.5 PK

6762

Subwoofer Speaker Low

13

0.5 BARE

5838

Ground

14-16

--

--

Not Used

### Radio/HVAC Control - Auxiliary X1 (UK6)

#### Connector Part Information

OEM: 15394149
Service: See Catalog
Description: 16-Way F Micro-Pack 064 Series (GY)

#### Terminal Part Information

Terminal/Tray: 15359541/4
Core/Insulation Crimp: M/M
Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Radio/HVAC Control - Auxiliary X1 (UK6)

Pin

Wire

Circuit

Function

1

0.35 OG/BK

5329

Infrared Audio Signal (+) (U42)

2

0.35 BN/WH

5331

Infrared Audio Common Signal (U42)

3

0.35 PU/WH

5330

Right Infrared Audio Signal (U42)

4

0.35 BARE

5332

Infrared Audio Drain Wire (U42)

5

0.5 RD/WH

2340

Battery Positive Voltage

6

0.5 BK/WH

351

Ground

7

0.35 PU/WH

1382

LED Dimming Signal

8-13

--

--

Not Used

14

0.35 PK

5829

Infrared Module Voltage (U42)

15

0.35 D-GN

5060

Low Speed GMLAN Serial Data

16

--

--

Not Used

### Radio/HVAC Control - Auxiliary X2 (UK6)

#### Connector Part Information

OEM: 15394152
Service: 19115676
Description: 16-Way F Micro-Pack 064 Series (BK)

#### Terminal Part Information

Terminal/Tray: 15359541/4
Core/Insulation Crimp: M/M
Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Radio/HVAC Control - Auxiliary X2 (UK6)

Pin

Wire

Circuit

Function

1

0.8 BN/WH

599

Left Rear Low Level Audio Signal (+)

2

0.8 BN

1999

Left Rear Low Level Audio Signal (-)

3

0.8 D-BU

546

Right Rear Low Level Audio Signal (+)

4

0.8 TN

1946

Right Rear Low Level Audio Signal (-)

5

0.35 BARE

1574

Drain Wire

6-8

--

--

Not Used

9

0.8 L-BU

5312

Left Rear Low Level Audio Signal (+)

10

0.8 BN

5314

Left Rear Low Level Audio Signal (-)

11

0.8 L-GN

5313

Right Rear Low Level Audio Signal (+)

12

0.8 TN/WH

5830

Right Rear Low Level Audio Signal (-)

13

0.35 BARE

6759

Audio Drain Wire

14-16

--

--

Not Used

### Rear Differential Clutch Control Module X1 (MH6)

#### Connector Part Information

OEM: 89047383
Service: 89047382
Description: 5-Way F (BK)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Rear Differential Clutch Control Module X1 (MH6)

Pin

Wire

Circuit

Function

1

--

--

Not Used

2

0.5 YE

9999

Transfer Case Fluid Temperature Signal

3

0.5 YE

9997

Transfer Case Actuator Low Control

4

0.5 YE

9998

Low Reference

5

0.5 YE

9996

Transfer Case Actuator High Control

### Rear Differential Clutch Control Module X2 (MH6)

#### Connector Part Information

OEM: 13509360
Service: See Catalog
Description: 10-Way F Kaizen 0.64 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Rear Differential Clutch Control Module X2 (MH6)

Pin

Wire

Circuit

Function

1-2

--

--

Not Used

3

0.5 BK

650

Ground

4

--

--

Not Used

5

0.35 L-BU

5986

Communication Enable

6

0.5 RD/WH

1740

Battery Positive Voltage

7

--

--

Not Used

8

0.35 TN

2501

High Speed GMLAN Serial Data Bus-

9

0.35 TN/BK

2500

High Speed GMLAN Serial Data Bus+

10

--

--

Not Used

### Rear Parking Assist (RPA) Display (UD7)

#### Connector Part Information

OEM: 12045813
Service: 12101889
Description: 4-Way F Metri-Pack 150 Series (CR)

#### Terminal Part Information

Terminal/Tray: 12064971/5
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Rear Parking Assist (RPA) Display (UD7)

Pin

Wire

Circuit

Function

A

0.35 WH

2370

Telltale Assembly Voltage

B

0.35 OG

2371

Left Amber Indicator Control

C

0.35 D-BU

2372

Center Amber Indicator Control

D

0.35 GY

2373

Red Indicator Control

### Rear Seat Audio (RSA) Control (RCA)

#### Connector Part Information

OEM: 31068-1010
Service: See Catalog
Description: 4-Way F HDAC64 SR Housing (BK)

#### Terminal Part Information

Terminal/Tray: 1393364-2/7
Core/Insulation Crimp: K/K
Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Rear Seat Audio (RSA) Control (RCA)

Pin

Wire

Circuit

Function

1

0.35 L-GN

1011

Remote Radio Control Signal

2

0.35 BK

850

Ground

3

0.35 PU/WH

1382

LED Dimming Signal

4

0.35 PU

1375

12-Volt Reference

### Rear Window Defogger Grid X1

#### Connector Part Information

OEM: 12092133
Service: 12167133
Description: 1-Way F Metri-Pack 630 Series Self Lock (BK)

#### Terminal Part Information

Terminal/Tray: 12034110/18
Core/Insulation Crimp: B/G
Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Rear Window Defogger Grid X1

Pin

Wire

Circuit

Function

A

5 PU

293

Rear Defog Element Voltage

### Rear Window Defogger Grid X2

#### Connector Part Information

OEM: 12092133
Service: 12167133
Description: 1-Way F Metri-Pack 630 Series Self Lock (BK)

#### Terminal Part Information

Terminal/Tray: 12034110/18
Core/Insulation Crimp: F/G
Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Rear Window Defogger Grid X2

Pin

Wire

Circuit

Function

A

3 BK

650

Ground

### Rear Window Washer Fluid Pump

#### Connector Part Information

OEM: 12020599
Service: 12102664
Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12077411/2
Core/Insulation Crimp: 2/5
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Rear Window Washer Fluid Pump

Pin

Wire

Circuit

Function

A

0.5 BK

1350

Ground

B

0.8 D-GN

392

Rear Window Washer Pump Control

### Rear Window Wiper Motor (without X88)

#### Connector Part Information

OEM: 12041429
Service: 12167129
Description: 5-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

Pins: A, B
Terminal/Tray: 12066214/2
Core/Insulation Crimp: F/D
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

Pins: C-E
Terminal/Tray: 12034046/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Rear Window Wiper Motor (without X88)

Pin

Wire

Circuit

Function

A

1 RD/WH

3840

Battery Positive Voltage

B

1 BK

650

Ground

C

0.5 L-GN

2270

Rear Window Washer Relay Control

D

0.5 GY

391

Rear Window Wiper Switch Signal

E

0.35 WH

2283

Rear Wiper/Washer Switch Voltage

### Rear Window Wiper Motor (X88)

#### Connector Part Information

OEM: 22715965
Service: See Catalog
Description: 5-Way F GT 280 Series (BK)

#### Terminal Part Information

Pins: A, E
Terminal/Tray: 12066214/2
Core/Insulation Crimp: F/D
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

Pins: C, D
Terminal/Tray: 12034046/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Rear Window Wiper Motor (X88)

Pin

Wire

Circuit

Function

A

1 BK

650

Ground

B

--

--

Not Used

C

0.5 L-GN

2270

Rear Window Washer Relay Control

D

0.5 GY

391

Rear Window Wiper Switch Signal

E

1 RD/WH

3840

Battery Positive Voltage

### Rearview Camera (UVC)

#### Connector Part Information

OEM: 1924212-1
Service: 19169090
Description: 6-Way F 0.64 Series Sealed (GY)

#### Terminal Part Information

Terminal/Tray: SAIT-A03T-M064/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215A/J-35616-64B (L-BU)

#### Rearview Camera (UVC)

Pin

Wire

Circuit

Function

1

0.35 PK

6972

Camera Signal 2 (+)

2

0.35 BARE

6974

Camera Shield

3

0.35 D-BU

38

Backup Lamp Relay Control

4

0.35 L-BU

6973

Low Reference

5

0.35 BK

650

Ground

6

0.35 PK/BK

239

Ignition Voltage

### Recirculation Actuator

#### Connector Part Information

OEM: 12064993
Service: 12102485
Description: 6-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12146447/3
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Recirculation Actuator

Pin

Wire

Circuit

Function

5

0.35 D-GN

1614

Recirculation Door Control B

6

0.35 TN/BK

2274

Recirculation Door Control A

7

--

--

Not Used

8

0.35 YE

1791

Low Reference

9

0.35 PU

1838

Recirculation Door Position Signal

10

0.35 GY

598

5-Volt Reference

### Remote Control Door Lock Receiver (RCDLR)

#### Connector Part Information

OEM: 15462684
Service: 88988745
Description: 4-Way F ILAG5 Series (GN)

#### Terminal Part Information

Terminal/Tray: IL-AG5-C1-5000/20
Core/Insulation Crimp: K/K
Release Tool/Test Probe: J-38125-211/J-35616-64B (L-BU)

#### Remote Control Door Lock Receiver (RCDLR)

Pin

Wire

Circuit

Function

1

0.35 RD/WH

1840

Battery Positive Voltage

2

0.35 D-GN

5060

Low Speed GMLAN Serial Data

3

--

--

Not Used

4

0.35 BK

650

Ground

### Seat Adjuster Switch - Driver (AG1)

#### Connector Part Information

OEM: 19177577
Service: 15306174
Description: 8-Way F GT 280 Series (BK)

#### Terminal Part Information

Terminal/Tray: 15304713/19
Core/Insulation Crimp: Pins A-C, E-H - 4/4
Core/Insulation Crimp: Pins B, D - F/D
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Seat Adjuster Switch - Driver (AG1)

Pin

Wire

Circuit

Function

A

2 D-GN

286

Driver Seat Front Vertical Motor Up Control

B

3 BK

550

Ground (without KA1)

2 BK

550

Ground (KA1)

C

2 TN

285

Driver Seat Horizontal Motor Forward Control

D

3 RD/WH

1140

Battery Positive Voltage

E

2 YE

282

Driver Seat Rear Vertical Motor Up Control

F

2 L-GN

284

Driver Seat Horizontal Motor Rearward Control

G

2 L-BU

283

Driver Seat Rear Vertical Motor Down Control

H

2 D-BU

287

Driver Seat Front Vertical Motor Down Control

### Seat Adjuster Switch - Driver (AG3)

#### Connector Part Information

OEM: 15326931
Service: 15306309
Description: 10-Way F GT 280 Series (BK)

#### Terminal Part Information

Terminal/Tray: 15304711/8
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Seat Adjuster Switch - Driver (AG3)

Pin

Wire

Circuit

Function

A

0.35 D-GN

1518

Power Seat Front Vertical Up Switch Signal

B

--

--

Not Used

C

0.35 L-GN

1523

Power Seat Horizontal Rearward Switch Signal

D

0.35 TN

1522

Power Seat Horizontal Forward Switch Signal

E

0.35 PU/WH

6205

Driver Position Switch High Reference

F

0.35 YE

1519

Power Seat Rear Vertical Up Switch Signal

G

0.35 D-GN/WH

1270

Power Seat Recline Rearward Switch Signal

H

0.35 GY/BK

1269

Power Seat Recline Forward Switch Signal

J

0.35 L-BU

1521

Power Seat Rear Vertical Down Switch Signal

K

0.35 D-BU

1520

Power Seat Front Vertical Down Switch Signal

### Seat Adjuster Switch - Driver (AH5)

#### Connector Part Information

OEM: 15326931
Service: 15306309
Description: 10-Way F GT 280 Series (BK)

#### Terminal Part Information

Pins: A-F, J, K
Terminal/Tray: 15304713/19
Core/Insulation Crimp: Pins A-D, F, J, K - 4/4
Core/Insulation Crimp: Pins E - F/D
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

Pins: G, H
Terminal/Tray: 15304711/8
Core/Insulation Crimp: 2/A
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Seat Adjuster Switch - Driver (AH5)

Pin

Wire

Circuit

Function

A

2 D-GN

286

Driver Seat Front Vertical Motor Up Control

B

2 BK

550

Ground

C

2 L-GN

284

Driver Seat Horizontal Motor Rearward Control

D

2 TN

285

Driver Seat Horizontal Motor Forward Control

E

3 RD/WH

1140

Battery Positive Voltage

F

2 YE

282

Driver Seat Rear Vertical Motor Up Control

G

1 L-BU

277

Driver Seat Recline Motor Rearward Control

H

1 L-GN

276

Driver Seat Recline Motor Forward Control

J

2 L-BU

283

Driver Seat Rear Vertical Motor Down Control

K

2 D-BU

287

Driver Seat Front Vertical Motor Down Control

### Seat Adjuster Switch - Passenger (AAQ)

#### Connector Part Information

OEM: 15326931
Service: 15306309
Description: 10-Way F GT 280 Series (BK)

#### Terminal Part Information

Pins: B-E
Terminal/Tray: 15304713/19
Core/Insulation Crimp: Pins B, E - F/D
Core/Insulation Crimp: Pins C, D - 4/4
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

Pins: G, H
Terminal/Tray: 15304711/8
Core/Insulation Crimp: 2/A
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Seat Adjuster Switch - Passenger (AAQ)

Pin

Wire

Circuit

Function

A

--

--

Not Used

B

3 BK

750

Ground

C

2 L-GN

290

Passenger Seat Horizontal Motor Rearward Control

D

2 TN

296

Passenger Seat Horizontal Motor Forward Control

E

3 RD/WH

3040

Battery Positive Voltage

F

--

--

Not Used

G

1 D-BU

77

Passenger Seat Recline Motor Rearward

H

1 D-GN

76

Passenger Seat Recline Motor Forward

J-K

--

--

Not Used

### Seat Adjuster Switch - Passenger (AG2)

#### Connector Part Information

OEM: 19177577
Service: 15306174
Description: 8-Way F GT 280 Series (BK)

#### Terminal Part Information

Pins: B-D, F
Terminal/Tray: 15304713/19
Core/Insulation Crimp: Pins B, D - F/D
Core/Insulation Crimp: Pins C, F - 4/4
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Seat Adjuster Switch - Passenger (AG2)

Pin

Wire

Circuit

Function

A

--

--

Not Used

B

3 BK

750

Ground

C

2 TN

296

Passenger Seat Horizontal Motor Forward Control

D

3 RD/WH

3040

Battery Positive Voltage

E

--

--

Not Used

F

2 L-GN

290

Passenger Seat Horizontal Motor Rearward Control

G-H

--

--

Not Used

### Seat Back Ventilation Heating and Cooling Module -- Driver (KB6)

#### Connector Part Information

OEM: 12064752
Service: 15305888
Description: 6-Way F Metri-Pack 280 Series, Unsealed (BK)

#### Terminal Part Information

Terminal/Tray: Pins A, C - 12066214/2
Core/Insulation Crimp: A/B
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

Terminal/Tray: Pins B, D, E - 12047581/2
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Seat Back Ventilation Heating and Cooling Module -- Driver (KB6)

Pin

Wire

Circuit

Function

A

2 RD/WH

640

Battery Positive Voltage

B

0.35 L-BU/WH

181

Left Heated/Cooled Seat Mode Signal

C

2 BK

550

Ground

D

0.35 D-BU

2425

Seat Back Temperature Sensor Signal

E

0.35 PK

2426

Low Reference

F

--

--

Not Used

### Seat Back Ventilation Heating and Cooling Module -- Passenger (KB6)

#### Connector Part Information

OEM: 12064752
Service: 15305888
Description: 6-Way F Metri-Pack 280 Series, Unsealed (BK)

#### Terminal Part Information

Terminal/Tray: Pins A, C - 12066214/2
Core/Insulation Crimp: A/B
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

Terminal/Tray: Pins B, D, E - 12047581/2
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Seat Back Ventilation Heating and Cooling Module -- Passenger (KB6)

Pin

Wire

Circuit

Function

A

2 RD/WH

640

Battery Positive Voltage

B

0.35 GY

5961

Right Heated/Cooled Seat Mode Signal

C

2 BK

750

Ground

D

0.35 TN

2436

Seat Back Temperature Sensor Signal

E

0.35 TN

2482

Low Reference

F

--

--

Not Used

### Seat Belt Buckle - Driver

#### Connector Part Information

OEM: 7282-6443-40
Service: See Catalog
Description: 2-Way M 1.5 Series (L-GY)

#### Terminal Part Information

Terminal/Tray: 7114-4100-08/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### Seat Belt Buckle - Driver

Pin

Wire

Circuit

Function

1

0.35 D-GN

5016

Seat Belt Switch - Left - Signal

2

0.35 PK

5057

Low Reference

### Seat Belt Buckle - Passenger

#### Connector Part Information

OEM: 7282-6443-40
Service: See Catalog
Description: 2-Way M 1.5 Series (L-GY)

#### Terminal Part Information

Terminal/Tray: 7114-4100-08/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### Seat Belt Buckle - Passenger

Pin

Wire

Circuit

Function

1

0.35 OG

1362

Seat Belt Switch - Right - Signal

2

0.35 PK

5057

Low Reference

### Seat Belt Buckle Pretensioner - Driver

#### Connector Part Information

OEM: PP10001460
Service Caution: The connector at the Inflatable Restraint Module cannot be disconnected or removed without damage to the module. If the connector is removed from the module, the entire module with harness must be replaced.
Description: 2-Way F Squib 90 (BK)

#### Terminal Part Information

Terminal/Tray: Service With Pigtail
Core/Insulation Crimp: N/A
Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Buckle Pretensioner - Driver

Pin

Wire

Circuit

Function

1

L-GN/RD

--

Seat Belt Buckle Pretensioner - Left - High Control

2

WH/RD

--

Seat Belt Buckle Pretensioner - Left - Low Control

### Seat Belt Buckle Pretensioner - Passenger

#### Connector Part Information

OEM: PP10001460
Service Caution: The connector at the Inflatable Restraint Module cannot be disconnected or removed without damage to the module. If the connector is removed from the module, the entire module with harness must be replaced.
Description: 2-Way F Squib 90 (BK)

#### Terminal Part Information

Terminal/Tray: Service With Pigtail
Core/Insulation Crimp: N/A
Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Buckle Pretensioner - Passenger

Pin

Wire

Circuit

Function

1

L-GN/RD

--

Seat Belt Buckle Pretensioner - Right - High Control

2

WH/RD

--

Seat Belt Buckle Pretensioner - Right - Low Control

### Seat Belt Retractor Pretensioner - Driver

#### Connector Part Information

OEM: PP10001460
Service: See Catalog
Description: 2-Way F Squib 90 (BK)

#### Terminal Part Information

Terminal/Tray: Service With Pigtail
Core/Insulation Crimp: N/A
Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Retractor Pretensioner - Driver

Pin

Wire

Circuit

Function

1

0.5 TN/WH

2118

Seat Belt Retractor Pretensioner - Left - High Control

2

0.5 OG/BK

2119

Seat Belt Retractor Pretensioner - Left - Low Control

### Seat Belt Retractor Pretensioner - Passenger

#### Connector Part Information

OEM: PP10001460
Service: See Catalog
Description: 2-Way F Squib 90 (BK)

#### Terminal Part Information

Terminal/Tray: Service With Pigtail
Core/Insulation Crimp: N/A
Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Retractor Pretensioner - Passenger

Pin

Wire

Circuit

Function

1

0.5 L-GN

2116

Seat Belt Retractor Pretensioner - Right - High Control

2

0.5 OG

2117

Seat Belt Retractor Pretensioner - Right - Low Control

### Seat Cushion Ventilation Heating and Cooling Module -- Driver (KB6)

#### Connector Part Information

OEM: 12064752
Service: 15305888
Description: 6-Way F Metri-Pack 280 Series, Unsealed (BK)

#### Terminal Part Information

Terminal/Tray: Pins A, C - 12066214/2
Core/Insulation Crimp: A/B
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

Terminal/Tray: Pins B, D, E - 12047581/2
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Seat Cushion Ventilation Heating and Cooling Module -- Driver (KB6)

Pin

Wire

Circuit

Function

A

2 RD/WH

640

Battery Positive Voltage

B

0.35 L-BU/WH

181

Left Heated/Cooled Seat Mode Signal

C

2 BK

550

Ground

D

0.35 OG

7018

Seat Cushion Temperature Sensor Signal

E

0.35 OG/WH

7019

Low Reference

F

--

--

Not Used

### Seat Cushion Ventilation Heating and Cooling Module -- Passenger (KB6)

#### Connector Part Information

OEM: 12064752
Service: 15305888
Description: 6-Way F Metri-Pack 280 Series, Unsealed (BK)

#### Terminal Part Information

Terminal/Tray: Pins A, C - 12066214/2
Core/Insulation Crimp: A/B
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

Terminal/Tray: Pins B, D, E - 12047581/2
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Seat Cushion Ventilation Heating and Cooling Module -- Passenger (KB6)

Pin

Wire

Circuit

Function

A

2 RD/WH

640

Battery Positive Voltage

B

0.35 GY

5961

Right Heated/Cooled Seat Mode Signal

C

2 BK

750

Ground

D

0.35 D-BU

5475

Seat Cushion Temperature Sensor Signal

E

0.35 PK

2435

Low Reference

F

--

--

Not Used

### Seat Front Vertical Motor - Driver (AG1 or AG3 or AH5)

#### Connector Part Information

OEM: 623346-1
Service: See Catalog
Description: 2-Way F (GY)

#### Terminal Part Information

Terminal/Tray: 4-965999-1/25
Core/Insulation Crimp: 4/A
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Seat Front Vertical Motor - Driver (AG1 or AG3 or AH5)

Pin

Wire

Circuit

Function

1

2 D-GN

286

Driver Seat Front Vertical Motor Up Control (AG1 or AH5)

1 D-GN

286

Driver Seat Front Vertical Motor Up Control (AG3)

2

2 D-BU

287

Driver Seat Front Vertical Motor Down Control (AG1 or AH5)

1 D-BU

287

Driver Seat Front Vertical Motor Down Control (AG3)

### Seat Front Vertical Motor Position Sensor - Driver (AG3)

#### Connector Part Information

OEM: 39-01-4030
Service: See Catalog
Description: 3-Way F Mini-Fit Series (NA)

#### Terminal Part Information

Terminal/Tray: 39-00-0059/28
Core/Insulation Crimp: K/K
Release Tool/Test Probe: J-38125-560/J-35616-12 (BU)

#### Seat Front Vertical Motor Position Sensor - Driver (AG3)

Pin

Wire

Circuit

Function

1

0.35 TN

6207

5-Volt Reference

2

0.35 BN/WH

557

Front Vertical Seat Motor Position Sensor Signal

3

0.35 GY

6206

Low Reference

### Seat Horizontal Motor - Driver (AG1 or AG3 or AH5)

#### Connector Part Information

OEM: 623346-1
Service: See Catalog
Description: 2-Way F (GY)

#### Terminal Part Information

Terminal/Tray: 4-965999-1/25
Core/Insulation Crimp: 4/A
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Seat Horizontal Motor - Driver (AG1 or AG3 or AH5)

Pin

Wire

Circuit

Function

1

2 TN

285

Driver Seat Horizontal Motor Forward Control (AG1 or AH5)

1 TN

285

Driver Seat Horizontal Motor Forward Control (AG3)

2

2 L-GN

284

Driver Seat Horizontal Motor Rearward Control (AG1 or AH5)

1 L-GN

284

Driver Seat Horizontal Motor Rearward Control (AG3)

### Seat Horizontal Motor - Passenger (AAQ or AG2)

#### Connector Part Information

OEM: 623346-1
Service: See Catalog
Description: 2-Way F (GY)

#### Terminal Part Information

Terminal/Tray: 4-965999-1/25
Core/Insulation Crimp: 4/A
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Seat Horizontal Motor - Passenger (AAQ or AG2)

Pin

Wire

Circuit

Function

1

2 TN

296

Passenger Seat Horizontal Motor Forward Control

2

2 L-GN

290

Passenger Seat Horizontal Motor Rearward Control

### Seat Horizontal Motor Position Sensor - Driver (AG3)

#### Connector Part Information

OEM: 39-01-4030
Service: See Catalog
Description: 3-Way F Mini-Fit Series (NA)

#### Terminal Part Information

Terminal/Tray: 39-00-0059/28
Core/Insulation Crimp: K/K
Release Tool/Test Probe: J-38125-560/J-35616-12 (BU)

#### Seat Horizontal Motor Position Sensor - Driver (AG3)

Pin

Wire

Circuit

Function

1

0.35 TN

6207

5-Volt Reference

2

0.35 D-GN

569

Horizontal Seat Motor Position Sensor Signal

3

0.35 GY

6206

Low Reference

### Seat Lumbar Horizontal Motor - Driver (AG3 or AH5)

#### Connector Part Information

OEM: 12020556
Service: 12101820
Description: 2-Way F Metri-Pack 480 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12084595/2
Core/Insulation Crimp: F/G
Release Tool/Test Probe: 12094430/J-35616-40 (BU)

#### Seat Lumbar Horizontal Motor - Driver (AG3 or AH5)

Pin

Wire

Circuit

Function

A

2 PK

610

Driver Seat Lumbar Motor Rearward Control

B

2 D-BU

611

Driver Seat Lumbar Motor Forward Control

### Seat Lumbar Horizontal Motor - Passenger (AAQ)

#### Connector Part Information

OEM: 12020556
Service: 12101820
Description: 2-Way F Metri-Pack 480 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12084595/2
Core/Insulation Crimp: F/G
Release Tool/Test Probe: 12094430/J-35616-40 (BU)

#### Seat Lumbar Horizontal Motor - Passenger (AAQ)

Pin

Wire

Circuit

Function

A

2 WH

210

Passenger Seat Lumbar Motor Rearward Control

B

2 D-BU

211

Passenger Seat Lumbar Motor Forward Control

### Seat Lumbar Switch - Driver (AG3 or AH5)

#### Connector Part Information

OEM: 12052854
Service: 88953358
Description: 7-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12015858/4
Core/Insulation Crimp: F/G
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Seat Lumbar Switch - Driver (AG3 or AH5)

Pin

Wire

Circuit

Function

A

2 D-BU

611

Driver Seat Lumbar Motor Forward Control

B-D

--

--

Not Used

E

3 BK

550

Ground

F

2 PK

610

Driver Seat Lumbar Motor Rearward Control

G

3 RD/WH

1140

Battery Positive Voltage

### Seat Lumbar Switch - Passenger (AAQ)

#### Connector Part Information

OEM: 12052854
Service: 88953358
Description: 7-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12015858/4
Core/Insulation Crimp: F/G
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Seat Lumbar Switch - Passenger (AAQ)

Pin

Wire

Circuit

Function

A

2 D-BU

211

Passenger Seat Lumbar Motor Forward Control

B-D

--

--

Not Used

E

3 BK

750

Ground

F

2 WH

210

Passenger Seat Lumbar Motor Rearward Control

G

3 RD/WH

3040

Battery Positive Voltage

### Seat Rear Vertical Motor - Driver (AG1 or AG3 or AH5)

#### Connector Part Information

OEM: 623346-1
Service: See Catalog
Description: 2-Way F (GY)

#### Terminal Part Information

Terminal/Tray: 4-965999-1/25
Core/Insulation Crimp: 4/A
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Seat Rear Vertical Motor - Driver (AG1 or AG3 or AH5)

Pin

Wire

Circuit

Function

1

2 YE

282

Driver Seat Rear Vertical Motor Up Control (AG1 or AH5)

1 YE

282

Driver Seat Rear Vertical Motor Up Control (AG3)

2

2 L-BU

283

Driver Seat Rear Vertical Motor Down Control (AG1 or AH5)

1 L-BU

283

Driver Seat Rear Vertical Motor Down Control (AG3)

### Seat Rear Vertical Motor Position Sensor - Driver (AG3)

#### Connector Part Information

OEM: 39-01-4030
Service: See Catalog
Description: 3-Way F Mini-Fit Series (NA)

#### Terminal Part Information

Terminal/Tray: 39-00-0059/28
Core/Insulation Crimp: K/K
Release Tool/Test Probe: J-38125-560/J-35616-12 (BU)

#### Seat Rear Vertical Motor Position Sensor - Driver (AG3)

Pin

Wire

Circuit

Function

1

0.35 TN

6207

5-Volt Reference

2

0.35 TN

568

Rear Vertical Seat Motor Position Sensor Signal

3

0.35 GY

6206

Low Reference

### Seat Recline Motor - Driver (AG3 or AH5)

#### Connector Part Information

OEM: 1326490-3
Service: See Catalog
Description: 4-Way F JR-POWER MICRO III (GY)

#### Terminal Part Information

Terminal/Tray: 4-965999-1/25
Core/Insulation Crimp: C/A
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Seat Recline Motor - Driver (AG3 or AH5)

Pin

Wire

Circuit

Function

1

1 L-BU

277

Driver Seat Recline Motor Rearward Control

2

1 L-GN

276

Driver Seat Recline Motor Forward Control

3-4

--

--

Not Used

### Seat Recline Motor - Passenger (AAQ)

#### Connector Part Information

OEM: 1326490-3
Service: See Catalog
Description: 4-Way F JR-POWER MICRO III (GY)

#### Terminal Part Information

Terminal/Tray: 4-965999-1/25
Core/Insulation Crimp: C/A
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Seat Recline Motor - Passenger (AAQ)

Pin

Wire

Circuit

Function

1

1 D-BU

77

Passenger Seat Recline Motor Rearward

2

1 D-GN

76

Passenger Seat Recline Motor Forward

3-4

--

--

Not Used

### Seat Recline Position Sensor - Driver (AG3)

#### Connector Part Information

OEM: 39-01-4030
Service: See Catalog
Description: 3-Way F Mini-Fit Series (NA)

#### Terminal Part Information

Terminal/Tray: 39-00-0059/28
Core/Insulation Crimp: K/K
Release Tool/Test Probe: J-38125-560/J-35616-12 (BU)

#### Seat Recline Position Sensor - Driver (AG3)

Pin

Wire

Circuit

Function

1

0.35 TN

6207

5-Volt Reference

2

0.35 WH/BK

570

Driver Seat Recline Motor Position Sensor Signal

3

0.35 GY

6206

Low Reference

### Speaker - Center I/P (UQA or UQS)

#### Connector Part Information

OEM: 12064869
Service: 12117323
Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

Terminal/Tray: 12064971/5
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Center I/P (UQA or UQS)

Pin

Wire

Circuit

Function

A

0.35 L-BU

1960

Front Center Speaker Output (-)

B

0.35 YE

1860

Front Center Speaker Output (+)

### Speaker - Left Front (UQA or UQS)

#### Connector Part Information

OEM: 12064869
Service: 12117323
Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

Terminal/Tray: 12047767/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Left Front (UQA or UQS)

Pin

Wire

Circuit

Function

A

0.8 GY

118

Left Front Speaker Output (-)

B

0.8 TN

201

Left Front Speaker Output (+)

### Speaker - Left Front (UQF)

#### Connector Part Information

OEM: 12064867
Service: 88987981
Description: 2-Way F Metri-Pack 150 Series (NA)

#### Terminal Part Information

Terminal/Tray: 12047767/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Left Front (UQF)

Pin

Wire

Circuit

Function

A

0.8 GY

118

Left Front Speaker Output (-)

B

0.8 TN

201

Left Front Speaker Output (+)

### Speaker - Left Front Tweeter

#### Connector Part Information

OEM: 12052833
Service: 12117275
Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12047581/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Speaker - Left Front Tweeter

Pin

Wire

Circuit

Function

A

0.8 GY

118

Left Front Speaker Output (-)

B

0.8 TN

201

Left Front Speaker Output (+)

### Speaker - Left Rear (UQA or UQS without W49)

#### Connector Part Information

OEM: 12064869
Service: 12117323
Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

Terminal/Tray: 12047767/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Left Rear (UQA or UQS without W49)

Pin

Wire

Circuit

Function

A

0.8 YE

116

Left Rear Speaker Output (-)

B

0.8 BN

199

Left Rear Speaker Output (+)

### Speaker - Left Rear (UQA or UQS with W49)

#### Connector Part Information

OEM: R63461-002
Service: 19168540
Description: 2-Way F GT150 Series (L-GY)

#### Terminal Part Information

Terminal/Tray: 15326030/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Left Rear (UQA or UQS with W49)

Pin

Wire

Circuit

Function

1

0.8 YE

116

Left Rear Speaker Output (-)

2

0.8 BN

199

Left Rear Speaker Output (+)

### Speaker - Left Rear (UQF)

#### Connector Part Information

OEM: 12064867
Service: 88987981
Description: 2-Way F Metri-Pack 150 Series (NA)

#### Terminal Part Information

Terminal/Tray: 12047767/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Left Rear (UQF)

Pin

Wire

Circuit

Function

A

0.8 YE

116

Left Rear Speaker Output (-)

B

0.8 BN

199

Left Rear Speaker Output (+)

### Speaker - Left Rear Compartment (UQA or UQS)

#### Connector Part Information

OEM: 12064869
Service: 12117323
Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

Terminal/Tray: 12064971/5
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Left Rear Compartment (UQA or UQS)

Pin

Wire

Circuit

Function

A

0.5 WH

1959

Left Rear Midrange Speaker Output (-)

B

0.5 TN

1859

Left Rear Midrange Speaker Output (+)

### Speaker - Right Front (UQA or UQS)

#### Connector Part Information

OEM: 12064869
Service: 12117323
Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

Terminal/Tray: 12047767/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Right Front (UQA or UQS)

Pin

Wire

Circuit

Function

A

0.8 D-GN

117

Right Front Speaker Output (-)

B

0.8 L-GN

200

Right Front Speaker Output (+)

### Speaker - Right Front (UQF)

#### Connector Part Information

OEM: 12064867
Service: 88987981
Description: 2-Way F Metri-Pack 150 Series (NA)

#### Terminal Part Information

Terminal/Tray: 12047767/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Right Front (UQF)

Pin

Wire

Circuit

Function

A

0.8 D-GN

117

Right Front Speaker Output (-)

B

0.8 L-GN

200

Right Front Speaker Output (+)

### Speaker - Right Front Tweeter

#### Connector Part Information

OEM: 12052833
Service: 12117275
Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12047581/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Speaker - Right Front Tweeter

Pin

Wire

Circuit

Function

A

0.8 D-GN

117

Right Front Speaker Output (-)

B

0.8 L-GN

200

Right Front Speaker Output (+)

### Speaker - Right Rear (UQA or UQS without W49)

#### Connector Part Information

OEM: 12064869
Service: 12117323
Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

Terminal/Tray: 12047767/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Right Rear (UQA or UQS without W49)

Pin

Wire

Circuit

Function

A

0.8 L-BU

115

Right Rear Speaker Output (-)

B

0.8 D-BU

46

Right Rear Speaker Output (+)

### Speaker - Right Rear (UQA or UQS with W49)

#### Connector Part Information

OEM: R63461-002
Service: 19168540
Description: 2-Way F GT150 Series (L-GY)

#### Terminal Part Information

Terminal/Tray: 15326030/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Right Rear (UQA or UQS with W49)

Pin

Wire

Circuit

Function

1

0.8 L-BU

115

Right Rear Speaker Output (-)

2

0.8 D-BU

46

Right Rear Speaker Output (+)

### Speaker - Right Rear (UQF)

#### Connector Part Information

OEM: 12064867
Service: 88987981
Description: 2-Way F Metri-Pack 150 Series (NA)

#### Terminal Part Information

Terminal/Tray: 12047767/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Right Rear (UQF)

Pin

Wire

Circuit

Function

A

0.8 L-BU

115

Right Rear Speaker Output (-)

B

0.8 D-BU

46

Right Rear Speaker Output (+)

### Speaker - Right Rear Compartment (UQA or UQS)

#### Connector Part Information

OEM: 12064869
Service: 12117323
Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

Terminal/Tray: 12047767/2
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Speaker - Right Rear Compartment (UQA or UQS)

Pin

Wire

Circuit

Function

A

0.8 WH

1959

Right Rear Midrange Speaker Output (-)

B

0.8 TN

1859

Right Rear Midrange Speaker Output (+)

### Speaker - Subwoofer (UQA or UQS)

#### Connector Part Information

OEM: 12052832
Service: 12101825
Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - Subwoofer (UQA or UQS)

Pin

Wire

Circuit

Function

A

1 L-GN/BK

1794

Subwoofer Speaker Output (-)

B

1 D-BU/WH

346

Subwoofer Speaker Output (+)

### Starter Motor X1 (LLT)

#### Connector Part Information

OEM: 13651088
Core/Insulation Crimp: N/A
Description: Ring Terminal

#### Starter Motor X1 (LLT)

Pin

Wire

Circuit

Function

A

32 RD

1

Battery Positive Voltage

### Starter Motor X2 (LLT)

#### Connector Part Information

OEM: 12089916
Service: 12101763
Description: 1-Way F Metri-Pack 280 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 12129493/2
Core/Insulation Crimp: 4/5
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Starter Motor X2 (LLT)

Pin

Wire

Circuit

Function

A

3 PU

6

Starter Solenoid Crank Voltage

### Steering Column Tilt/Telescope Actuator X1 (N38)

#### Connector Part Information

OEM: 19177542
Service: 88988300
Description: 4-Way F GT 280 Series (BK)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Steering Column Tilt/Telescope Actuator X1 (N38)

Pin

Wire

Circuit

Function

A

1 BN

2112

Steering Column Tilt Motor Control - Down

B

1 PK

2111

Steering Column Tilt Motor Control - Up

C

1 OG

2098

Steering Column Telescope Motor Forward

D

1 TN

2110

Steering Column Telescope Motor Rearward

### Steering Column Tilt/Telescope Actuator X2 (N38)

#### Connector Part Information

OEM: 19177540
Service: 15306414
Description: 4-Way F GT 150 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12191812/19
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Steering Column Tilt/Telescope Actuator X2 (N38)

Pin

Wire

Circuit

Function

A

0.35 OG

2154

Steering Column Tilt Sensor Signal

B

0.35 GY

6206

Low Reference

C

0.35 TN

6207

5-Volt Reference

D

0.35 OG

2153

Steering Column Telescope Sensor Signal

### Steering Wheel Control Switch - Left

#### Connector Part Information

OEM: 30700-1100
Service: See Catalog
Description: 10-Way F 0.64 Series (GY)

#### Terminal Part Information

Terminal/Tray: 1393364-2/7
Core/Insulation Crimp: K/K
Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Steering Wheel Control Switch - Left

Pin

Wire

Circuit

Function

1

0.35 PU

1375

12-Volt Reference

2

--

--

Not Used

3

0.35 GY

1884

Cruise Control Switch Signal

4-5

--

--

Not Used

6

0.35 PU/WH

7005

LED Dimming Signal

7

--

--

Not Used

8

0.35 BK/WH

1551

Ground

9

0.35 GN/WH

7158

Cruise Control Indicator Dimming Signal

10

--

--

Not Used

### Steering Wheel Control Switch - Right (UK3)

#### Connector Part Information

OEM: 31068-1010
Service: See Catalog
Description: 4-Way F HDAC64 SR Housing Series (BK)

#### Terminal Part Information

Terminal/Tray: 1393364-2/7
Core/Insulation Crimp: K/K
Release Tool/Test Probe: 15315247/J-35616-64B (L-BU)

#### Steering Wheel Control Switch - Right (UK3)

Pin

Wire

Circuit

Function

1

0.35 BK/WH

1551

Ground

2

0.35 PU/WH

7005

LED Dimming Signal

3

0.35 PU

1375

12-Volt Reference

4

0.35 D-BU

1796

Steering Wheel Controls Signal

### Steering Wheel Speed Position Sensor

#### Connector Part Information

OEM: AIT2PB-06-01FS
Service: See Catalog
Description: 6-Way F AIT II Series (NA)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Steering Wheel Speed Position Sensor

Pin

Wire

Circuit

Function

1

--

--

Not Used

2

0.5 L-GN/BK

6432

CAN Bus Low Serial Data

3

0.5 TN/WH

6433

CAN Bus High Serial Data

4

--

--

Not Used

5

0.5 D-GN

2087

12-Volt Reference

6

0.5 L-BU

2088

Low Reference

### Steering Wheel/Column Tilt/Telescope Switch (N38)

#### Connector Part Information

OEM: AIT2PB-06-1AK
Service: See Catalog
Description: 6-Way AIT II Series (BK)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Steering Wheel/Column Tilt/Telescope Switch (N38)

Pin

Wire

Circuit

Function

1

0.35 RD/WH

2140

Battery Positive Voltage

2

0.35 GY

2096

Steering Column Tilt and Telescope Up Switch Signal

3

0.35 PK

2094

Steering Column Tilt and Telescope Forward Switch Signal

4

--

--

Not Used

5

0.35 OG

2095

Steering Column Tilt and Telescope Reverse Switch Signal

6

0.35 YE

2097

Steering Column Tilt and Telescope Down Switch Signal

### Sunload Sensor (CJ2)

#### Connector Part Information

OEM: 12064760
Service: 12085208
Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12064971/5
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Sunload Sensor (CJ2)

Pin

Wire

Circuit

Function

A

0.35 L-BU/BK

590

Driver Sunload Sensor Signal

B

0.35 GY

1548

Passenger Sunload Sensor Signal

C

0.35 BK/WH

1551

Ground

D

0.35 L-GN/BK

1137

DRL Ambient Light Sensor Signal

### Sunroof Control Module (C3U)

#### Connector Part Information

OEM: 7283-5909-40
Service: See Catalog
Description: 10-Way F (L-GY)

#### Terminal Part Information

Pin: 1, 6
Terminal/Tray: 7116-4101-08/9
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094430/J-35616-2A (GY)

Pin: 3
Terminal/Tray: 7116-4110-02/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

Pins: 5, 7, 10
Terminal/Tray: 7116-4100-08/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Sunroof Control Module (C3U)

Pin

Wire

Circuit

Function

1

3.0 BK

850

Ground

2

--

--

Not Used

3

0.5 YE

43

Ignition Voltage

4

--

--

Not Used

5

0.35 BN

100

Sunroof Switch Open Signal

6

1 RD/WH

3440

Battery Positive Voltage

7

0.35 WH

--

Serial Communication

8-9

--

--

Not Used

10

0.35 OG

110

Sunroof Switch Close Signal

### Sunroof Shade Module (C3U)

#### Connector Part Information

OEM: 7283-5909-40
Service: See Catalog
Description: 10-Way F (L-GY)

#### Terminal Part Information

Pin: 1, 6
Terminal/Tray: 7116-4101-08/9
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 12094430/J-35616-2A (GY)

Pin: 3
Terminal/Tray: 7116-4110-02/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094430/J-35616-4A (PU)

Pins: 5, 7, 10
Terminal/Tray: 7116-4100-08/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Sunroof Shade Module (C3U)

Pin

Wire

Circuit

Function

1

1 BK

850

Ground

2

--

--

Not Used

3

0.5 YE

43

Ignition Voltage

4

--

--

Not Used

5

0.35 D-BU

5304

Front Sunshade Switch Open Signal

6

1 RD/WH

3440

Battery Positive Voltage

7

PU

--

Serial Communication

8-9

--

--

Not Used

10

0.35 YE/BK

5305

Front Sunshade Switch Close Signal

### Sunroof Shade Switch (C3U)

#### Connector Part Information

OEM: 12124997
Service: 12167130
Description: 5-Way F Metri-Pack 150 Series, Unsealed (BK)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Sunroof Shade Switch (C3U)

Pin

Wire

Circuit

Function

A

0.35 GY

8

Instrument Panel Lamp Voltage

B

0.35 BK

850

Ground

C

--

--

Not Used

D

0.35 L-BU

5304

Front Sunshade Switch Open Signal

E

0.35 YE

5305

Front Sunshade Switch Close Signal

### Sunroof Switch (C3U)

#### Connector Part Information

OEM: 12124997
Service: 12167130
Description: 5-Way F Metri-Pack 150 Series, Unsealed (BK)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Sunroof Switch (C3U)

Pin

Wire

Circuit

Function

A

0.35 GY

8

Instrument Panel Lamp Voltage

B

0.35 BK

850

Ground

C

--

--

Not Used

D

0.35 BN

100

Sunroof Switch Open Signal

E

0.35 OG

110

Sunroof Switch Close Signal

### Sunshade - Left (DH6)

#### Connector Part Information

OEM: 12047663
Service: 12085481
Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12047581/2
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Sunshade - Left (DH6)

Pin

Wire

Circuit

Function

A

0.5 OG

1732

Courtesy Lamps Voltage

B

0.5 BK

850

Ground

### Sunshade - Right (DH6)

#### Connector Part Information

OEM: 12047663
Service: 12085481
Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12047581/2
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Sunshade - Right (DH6)

Pin

Wire

Circuit

Function

A

0.5 OG

1732

Courtesy Lamps Voltage

B

0.5 BK

850

Ground

### Tail Lamp - Left (Z88)

#### Connector Part Information

OEM: 12124662
Service: See Catalog
Description: 5-Way F Metri-Pack 150 Series, Sealed (BN)

#### Terminal Part Information

Terminal/Tray: 12048074/2
Core/Insulation Crimp: E/1
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Tail Lamp - Left (Z88)

Pin

Wire

Circuit

Function

A

0.5 PU

709

Left Park Lamp Voltage

B

--

--

Not Available

C

0.5 YE/BK

5356

Left Tail Lamp Outage Detection Signal

D

0.8 BK

650

Ground

E

0.8 YE

18

Left Rear Stop/Turn Lamp Voltage

### Tail Lamp - Right (Z88)

#### Connector Part Information

OEM: 12124662
Service: See Catalog
Description: 5-Way F Metri-Pack 150 Series, Sealed (BN)

#### Terminal Part Information

Terminal/Tray: 12048074/2
Core/Insulation Crimp: E/1
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Tail Lamp - Right (Z88)

Pin

Wire

Circuit

Function

A

0.5 BN/WH

309

Right Park Lamp Voltage

B

--

--

Not Available

C

0.5 PU

5357

Right Tail Lamp Outage Detection Signal

D

0.8 BK

850

Ground

E

0.8 D-GN

19

Right Rear Stop/Turn Lamp Voltage

### Tail/Stop and Turn Signal Lamp - Left (W49 or WDA or X88)

#### Connector Part Information

OEM: 12450004
Service: See Catalog
Description: 3-Way F CIC W3 Socket (L-GY)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Tail/Stop and Turn Signal Lamp - Left (W49 or WDA or X88)

Pin

Wire

Circuit

Function

A

RD

--

Left Rear Stop/Turn Voltage (WDA)

WH

--

Left Rear Stop/Turn Voltage (W49)

0.8 RD

--

Left Rear Stop/Turn Voltage (X88)

B

BK

--

Ground (W49 or WDA)

BK

--

Ground (W49 or WDA)

0.8 BK

--

Ground (X88)

C

L-BU

--

Park Lamps Voltage (WDA)

L-BU

--

Park Lamps Voltage (WDA)

D-BU

--

Park Lamps Voltage (W49)

D-BU

--

Park Lamps Voltage (W49)

0.8 L-BU

--

Park Lamps Voltage (X88)

### Tail/Stop and Turn Signal Lamp - Right (W49 or WDA or X88)

#### Connector Part Information

OEM: 12450004
Service: See Catalog
Description: 3-Way F CIC W3 Socket (L-GY)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Tail/Stop and Turn Signal Lamp - Right (W49 or WDA or X88)

Pin

Wire

Circuit

Function

A

RD

--

Right Rear Stop/Turn Voltage (WDA)

WH

--

Right Rear Stop/Turn Voltage (W49)

0.8 RD

--

Right Rear Stop/Turn Voltage (X88)

B

BK

--

Ground (W49 or WDA)

BK

--

Ground (W49 or WDA)

0.8 BK

--

Ground (X88)

C

L-BU

--

Park Lamps Voltage (WDA)

L-BU

--

Park Lamps Voltage (WDA)

D-BU

--

Park Lamps Voltage (W49)

D-BU

--

Park Lamps Voltage (W49)

0.8 L-BU

--

Park Lamps Voltage (X88)

### Theft Deterrent Module (TDM)

#### Connector Part Information

OEM: 50579705
Service: See Catalog
Description: 5-Way F 2.54mm (BK)

#### Terminal Part Information

Terminal/Tray: 16-02-1110/20
Core/Insulation Crimp: H/H
Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Theft Deterrent Module (TDM)

Pin

Wire

Circuit

Function

1

0.35 RD/WH

1040

Battery Positive Voltage

2

0.35 BN

4

Ignition Voltage

3

0.35 BK/WH

1551

Ground

4

--

--

Not Used

5

0.35 D-GN

5060

Low Speed GMLAN Serial Data

### Throttle Body (LLT)

#### Connector Part Information

OEM: 15355297
Service: 19115594
Description: 6-Way F GT 150 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 15326427/5
Core/Insulation Crimp: Pins A, B - 2/A
Core/Insulation Crimp: Pins C, D, E, F - E/A
Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Throttle Body (LLT)

Pin

Wire

Circuit

Function

A

0.75 BN

582

TAC Motor Control - 2

B

0.75 YE

581

TAC Motor Control - 1

C

0.5 TN

2752

Low Reference

D

0.5 D-GN

485

TP Sensor 1 Signal

E

0.5 GY

2701

5-Volt Reference

F

0.5 PU

486

TP Sensor 2 Signal

### Trailer Connector (V92)

#### Connector Part Information

OEM: 15354653
Service: 15306164
Description: 7-Way F Metri-Pack 280, Sealed (BK)

#### Terminal Part Information

Pins: A, D, F, G
Terminal/Tray: 12110847/4
Core/Insulation Crimp: E/5
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

Pins: C, E
Terminal/Tray: 12110845/4
Core/Insulation Crimp: A/5
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

Pins: B
Terminal/Tray: 15305232/23
Core/Insulation Crimp: Pins B - B/F/3
Core/Insulation Crimp: Pins B - F/3
Release Tool/Test Probe: J-38125-11A/J-35616-42 (RD)

#### Trailer Connector (V92)

Pin

Wire

Circuit

Function

A

0.5 L-GN

1624

Trailer Backup Lamps Voltage

B

2 BK

850

Ground

C

2 D-BU

47

Trailer Auxiliary Voltage

D

0.5 D-GN

1619

Stop Lamp Voltage

E

2 RD/BK

542

Battery Positive Voltage

F

0.5 BN

2109

Trailer Park Lamps Voltage

G

0.5 YE

1618

Stop Lamp Voltage

### Turn Signal Lamp - Left Front (W49 or Z88)

#### Connector Part Information

OEM: 1-1438608-3
Service: See Catalog
Description: 2-Way F MQS Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Turn Signal Lamp - Left Front (W49 or Z88)

Pin

Wire

Circuit

Function

1

0.8 YE

--

Left Turn Signal Indicator Lamp Voltage (Z88)

0.8 BK

--

Ground (W49)

2

0.8 BK

--

Ground (Z88)

0.8 GN

--

Left Turn Signal Indicator Lamp Voltage (W49)

### Turn Signal Lamp - Lower Left Front (WDA)

#### Connector Part Information

OEM: 1-1438608-3
Service: See Catalog
Description: 2-Way F MQS Series, Sealed (BU)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Turn Signal Lamp - Lower Left Front (WDA)

Pin

Wire

Circuit

Function

1

0.5 L-BU/WH

1314

Left Turn Signal Indicator Lamp Voltage

2

0.5 BK

1350

Ground

### Turn Signal Lamp - Lower Right Front (WDA)

#### Connector Part Information

OEM: 1-1438608-3
Service: See Catalog
Description: 2-Way F MQS Series, Sealed (BU)

#### Terminal Part Information

Terminal/Tray: 962885-5/15
Core/Insulation Crimp: 6/6
Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Turn Signal Lamp - Lower Right Front (WDA)

Pin

Wire

Circuit

Function

1

0.5 L-BU/WH

1314

Right Turn Signal Indicator Lamp Voltage

2

0.5 BK

1350

Ground

### Turn Signal Lamp - Right Front (W49 or Z88)

#### Connector Part Information

OEM: 1-1438608-3
Service: See Catalog
Description: 2-Way F MQS Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Turn Signal Lamp - Right Front (W49 or Z88)

Pin

Wire

Circuit

Function

1

0.8 YE

--

Right Turn Signal Indicator Lamp Voltage (Z88)

0.8 BK

--

Ground (W49)

2

0.8 BK

--

Ground (Z88)

0.8 GN

--

Right Turn Signal Indicator Lamp Voltage (W49)

### Turn Signal Lamp - Upper Left Front (WDA)

#### Connector Part Information

OEM: 1-1438608-3
Service: See Catalog
Description: 2-Way F MQS Series, Sealed (BU)

#### Terminal Part Information

Terminal/Tray: See Terminal Repair Kit
Core/Insulation Crimp: See Terminal Repair Kit
Release Tool/Test Probe: See Terminal Repair Kit

#### Turn Signal Lamp - Upper Left Front (WDA)

Pin

Wire

Circuit

Function

1

0.5 L-BU/WH

1314

Left Turn Signal Indicator Lamp Voltage

2

0.5 BK

1350

Ground

### Turn Signal Lamp - Upper Right Front (WDA)

#### Connector Part Information

OEM: 1-1438608-3
Service: See Catalog
Description: 2-Way F MQS Series, Sealed (BU)

#### Terminal Part Information

Terminal/Tray: 962885-5/15
Core/Insulation Crimp: 6/6
Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Turn Signal Lamp - Upper Right Front (WDA)

Pin

Wire

Circuit

Function

1

0.5 L-BU/WH

1314

Right Turn Signal Indicator Lamp Voltage

2

0.5 BK

1350

Ground

### Turn Signal/Multifunction Switch X1

#### Connector Part Information

OEM: AIT2PB101FS
Service: See Catalog
Description: 10-Way F (WH)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Turn Signal/Multifunction Switch X1

Pin

Wire

Circuit

Function

1

0.35 BK/WH

1551

Ground

2

0.35 L-BU/WH

1414

Left Turn Signal Switch Signal

3

0.35 D-BU/WH

1415

Right Turn Signal Switch Signal

4

0.35 L-BU

1714

Windshield Wiper Switch Low Signal

5

0.35 L-GN

1715

Windshield Wiper Switch High Signal

6

0.35 PK

94

Windshield Washer Switch Signal

7

0.35 TN/BK

6009

Low Reference

8-10

--

--

Not Used

### Turn Signal/Multifunction Switch X2

#### Connector Part Information

OEM: AIT2PB101BH
Service: See Catalog
Description: 10-Way JST (GY)

#### Terminal Part Information

Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Turn Signal/Multifunction Switch X2

Pin

Wire

Circuit

Function

1-6

--

--

Not Used

7

0.35 PU

524

Headlamp Dimmer Switch High Beam Signal

8

0.35 BK/WH

1551

Ground

9

--

--

Not Used

10

0.35 BN

1356

Flash To Pass Switch Signal

### Variable Effort Steering Actuator (NV7)

#### Connector Part Information

OEM: 85202-1
Service: See Catalog
Description: 2-Way F JPT Series (BK)

#### Terminal Part Information

Terminal/Tray: 4-964286-1/16
Core/Insulation Crimp: E/1
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Variable Effort Steering Actuator (NV7)

Pin

Wire

Circuit

Function

1

0.5 BN

1295

Variable Effort Steering Actuator Control

2

0.5 WH

1294

Variable Effort Steering Actuator Voltage

### Vehicle Communications Interface Module (VCIM) X1 (UE1)

#### Connector Part Information

OEM: 15431362
Service: 15306351
Description: 16-Way F Micro64 Unsealed (WH)

#### Terminal Part Information

Pins: 1-3, 6, 7, 10-12, 15
Terminal/Tray: 15445905/23
Core/Insulation Crimp: Pins 1-3, 6, 10-12 - J/J
Core/Insulation Crimp: Pins 7, 15 - K/K
Release Tool/Test Probe: 12180559/J-35616-6 (BN)

#### Vehicle Communications Interface Module (VCIM) X1 (UE1)

Pin

Wire

Circuit

Function

1

0.35 D-GN

5060

Low Speed GMLAN Serial Data

2

0.35 BN/WH

2517

Keypad Red LED Signal

3

0.35 YE/BK

2516

Keypad Green LED Signal

4-5

--

--

Not Used

6

0.35 L-GN/BK

2515

Keypad Voltage

7

0.8 BK

650

Ground

8-9

--

--

Not Used

10

0.35 TN/BK

2500

High Speed GMLAN Serial Data Bus+

11

0.35 D-GN/WH

2514

Keypad Signal

12

0.35 TN

2501

High Speed GMLAN Serial Data Bus-

13-14

--

--

Not Used

15

0.8 RD/WH

4640

Battery Positive Voltage

16

--

--

Not Used

### Vehicle Communications Interface Module (VCIM) X2 (UE1)

#### Connector Part Information

OEM: 15431365
Service: 88952886
Description: 12-Way F Micro64 Series, Unsealed (NA)

#### Terminal Part Information

Terminal/Tray: 15445905/23
Core/Insulation Crimp: J/J
Release Tool/Test Probe: 12180559/J-35616-6 (BN)

#### Vehicle Communications Interface Module (VCIM) X2 (UE1)

Pin

Wire

Circuit

Function

1

0.35 OG/BK

1406

Remote Playback Device Left Audio Signal

2

0.35 L-BU

1405

Remote Playback Device Audio Common Signal

3

0.35 TN/BK

2500

High Speed GMLAN Serial Data Bus+

4

0.35 TN

2501

High Speed GMLAN Serial Data Bus-

5-7

--

--

Not Used

8

0.35 BARE

814

Drain

9

0.35 GY

655

Cellular Microphone Signal

10

0.35 BARE

514

Ground

11-12

--

--

Not Used

### Vehicle Communications Interface Module (VCIM) X3 (UE1)

#### Connector Part Information

OEM: 15431359
Service: See Catalog
Description: 16-Way F Micro 100A (GY)

#### Terminal Part Information

Terminal/Tray: 175266-5/15
Core/Insulation Crimp: J/J
Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Vehicle Communications Interface Module (VCIM) X3 (UE1)

Pin

Wire

Circuit

Function

1

--

--

Not Used

2

0.35 PK

5149

Voice Recognition Audio Signal

3

--

--

Not Used

4

0.35 PK/BK

5152

Low Reference

5

0.35 BARE

1792

Drain

6-16

--

--

Not Used

### Wheel Speed Sensor (WSS) - Left Front

#### Connector Part Information

OEM: 7287-0973-30
Service: 19153615
Description: 2-Way F 1.5 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 34083-1002/28
Core/Insulation Crimp: C/E/1
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Wheel Speed Sensor (WSS) - Left Front

Pin

Wire

Circuit

Function

1

0.5 L-BU

830

Left Front Wheel Speed Sensor Signal

2

0.5 YE

873

Low Reference

### Wheel Speed Sensor (WSS) - Left Rear

#### Connector Part Information

OEM: 7287-0973-30
Service: 19153615
Description: 2-Way F 1.5 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 34083-1002/28
Core/Insulation Crimp: C/E/1
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Wheel Speed Sensor (WSS) - Left Rear

Pin

Wire

Circuit

Function

1

0.5 TN

884

Left Rear Wheel Speed Sensor Signal

2

0.5 OG

885

Low Reference

### Wheel Speed Sensor (WSS) - Right Front

#### Connector Part Information

OEM: 7287-0973-30
Service: 19153615
Description: 2-Way F 1.5 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 34083-1002/28
Core/Insulation Crimp: C/E/1
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Wheel Speed Sensor (WSS) - Right Front

Pin

Wire

Circuit

Function

1

0.5 D-GN

872

Right Front Wheel Speed Sensor Signal

2

0.5 TN

833

Low Reference

### Wheel Speed Sensor (WSS) - Right Rear

#### Connector Part Information

OEM: 7287-0973-30
Service: 19153615
Description: 2-Way F 1.5 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 34083-1002/28
Core/Insulation Crimp: C/E/1
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Wheel Speed Sensor (WSS) - Right Rear

Pin

Wire

Circuit

Function

1

0.5 BN

882

Right Rear Wheel Speed Sensor Signal

2

0.5 WH

883

Low Reference

### Window Motor - Driver (AXC or AXE)

#### Connector Part Information

OEM: 2-1355696-1
Service: 88988401
Description: 6-Way F Timer Jr-Power Series, Sealed (GY)

#### Terminal Part Information

Pins: 1, 4
Terminal/Tray: 4-964273-1/15
Core/Insulation Crimp: C/5
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

Pins: 6
Terminal/Tray: 4-964286-1/16
Core/Insulation Crimp: E/1
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Window Motor - Driver (AXC or AXE)

Pin

Wire

Circuit

Function

1

2 RD/WH

3340

Battery Positive Voltage

2-3

--

--

Not Used

4

2 BK

550

Ground

5

--

--

Not Used

6

0.35 BN

6132

Linear Interconnect Network Bus

### Window Motor - Driver (without AXC or AXE)

#### Connector Part Information

OEM: 12129487
Service: 88988609
Description: 2-Way F Metri-Pack 280 Series, Flexlock, Sealed (GY)

#### Terminal Part Information

Terminal/Tray: 12110845/4
Core/Insulation Crimp: F/5
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Motor - Driver (without AXC or AXE)

Pin

Wire

Circuit

Function

A

3 BN

165

Power Window Motor Left Front Down Control

B

3 D-BU

164

Power Window Motor Left Front Up Control

### Window Motor - Left Rear

#### Connector Part Information

OEM: 12129487
Service: 88988609
Description: 2-Way F Metri-Pack 280 Series, Flexlock, Sealed (GY)

#### Terminal Part Information

Terminal/Tray: 12110853/4
Core/Insulation Crimp: F/5
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Motor - Left Rear

Pin

Wire

Circuit

Function

A

3 BN

669

Power Window Motor Left Rear Down Control

B

3 D-BU

668

Power Window Motor Left Rear Up Control

### Window Motor - Passenger (AXC)

#### Connector Part Information

OEM: 2-1355696-1
Service: 88988401
Description: 6-Way F Timer Jr-Power Series, Sealed (GY)

#### Terminal Part Information

Pins: 1, 4
Terminal/Tray: 4-964273-1/15
Core/Insulation Crimp: C/5
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

Pins: 6
Terminal/Tray: 4-964286-1/16
Core/Insulation Crimp: E/1
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Window Motor - Passenger (AXC)

Pin

Wire

Circuit

Function

1

2 RD/WH

3340

Battery Positive Voltage

2-3

--

--

Not Used

4

2 BK

750

Ground

5

--

--

Not Used

6

0.35 D-BU

6133

Linear Interconnect Network Bus

### Window Motor - Passenger (without AXC)

#### Connector Part Information

OEM: 12129487
Service: 88988609
Description: 2-Way F Metri-Pack 280 Series, Flexlock, Sealed (GY)

#### Terminal Part Information

Terminal/Tray: 12110845/4
Core/Insulation Crimp: A/5
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Motor - Passenger (without AXC)

Pin

Wire

Circuit

Function

A

2 BN

667

Power Window Motor Right Front Down Control

B

2 D-BU

666

Power Window Motor Right Front Up Control

### Window Motor - Right Rear

#### Connector Part Information

OEM: 12129487
Service: 88988609
Description: 2-Way F Metri-Pack 280 Series, Flexlock, Sealed (GY)

#### Terminal Part Information

Terminal/Tray: 12110853/4
Core/Insulation Crimp: F/5
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Motor - Right Rear

Pin

Wire

Circuit

Function

A

3 BN

671

Power Window Motor Right Rear Down Control

B

3 D-BU

670

Power Window Motor Right Rear Up Control

### Window Switch - Driver X1 (without AXC or AXE)

#### Connector Part Information

OEM: 7283-9028-30
Service: See Catalog
Description: 8-Way F YESC Kaizen Series (BK)

#### Terminal Part Information

Pins: 1
Terminal/Tray: 7114-4100-08/9
Core/Insulation Crimp: E/C
Release Tool/Test Probe: 15315247/J-35616-3 (GY)

Pins: 2-8
Terminal/Tray: 7116-4618-02/14
Core/Insulation Crimp: P/P
Release Tool/Test Probe: J-38125-215/J-35616-64B (L-BU)

#### Window Switch - Driver X1 (without AXC or AXE)

Pin

Wire

Circuit

Function

1

0.35 PU/WH

1382

LED Dimming Signal

2

0.35 D-BU

1307

Power Window Master Switch Lockout Signal

3

0.35 PU

169

Power Window Master Switch Left Rear Down Signal

4

0.35 D-GN

168

Power Window Master Switch Left Rear Up Signal

5

0.35 TN

167

Power Window Master Switch Right Front Down Signal

6

0.35 L-BU

166

Power Window Master Switch Right Front Up Signal

7

0.35 PU

171

Power Window Master Switch Right Rear Down Signal

8

0.35 L-GN

170

Power Window Master Switch Right Rear Up Signal

### Window Switch - Driver X2 (without AXC or AXE)

#### Connector Part Information

OEM: 19177577
Service: 15306174
Description: 8-Way F GT 280 Series (BK)

#### Terminal Part Information

Pins: A, D, E, H
Terminal/Tray: 15304713/19
Core/Insulation Crimp: F/D
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

Pins: F, G
Terminal/Tray: 15304711/8
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Switch - Driver X2 (without AXC or AXE)

Pin

Wire

Circuit

Function

A

3 BK

550

Ground

B-C

--

--

Not Used

D

3 BN

165

Power Window Motor Left Front Down Control

E

3 D-BU

164

Power Window Motor Left Front Up Control

F

0.35 L-BU/WH

280

Power Window Master Switch Lockout Right Rear Signal

G

0.35 YE

43

Ignition Voltage

H

3 RD/WH

3340

Battery Positive Voltage

### Window Switch - Left Rear

#### Connector Part Information

OEM: 19177577
Service: 15306174
Description: 8-Way F GT 280 Series (BK)

#### Terminal Part Information

Pins: A-D
Terminal/Tray: 15304711/8
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

Pins: E-H
Terminal/Tray: 15304713/19
Core/Insulation Crimp: Pins E, H - F/D
Core/Insulation Crimp: Pins F, G - 4/4
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Switch - Left Rear

Pin

Wire

Circuit

Function

A

0.35 D-GN

168

Power Window Master Switch Left Rear Up Signal

B

--

--

Not Used

C

0.35 PU

169

Power Window Master Switch Left Rear Down Signal

D

0.35 D-BU

1307

Power Window Master Switch Lockout Signal

E

3 D-BU

668

Power Window Motor Left Rear Up Control

F

2 BK

550

Ground

G

2 RD/WH

3340

Battery Positive Voltage

H

3 BN

669

Power Window Motor Left Rear Down Control

### Window Switch - Passenger (without AXC or AXE)

#### Connector Part Information

OEM: 19177577
Service: 15306174
Description: 8-Way F GT 280 Series (BK)

#### Terminal Part Information

Pins: A-D
Terminal/Tray: 15304711/8
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

Pins: E-H
Terminal/Tray: 15304713/19
Core/Insulation Crimp: 4/4
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Switch - Passenger (without AXC or AXE)

Pin

Wire

Circuit

Function

A

0.35 L-BU

166

Power Window Master Switch Right Front Up Signal

B

0.35 GY

8

Instrument Panel Lamp Voltage

C

0.35 TN

167

Power Window Master Switch Right Front Down Signal

D

0.35 YE

43

Ignition Voltage

E

2 D-BU

666

Power Window Motor Right Front Up Control

F

2 BK

750

Ground

G

2 RD/WH

3340

Battery Positive Voltage

H

2 BN

667

Power Window Motor Right Front Down Control

### Window Switch - Right Rear

#### Connector Part Information

OEM: 19177577
Service: 15306174
Description: 8-Way F GT 280 Series (BK)

#### Terminal Part Information

Pins: A-D
Terminal/Tray: 15304711/8
Core/Insulation Crimp: E/A
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

Pins: E-H
Terminal/Tray: 15304713/19
Core/Insulation Crimp: Pins E, H - F/D
Core/Insulation Crimp: Pins F, G - 4/4
Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Window Switch - Right Rear

Pin

Wire

Circuit

Function

A

0.35 L-GN

170

Power Window Master Switch Right Rear Up Signal

B

--

--

Not Used

C

0.35 PU

171

Power Window Master Switch Right Rear Down Signal

D

0.35 L-BU/WH

280

Power Window Master Switch Lockout Right Rear Signal

E

3 D-BU

670

Power Window Motor Right Rear Up Control

F

2 BK

750

Ground

G

2 RD/WH

3340

Battery Positive Voltage

H

3 BN

671

Power Window Motor Right Rear Down Control

### Windshield Washer Fluid Level Switch

#### Connector Part Information

OEM: 19177500
Service: 88987993
Description: 2-Way F GT 150 Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 15326267/19
Core/Insulation Crimp: E/4
Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Windshield Washer Fluid Level Switch

Pin

Wire

Circuit

Function

1

0.5 BK

1350

Ground

2

0.35 TN

185

Low Washer Fluid Indicator Control

### Windshield Washer Fluid Pump

#### Connector Part Information

OEM: 12052641
Service: 12102747
Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

Terminal/Tray: 12048074/2
Core/Insulation Crimp: E/1
Release Tool/Test Probe: 12094429/J-35616-14 (GN)

#### Windshield Washer Fluid Pump

Pin

Wire

Circuit

Function

A

0.5 OG

228

Windshield Washer Pump Control

B

0.5 BK

1350

Ground

### Windshield Washer Solvent Heater X1 (XA7)

#### Connector Part Information

OEM: 7282-3214-30
Service: 19115654
Description: 2-Way M Y-Type 9.5 Series, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 7114-3250/14
Core/Insulation Crimp: G/3
Release Tool/Test Probe: 12094430/J-35616-21 (RD)

#### Windshield Washer Solvent Heater X1 (XA7)

Pin

Wire

Circuit

Function

1

5 RD/WH

1440

Battery Positive Voltage

2

5 BK

1750

Ground

### Windshield Washer Solvent Heater X2 (XA7)

#### Connector Part Information

OEM: 33472-0611
Service: 19115669
Description: 6-Way F Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 33012-1003/23
Core/Insulation Crimp: 2/E/2
Release Tool/Test Probe: J-38125-217/J-35616-14 (GN)

#### Windshield Washer Solvent Heater X2 (XA7)

Pin

Wire

Circuit

Function

1

0.35 L-GN

6096

Washer Fluid Heated Control Switch Signal

2

0.35 D-BU/WH

5970

Washer Fluid Heated Control Switch LED Voltage

3

--

--

Not Used

4

0.35 BK

1450

Ground

5

0.35 PK

94

Windshield Washer Switch Signal

6

0.35 OG

300

Power Mode

### Windshield Wiper Motor

#### Connector Part Information

OEM: 19207310
Service: 88987987
Description: 4-Way F Timer Jr-Power Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 4-964273-1/15
Core/Insulation Crimp: E/1
Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Windshield Wiper Motor

Pin

Wire

Circuit

Function

1

1 PU

92

Windshield Wiper Motor High Speed

2

1 D-GN

95

Windshield Washer Switch Signal

3

0.35 YE

196

Windshield Wiper Motor Park Switch Signal

4

1 BK

1650

Ground

### Yaw and Lateral Accelerometer Sensor

#### Connector Part Information

OEM: 1-967640-1
Service: 88953370
Description: 4-Way F MQS Socket Housing, Sealed (BK)

#### Terminal Part Information

Terminal/Tray: 962885-5/15
Core/Insulation Crimp: 6/6
Release Tool/Test Probe: 12094429/J-35616-64B (L-BU)

#### Yaw and Lateral Accelerometer Sensor

Pin

Wire

Circuit

Function

1

0.5 L-BU

2088

Low Reference

2

0.5 L-GN/BK

6432

CAN Bus Low Serial Data

3

0.5 TN/WH

6433

CAN Bus High Serial Data

4

0.5 D-GN

2087

12-Volt Reference