For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front floor console armrest bin assembly. Refer to Front Floor Console Armrest Compartment Replacement.

1 | Front Floor Console Extension Accessory Upper Bezel Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Front Floor Console Extension Accessory Upper Bezel

#### Procedure

Disconnect the electrical connections.