For 1990-2009 cars

## Front Floor Console Extension Panel Replacement - Left Side Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left front seat . Refer to Bucket Seat Replacement.

1 | Front Floor Console Extension Panel.
2 | Retainer Clips (Qty: 6).

## Front Floor Console Extension Panel Replacement - Left Side Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left front seat . Refer to Bucket Seat Replacement .

1 | Front Floor Console Extension Panel
2 | Retainer Clip (Qty: 5)

## Front Floor Console Extension Panel Replacement - Left Side OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left front seat . Refer to Bucket Seat Replacement .

1 | Front Floor Console Extension Panel
2 | Retainer Clip (Qty: 5)

## Front Floor Console Extension Panel Replacement - Left Side Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left front seat. Refer to Bucket Seat Replacement.

1 | Front Floor Console Extension Panel

#### Procedure

Grasp the front floor console extension panel and pull outward releasing the clips securing the extension panel to the console assembly.