For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Catalytic Converter Brace Bolt | 41 N·m | 30 lb ft
Catalytic Converter Hanger Clamp Nut | 18 N·m | 13 lb ft
Catalytic Converter to Exhaust Flexible Pipe Nut | 28 N·m | 21 lb ft
Catalytic Converter to Exhaust Manifold Nut | 50 N·m | 37 lb ft
Exhaust Flexible Pipe to Three-Way Converter Nut | 50 N·m | 37 lb ft
Exhaust Manifold Bolt | 20 N·m | 15 lb ft
Exhaust Manifold Heat Shield Bolt | 10 N·m | 89 lb in
Exhaust Manifold Lower Heat Shield Bolt (Small Bolt) | 10 N·m | 89 lb in
Exhaust Manifold Lower Heat Shield Bolt (Large Bolt) | 50 N·m | 37 lb ft
Exhaust Muffler Heat Shield Nut | 9 N·m | 80 lb in
Three-Way Catalytic Converter to Muffler Assembly Nut | 50 N·m | 37 lb ft