For 1990-2009 cars

## Front Bumper Fascia Bracket Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the front fascia. Refer to Front Bumper Fascia Replacement

1 | Front Bumper Bracket Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in).
2 | Front Bumper Bracket Rivets
3 | Front Bumper Bracket

## Front Bumper Fascia Bracket Replacement Outlook

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front fascia. Refer to Front Bumper Fascia Replacement.

1 | Front Bumper Fascia Bracket/Reinforcement Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in).
2 | Front Bumper Fascia Bracket/Reinforcement