For 1990-2009 cars

### Inside Rearview Mirror with Automatic Day-Night System Operation

The inside rearview mirror uses 2 photocell sensors. One sensor is the rear light sensor, located on the face side of the mirror, facing the rear of the vehicle. The rear light sensor is used to determine light conditions present at the mirror face. The other sensor is the front light sensor, located on the backside of the mirror, facing the front of the vehicle. The front light sensor is used to determine the exterior light conditions at the front of the vehicle. With a low exterior light condition detected by the front light sensor and a high light condition from the rear light sensor, the inside rearview mirror will automatically darken the face of the inside rearview mirror and the left outside rearview mirror. The inside rearview mirror provides a signal circuit and a low reference circuit to the left mirror face to darken the mirror when needed.

With the gear selector lever in the REVERSE position, backup lamp supply voltage is supplied as an input to the inside rearview mirror. The mirror monitors this input to disable the automatic day-night feature. This allows the driver to see objects in the mirror clearly when backing up, regardless of the rear light sensor status.

### Driver Outside Rearview Mirror with Automatic Day-Night System Operation (RPO DNP only)

The automatic day-night feature of the driver outside rearview mirror is controlled by the inside rearview mirror. The inside rearview mirror supplies a signal and low reference to the driver outside rearview mirror. At night, with the automatic day-night feature enabled, the driver outside rearview mirror will automatically darken with the inside rearview mirror to reduce glare from headlamps behind the vehicle.

### Inside Rearview Mirror with Automatic Day-Night Switch Operation

The ON/OFF switch is used to enable/disable the automatic day-night feature of the inside rearview mirror. To enable the automatic day-night feature, turn the ignition ON and depress the ON/OFF switch. A green indicator will illuminate on the inside rearview mirror when the automatic day-night feature is enabled. To disable the automatic day-night feature depress the ON/OFF switch.