For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left side instrument panel insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side .

1 | Body Control Module

#### Procedure

1. Disconnect the electrical connectors.
2. Reprogram the module if replaced. Refer to Control Module References .

Tip
Push tab to release the body control module from the bracket.