For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front driver side door trim panel. Refer to Front Side Door Trim Panel Replacement - Left Side.

1 | Driver Seat Adjustable Memory Switch Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
2 | Driver Seat Adjustable Memory Switch

#### Procedure

Disconnect the electrical connector.