For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Bumper Air Deflector Screw/Bolt | 2 N·m | 18 lb in
Front Bumper Fascia Bolts | 10 N·m | 89 lb in
Front Bumper Fascia Shield Screw | 2 N·m | 18 lb in
Front Bumper Impact Bar Bolts | 30 N·m | 22 lb ft
Rear Bumper Fascia (Inside Wheel Well) Bolts | 10 N·m | 89 lb in
Rear Bumper Fascia Center Bracket Bolts | 10 N·m | 89 lb in
Rear Bumper Fascia Retainers | 2 N·m | 18 lb in
Rear Bumper Fascia Side Bracket Bolts | 7 N·m | 62 lb in
Rear Bumper Fascia Screws | 2 N·m | 18 lb in
Rear Bumper Fascia Tail Lamp Pocket Screws | 2 N·m | 18 lb in
Rear Bumper Fascia Upper Bracket Bolts | 10 N·m | 89 lb in
Rear Bumper Impact Bar Bolts | 30 N·m | 22 lb ft