For 1990-2009 cars

Table 1: | Engine Specifications

The following approximate capacities are given in English and metric conversions. See Recommended Fluids and Lubricants for more information.

Application | Capacities
--- | ---
English | Metric
Air Conditioning Refrigerant R134a | For the air conditioning system refrigerant charge amount, see the refrigerant caution label located under the hood. See your dealer/retailer for more information.
Cooling System | 11.4 qt | 10.8 L
Engine Oil with Filter | 5.5 qt | 5.2 L
Fuel Tank | 22.0 gal | 83.3 L
Transmission Fluid* | 5.3 qt | 5.0 L
Wheel Nut Torque | 140 lb ft | 190 N·m
*See Automatic Transmission Fluid for information on checking fluid level.
All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual. Recheck fluid level after filling.

#### Engine Specifications

Engine | VIN Code | Transmission | Spark Plug Gap
--- | --- | --- | ---
3.6L V6 Engine | D | Automatic | 0.043 in (1.10 mm)