For 1990-2009 cars

#### Refrigerant System Capacities

Application | Specification
--- | ---
Metric | English
PAG Oil GM P/N 12378526 for United States PAG Oil GM P/N 88900060 for Canada PAG Oil Saturn P/N 22695048
Total System PAG Oil Capacity | 195 ml | 6.5 oz
Compressor | 75 ml¹ | 2.5 oz¹
The Denso service compressor contains 75 ml (2.5 oz) of PAG oil.
Condenser | 10 ml¹ | 0.3 oz¹
Desiccant Cartridge | 10 ml¹ | 0.3 oz¹
Evaporator, Front | 10 ml¹ | 0.3 oz¹
Evaporator, Rear | 10 ml¹ | 0.3 oz¹
Abrupt Refrigerant Loss | 60 ml² | 2.0 oz²
Refrigerant Charge, R134a | 1.05 kg | 2.3 Lb
¹If more than the specified amount of PAG oil was drained from a component, add the equal amount of oil drained. ²Abrupt refrigerant loss due to large leak, hose rupture, collision, or pressure relief valve opening. Conditions that allow the refrigerant to seep or bleed off over time do not cause this oil loss. Upon replacement of a component that caused a large refrigerant loss, also add the required amount of oil for the particular component.