For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the left instrument panel insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Left Side.

1 | Brake Pedal Position Sensor Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 3 N·m (27 lb in)
2 | Brake Pedal Position Sensor

#### Procedure

1. Disconnect the brake pedal position sensor electrical connector.
2. After the installation is complete, calibrate the brake pedal position sensor. Refer to Brake Pedal Position Sensor Calibration.