For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Low and Reverse Clutch Retainer Ring
2 | Low and Reverse Clutch Assembly
3 | 1-2-3-4 Clutch (w/Friction Material) Plate Assembly (Qty: 2)
4 | 1-2-3-4 Clutch Plate (Qty: 2)
5 | 1-2-3-4 Clutch (Waved) Plate
6 | 1-2-3-4 Clutch Spring Retainer Ring
7 | 1-2-3-4 Clutch Spring
8 | 1-2-3-4 Clutch Piston Tip

• | Use pliers to remove the piston.

• | Inspect the piston seals for damage and/or wear. The piston is reusable.