For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear floor console front upper trim panel assembly. Refer to Rear Floor Console Front Trim Upper Panel Replacement.

1 | Rear Floor Console Rear Release Latch Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Floor Console Release Latch Assembly