For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the ignition lock cylinder opening trim cover. Refer to Ignition Lock Cylinder Opening Trim Cover Replacement .
2. Remove the ignition lock cylinder. Refer to Ignition Lock Cylinder Replacement .

1 | Theft Deterrent Module Assembly

#### Procedure

1. Disconnect the electrical connector.
2. Program the theft deterrent control module after replacement. Refer to Control Module References .