For 1990-2009 cars

## Rear Wheel Opening Molding Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .

1 | Rear Wheel Opening Flare Integral Retainers (Qty: 7)

#### Procedure

Secure the center retainer to the center upper wheelhouse opening followed by the remainder of the retainers.

2 | Rear Wheel Opening Flare Tabs (Qty: 2)
3 | Rear Wheel Opening Flare

## Rear Wheel Opening Molding Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

1 | Rear Wheel Opening Flare Integral Retainer (Qty: 7)
2 | Rear Wheel Opening Flare

#### Procedure

Align the center pin first to the body panel and secure the retainers on each side of the pin.