For 1990-2009 cars

Table 1: | Control Valve Body Cover Removal
Table 2: | Control Solenoid (w/Body and TCM) Valve Assembly Removal
Table 3: | Control Valve Body Assembly and Output Speed Sensor Removal

### Control Valve Body Cover Removal

Callout | Component Name
--- | ---
1 | Control Valve Body Cover Stud M6 x 30 (Qty: 2)
2 | Control Valve Body Cover Bolt M6 x 30 (Qty: 12)
3 | Control Valve Body Cover
4 | Control Valve Body Cover Gasket Tip Do not re-use the valve body cover gasket.
5 | Control Valve Body Cover Wiring Connector Hole Seal Caution: Support the control solenoid valve assembly around the connector when removing the seal. Excessive pulling force can damage the internal electrical connections.
6 | Shift Position Switch Connector
7 | Output Speed Sensor Connector
8 | Input Speed Sensor Connector

### Control Solenoid (w/Body and TCM) Valve Assembly Removal

Callout | Component Name
--- | ---
1 | Control Valve Body Bolt M6 x 80 (Qty: 4)
2 | Control Solenoid Valve Spring
3 | Control Valve Body Bolt M6 x 65 (Qty: 2)
4 | Control Valve Body Bolt M6 x 42 (Qty: 1)
5 | Control Valve Body Bolt M6 x 95 (Qty: 3)
6 | Control Valve Body Bolt M6 x 55 (Qty: 1)
7 | Control Solenoid (w/Body and TCM) Valve Assembly
8 | Control Solenoid Valve Assembly Filter Plate Caution: Use care when removing or installing the filter plate assembly. A broken or missing retaining tab may not adequately secure the filter plate to the control solenoid valve assembly, resulting in possible damage or contamination.

Tip

• | Discard the filter plate. It is not reusable.

• | Inspect the pressure switch manifold seals for damage. Replace the control valve assembly as necessary.

### Control Valve Body Assembly and Output Speed Sensor Removal

Callout | Component Name
--- | ---
1 | Control Valve Body Bolt M6 x 65 (Qty: 8)
2 | Control Valve Body Bolt M6 x 55 (Qty: 2)
3 | Manual Shaft Detent Assembly
4 | Control Valve Body Assembly
5 | A/Trans Output Speed Sensor Bolt M6 x 25
6 | A/Trans Output Speed Sensor
7 | 1-2-3-4 Clutch Fluid Passage Seal Tip The seal is not reusable.