For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front seat back cushion cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement.

1 | Front Seat Back Cushion Support Assembly Retainer (Qty: 5)
2 | Front Seat Back Cushion Support Assembly Screw (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Front Seat Back Cushion Support Assembly