For 1990-2009 cars

Callous | Component Name
--- | ---
1 | Rear Side Door Window Reveal Molding Lower Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 5 N·m (44 lb in)
2 | Rear Side Door Window Reveal Molding Upper Screw Tip: Replace the clip if damaged, transfer the clip to the new part.
3 | Rear Side Door Window Upper Reveal Molding Rivets (Qty: 6)
4 | Rear Side Door Window Upper Reveal Molding