For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the instrument panel center compartment. Refer to Instrument Panel Center Compartment Replacement .

1 | Radio Front Speaker Screw (Qty: 2) Caution: Refer to Component Fastener Tightening Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Radio Front Speaker Assembly

#### Procedure

Disconnect the electrical connector.