For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Liftgate Trim Panel Plug

#### Procedure

1. From inside the vehicle lower the second and third, if applicable, row seats.
2. Use a small flat-bladed tool to remove the access plug from the liftgate lower interior trim panel.
3. Push on a silver lever located on the right just through the access hole to unlock the liftgate.
4. Open the liftgate from the outside of the vehicle using the exterior handle.