For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front carpet retainer. Refer to Front Carpet Retainer Replacement .
2. Remove the rear carpet retainer. Refer to Rear Carpet Retainer Replacement .
3. Remove the seat belt anchor bolt from the front seat. Refer to Seat Belt Retractor Pretensioner Replacement - Front .

1 | Center Pillar Lower Garnish Molding Clip (Qty: 4)
2 | Center Pillar Lower Garnish Molding Assembly