For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Park Pawl Actuator Bracket Bolt M6 x 25 (Qty: 2)
2 | Park Pawl Actuator Bracket
3 | Park Pawl Shaft
4 | Park Pawl
5 | Park Pawl Spring
6 | Park Pawl Actuator Guide Pin
7 | Park Pawl Actuator Guide
8 | Manual Shift Detent Lever Pin Tip

• | Use a small nail puller or other suitable tool.

• | Discard the pin. The pin is not reusable.

#### Special Tools

• | J 6125-1B Slide Hammer with Adapter

• | J 23129 Universal Seal Remover

For equivalent regional tools, refer to Special Tools.

9 | Manual Shaft Detent (w/Shift Position Switch) Lever Assembly Tip Rotate the assembly counterclockwise so the actuator rod will fit through the case opening.
10 | Park Pawl Actuator Assembly