For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Ball Joint to Lower Control Arm Mounting Nuts and Bolts | 68 N·m | 50 lb ft
Front Frame Reinforcement Mounting Bolts | 50 N·m | 37 lb ft
Front Frame to Body Bolts

- First Pass

100 N·m

74 lb ft

- Final Pass

+ 90°

Front Wheel Bearing and Hub to Knuckle Bolts | 140 N·m | 103 lb ft
Front Lower Control Arm Front Nut | 195 N·m | 144 lb ft
Front Lower Control Arm Bushings Nuts | 75 N·m | 55 lb ft
Front Lower Control Arm Bushing Rear Nut | 150 N·m | 111 lb ft
Lower Control Arm Ball Stud Nuts

- First Pass

40 N·m

30 lb ft

- Final Pass

+ 120°

Stabilizer Link to Stabilizer Shaft Nuts | 75 N·m | 55 lb ft
Stabilizer Link to Strut Nuts | 70 N·m | 52 lb ft
Stabilizer Shaft Clamp to Frame Bolts | 50 N·m | 37 lb ft
Steering Knuckle to Strut Bolts | 195 N·m | 144 lb ft
Strut Mount Nut | 85 N·m | 63 lb ft
Strut to Body Mounting Nuts | 45 N·m | 33 lb ft
Upper Strut to Bearing Plate Nuts | 83 N·m | 61 lb ft