For 1990-2009 cars

## Tail Lamp Bulb Replacement Acadia

Callout | Component Name
--- | ---

#### Procedure

Remove the tail lamp assembly. Refer to Tail Lamp Replacement.

1 | Stop, Tail, Turn Signal Lamp Bulb Socket

#### Procedure

Rotate and remove the lamp socket from the tail lamp housing.

2 | Stop, Tail, Turn Signal Lamp Bulb Tip Pull the bulb straight from the lamp socket.

## Tail Lamp Bulb Replacement Enclave

Callout | Component Name
--- | ---

#### Procedure

Remove the tail lamp assembly. Refer to Tail Lamp Replacement.

1 | Stop, Tail, Turn Signal Lamp Bulb Socket

#### Procedure

Rotate and remove the lamp socket from the tail lamp housing.

2 | Stop, Tail, Turn Signal Lamp Bulb Tip Pull the bulb straight from the lamp socket.
3 | Rear Side Marker Lamp Socket

#### Procedure

Rotate and remove the lamp socket from the tail lamp housing.

4 | Rear Side Marker Lamp Bulb

## Tail Lamp Bulb Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the tail lamp assembly. Refer to Tail Lamp Replacement.

1 | Stop, Tail, Turn Signal Lamp Bulb Socket

#### Procedure

Rotate and remove the lamp socket from the tail lamp housing.

2 | Stop, Tail, Turn Signal Lamp Bulb Tip Pull the bulb straight from the lamp socket.

## Tail Lamp Bulb Replacement Traverse

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the tail lamp assembly. Refer to Tail Lamp Replacement.

1 | Stop and Turn Lamp Bulb Socket

#### Procedure

Rotate and remove the lamp socket from the tail lamp housing.

2 | Stop and Turn Lamp Bulb Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Pull the bulb straight from the lamp socket.