For 1990-2009 cars

## Daytime Running Lamp Bulb Replacement Enclave

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front wheelhouse liner. Refer to Front Wheelhouse Front Liner Replacement.

1 | Daytime Running Lamp Socket Assembly Tip Rotate counterclockwise the bulb socket and pull downward.
2 | Daytime Running Lamp Bulb Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Pull the bulb straight from the socket assembly.

## Daytime Running Lamp Bulb Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the headlamp capsule from the vehicle. Refer to Headlamp Capsule Replacement.

1 | Headlamp Bulb Accessory Cover

#### Procedure

Rotate the bulb cover counterclockwise from the headlamp capsule and remove.

2 | Daytime Running Lamp Bulb Warning: Refer to Halogen Bulb Warning in the Preface section.

#### Procedure

Rotate the bulb socket and disconnect the electrical connector from the bulb socket.