For 1990-2009 cars

## Instrument Panel Center Compartment Replacement Traverse

Callout | Component Name
--- | ---
1 | Instrument Panel Center Compartment Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Center Compartment Assembly

#### Procedure

Use a flat bladed plastic trim tool in order to release the retainer clips securing the instrument panel storage compartment to the instrument panel assembly.

## Instrument Panel Center Compartment Replacement Acadia

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.

1 | Instrument Panel Center Compartment Screw (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Center Compartment Assembly
3 | Retainer Clip (Qty: 2)

## Instrument Panel Center Compartment Replacement Enclave

Callout | Component Name
--- | ---
1 | Instrument Panel Center Compartment Screws Qty: (2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Instrument Panel Center Compartment Assembly

#### Procedure

Use a flat bladed plastic trim tool in order to release the forward edge of the instrument panel storage compartment from the instrument panel.

2 | Retainer Clips (Qty: 2)

## Instrument Panel Center Compartment Replacement OUTLOOK

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement.

1 | Compartment Inner Trim Panel
2 | Instrument Panel Center Compartment Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
3 | Instrument Panel Center Compartment Assembly
4 | Retainer Clip (Qty: 6)