For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptor

DTC P1629: Theft Deterrent Fuel Enable Signal Not Received

### Circuit/System Description

The theft deterrent module (TDM) sends the prerelease password to the engine control module (ECM) via the serial data circuit. The ECM then sends a challenge to the TDM. Both the ECM and TDM perform a calculation on this challenge. If the calculated response from the TDM equals the calculation performed by the ECM, the ECM will allow vehicle starting.

### Conditions for Running the DTC

• | Ignition is in the ACCESSORY or RUN position.

• | The ECM is not in learn mode.

### Conditions for Setting the DTC

The ECM receives does not receive the challenge response from the TDM within the required amount of time.

### Action Taken When the DTC Sets

The security indicator will illuminate.

### Conditions for Clearing the DTC

• | A current DTC P1629 will be cleared when a challenge response is received.

• | A history DTC will be cleared after 40 malfunction-free ignition cycles or when a scan tool is used to clear DTCs.

### Diagnostic Aids

DTC P1629 is an indicator that the challenge/response was not received within the required time. This does not necessarily indicate a fault is present with the TDM or ECM. Factors such as a long engine crank, a delay in the serial data communication, or B-codes set in the TDM will cause DTC P1629 to set. This DTC should not be used as a fault indicator, but rather as a symptom to assist in the diagnosis of these other systems.

### Reference Information

#### Schematic Reference

Immobilizer Schematics

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Immobilizer Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

Control Module References for scan tool information